(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VCC")
	(net 3 "PF3{slash}SDC0_CMD{slash}JTAG_DO")
	(net 4 "FB3")
	(net 5 "PB5{slash}PWM1{slash}PB_EINT5")
	(net 6 "+3V3")
	(net 7 "+1V8")
	(net 8 "PE2{slash}CSI_HSYNC{slash}LCD_HSYNC")
	(net 9 "PB0{slash}UART2_TX{slash}PB_EINT0")
	(net 10 "FB2")
	(net 11 "PE6{slash}CSI_D2{slash}LCD_D4")
	(net 12 "PF1{slash}SDC0_D0{slash}JTAG_DI")
	(net 13 "PB1{slash}UART2_RX{slash}PB_EINT1")
	(net 14 "PE19{slash}CSI_D15{slash}LCD_D21")
	(net 15 "USB-DP")
	(net 16 "EPHY-RTX")
	(net 17 "+1V2")
	(net 18 "FB1")
	(net 19 "PG5{slash}SDC1_D3{slash}PG_EINT5")
	(net 20 "+3V0")
	(net 21 "HPVCCIN")
	(net 22 "HPVCC")
	(net 23 "PE4{slash}CSI_D0{slash}LCD_D2")
	(net 24 "RTC_VIO")
	(net 25 "PG4{slash}SDC1_D2{slash}PG_EINT4")
	(net 26 "HP_VCCBP")
	(net 27 "PE9{slash}CSI_D5{slash}LCD_D7")
	(net 28 "PB8{slash}TWI1_SCK{slash}UART0_TX{slash}PB_EINT8")
	(net 29 "VCC_RTC")
	(net 30 "MCSI-CKP")
	(net 31 "PC1{slash}SDC2_CMD{slash}SPI0_CLK")
	(net 32 "PF6")
	(net 33 "PF5{slash}SDC0_D2{slash}JTAG_CK")
	(net 34 "SVREF")
	(net 35 "GNDA")
	(net 36 "MICIN1N")
	(net 37 "HPVCCBP")
	(net 38 "/电源/VRA2")
	(net 39 "PE23{slash}LCD_D22{slash}UART1_RTS")
	(net 40 "/电源/VRA1")
	(net 41 "/电源/X24MIN")
	(net 42 "/电源/X24MOUT")
	(net 43 "PE18{slash}CSI_D14{slash}LCD_D20")
	(net 44 "EPHY-TXN")
	(net 45 "PE17{slash}CSI_D13{slash}LCD_D19")
	(net 46 "EPHY-LINK-LED")
	(net 47 "/电源/X32KOUT")
	(net 48 "PF4{slash}SDC0_D3{slash}UART0_RX")
	(net 49 "PF2{slash}SDC0_CLK{slash}UART0_TX")
	(net 50 "PB3{slash}UART2_CTS{slash}PB_EINT3")
	(net 51 "/电源/X32KIN")
	(net 52 "PE11{slash}CSI_D7{slash}LCD_D11")
	(net 53 "/电源/RESET")
	(net 54 "LRADC0")
	(net 55 "Net-(D1-A)")
	(net 56 "Net-(D2-A)")
	(net 57 "PE21{slash}CSI_SCK{slash}TWI1_SCK{slash}UART1_TX")
	(net 58 "HPOUTL")
	(net 59 "PE20{slash}CSI_FIELD{slash}CSI_MIPI_MCLK")
	(net 60 "MCSI-D1P")
	(net 61 "PE8{slash}CSI_D4{slash}LCD_D6")
	(net 62 "VBAT")
	(net 63 "/电源/CC1")
	(net 64 "PE5{slash}CSI_D1{slash}LCD_D3")
	(net 65 "PE14{slash}CSI_D10{slash}LCD_D14")
	(net 66 "BT_3V3")
	(net 67 "PE16{slash}CSI_D12{slash}LCD_D18")
	(net 68 "PB6{slash}TWI0_SCK{slash}PB_EINT6")
	(net 69 "VRA1")
	(net 70 "/电源/CC2")
	(net 71 "MCSI-CKN")
	(net 72 "PF0{slash}SDC0_D1{slash}JTAG_MS")
	(net 73 "DEBUG_DP")
	(net 74 "/网口/XTAL_IN")
	(net 75 "DEBUG_DN")
	(net 76 "SW3")
	(net 77 "PC3{slash}SDC2_D0{slash}SPI0_MOSI")
	(net 78 "EPHY-RXP")
	(net 79 "SW2")
	(net 80 "SW1")
	(net 81 "MCSI-D0N")
	(net 82 "VRA2")
	(net 83 "EPHY-SPD-LED")
	(net 84 "Net-(R9-Pad2)")
	(net 85 "Net-(R10-Pad2)")
	(net 86 "Net-(U1B-SZQ)")
	(net 87 "PG3{slash}SDC1_D1{slash}PG_EINT3")
	(net 88 "EPHY-RXN")
	(net 89 "HPCOM")
	(net 90 "PE0{slash}CSI_PCLK{slash}LCD_CLK")
	(net 91 "PB2{slash}UART2_RTS{slash}PB_EINT2")
	(net 92 "PE13{slash}CSI_D9{slash}LCD_D13")
	(net 93 "PB7{slash}TWI0_SDA{slash}PB_EINT7")
	(net 94 "/网口/XTAL_OUT")
	(net 95 "unconnected-(J2-Pin_40-Pad40)")
	(net 96 "EPHY-TXP")
	(net 97 "MCSI-D1N")
	(net 98 "PE12{slash}CSI_D8{slash}LCD_D12")
	(net 99 "PE10{slash}CSI_D6{slash}LCD_D10")
	(net 100 "Net-(U2-V3)")
	(net 101 "Net-(J3-Pad10)")
	(net 102 "Net-(J3-Pad12)")
	(net 103 "PE3{slash}CSI_VSYNC{slash}LCD_VSYNC")
	(net 104 "USB-DM")
	(net 105 "PG2{slash}SDC1_D0{slash}PG_EINT2")
	(net 106 "HPOUTR")
	(net 107 "Net-(U7-BT_WAKE)")
	(net 108 "Net-(U7-BT_HOST_WAKE)")
	(net 109 "PE7{slash}CSI_D3{slash}LCD_D5")
	(net 110 "PC2{slash}SDC2_RST{slash}SPI0_CS")
	(net 111 "MICIN1P")
	(net 112 "/网口/VIN_LDO_OUT")
	(net 113 "MCSI-D0P")
	(net 114 "PG1{slash}SDC1_CMD{slash}PG_EINT1")
	(net 115 "PC0{slash}SDC2_CLK{slash}SPI0_MISO")
	(net 116 "PB4{slash}PWM0{slash}PB_EINT4")
	(net 117 "HBIAS")
	(net 118 "/网口/BT_RST_N")
	(net 119 "PE15{slash}CSI_D11{slash}LCD_D15")
	(net 120 "PE22{slash}CSI_SDA{slash}TWI1_SDA{slash}UART1_RX")
	(net 121 "PE1{slash}CSI_MCLK{slash}LCD_DE")
	(net 122 "PB9{slash}TWI1_SDA{slash}UART0_RX{slash}PB_EINT9")
	(net 123 "/网口/WL_REG_ON")
	(net 124 "/网口/WL_HOST_WAKE")
	(net 125 "PE24{slash}LCD_D23{slash}UART1_CTS")
	(net 126 "PG0{slash}SDC1_CLK{slash}PG_EINT0")
	(net 127 "HPCOMFB")
	(net 128 "/网口/UART_RTS_N")
	(net 129 "/网口/UART_TXD")
	(net 130 "unconnected-(U2-~{RTS}-Pad4)")
	(net 131 "/网口/UART_RXD")
	(net 132 "/网口/UART_CTS_N")
	(net 133 "unconnected-(U6-GND-Pad4)")
	(net 134 "unconnected-(U7-GPIO1-Pad40)")
	(net 135 "unconnected-(U7-NC-Pad5)")
	(net 136 "unconnected-(U7-PCM_CLK-Pad26)")
	(net 137 "unconnected-(U7-GPIO4-Pad37)")
	(net 138 "unconnected-(U7-NC-Pad35)")
	(net 139 "unconnected-(U7-GPIO3-Pad38)")
	(net 140 "unconnected-(U7-PCM_IN-Pad27)")
	(net 141 "unconnected-(J2-Pin_37-Pad37)")
	(net 142 "unconnected-(U7-TP3(NC)-Pad47)")
	(net 143 "unconnected-(U7-NC-Pad30)")
	(net 144 "unconnected-(U7-PCM_OUT-Pad25)")
	(net 145 "unconnected-(U7-TP1-Pad45)")
	(net 146 "unconnected-(U7-NC-Pad32)")
	(net 147 "/网口/VDDIO")
	(net 148 "unconnected-(U7-TP2-Pad46)")
	(net 149 "unconnected-(U7-GPIO2-Pad39)")
	(net 150 "unconnected-(U7-FM_RX-Pad4)")
	(net 151 "unconnected-(U7-NC-Pad29)")
	(net 152 "unconnected-(U7-PCM_SYNC-Pad28)")
	(net 153 "/网口/WL_BT_ANT")
	(net 154 "unconnected-(U7-CLK_REQ-Pad8)")
	(net 155 "unconnected-(J1-SBU2-PadB8)")
	(net 156 "unconnected-(J1-SBU1-PadA8)")
	(net 157 "unconnected-(J3-Pad4)")
	(net 158 "unconnected-(J3-Pad7)")
	(net 159 "unconnected-(J3-Pad8)")
	(net 160 "unconnected-(J3-Pad5)")
	(net 161 "unconnected-(J3-PadSH)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "002841f8-a06b-4120-a5a2-1c3092bd30e5")
		(at 75.5 70.49)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "28cd0470-9242-47f4-86b8-f8ae3e8153c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c4f572fa-5ee5-43aa-86ce-3d4908d3e42f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a814aad9-3569-4e42-a08d-2aea342e557d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43bd3e21-18c2-4ff6-ba74-b716e5a48856")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/e54a4f73-073e-44d8-9dc7-f1d74ace721c")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c80b347-d462-4877-9918-95bb6d1b0296")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ede448a-26cd-4e75-8866-0e4837e430b9")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b261819-93f0-4f17-9388-fd5c31c58d76")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b1c7e638-21a0-4a16-9781-7000ce35d965")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "615c22a1-5082-4ff2-add1-79c0bcb19bfc")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc87b0ca-5891-4bef-b71e-20cb68996870")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f458949d-f46f-472b-b3f7-454225b6c84b")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02826c10-0d6c-4d27-8b41-7b4a96d09bcb")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f9d4fe2-eed3-4aaf-8856-7e80a4f73ee4")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4335eae6-a247-4413-a375-41ace8e74854")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a3a63cc4-b31b-4782-b247-371978738163")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "SVREF")
			(pintype "passive")
			(uuid "c5f59943-af28-4702-a41f-1d212516a66c")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6b84efb9-d11f-4647-bd58-a781df17cc79")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "02283806-c7e4-44a5-9cdb-88aa19312e5f")
		(at 83.52 75.51)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "33f85adf-518d-4552-a8b9-7ba891b7ed39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "200K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "550cd34c-df2b-41d4-a0dd-2437b9e9fd9e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c90f90c-14af-4068-a5ae-29cdc0eb7527")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db0052e0-f5f6-41c8-82b5-e8c63f5b5c20")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/17fee767-7fb0-472c-93a9-c5f3b7b790a3")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f3586b6-57b1-483c-a549-6a04640ec88b")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd893d5d-7ef9-45c5-afc3-d93ed120d13d")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a30cb0b1-d5a6-437c-a5e3-1a558eeeaae5")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8a84adc-674f-46d4-91f6-fbb77fc79e82")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f986b0da-1539-4992-93f6-9aa12a6e77ec")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c35a8414-d838-4492-a690-ee53d10af919")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f93d51a-cab0-4676-aef2-02447f30bc81")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e2629a1-c6e9-4bd6-80ca-cf3a1d03e0c0")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ffc84a9-30bc-4d21-b23a-f577512f0d62")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4dac2762-7ae3-414b-a953-b263c687f18c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0fb7dafc-2982-4521-a024-7fdea3ce7cf0")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/电源/VRA2")
			(pintype "passive")
			(uuid "55cf04d8-a881-433c-a95a-4a1665ca7a10")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "9268c62e-8004-44d1-83d1-e0df9bcf4260")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "02423873-f266-4287-a275-0331615892b5")
		(at 64.75 112.14)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "665675cd-d3e5-4916-876d-e462f6c45ae3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b62fb9d0-becd-48e8-bf1c-0e005fca0434")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5d5cfec-d0b1-41de-a616-05a488243ba2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "02d72c6c-f14b-43cf-a712-63053f02d3f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/d3e44f2a-5975-465f-bbb7-81cc9528dd36")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf78c16b-0157-4dcb-a6f0-b2f21f5f8a77")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f705a6ea-e089-47f2-8497-bd4d21a68327")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0736f88b-74cd-478f-a8bb-c93d6ca73000")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d28ec65b-854b-4521-a663-a89bba8a3806")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af12d7df-8a65-4627-ac21-1547e687f968")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18d3b33b-a59a-4ca7-93cf-8f3e4b7149a1")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8336a99d-ca71-4b2a-adea-9860378ba4bb")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07479e09-5851-4396-a0a4-20c69fec4450")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a092a88-8faf-4444-9fe2-a3481fc769f9")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e64edb8b-9281-41e9-9665-d3a7b33967ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "abd3789b-8155-4ea2-bff4-998a8a95f33f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "73d257cd-191a-4fd3-827e-17b1a7c0eb7e")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "dc22aa3c-ced5-468a-b88f-cb2f016ad816")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "03e3129a-578a-4412-8a02-60fb42d21844")
		(at 75.5 83.04)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2593596a-1f6f-44d4-9779-5388380ee65b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8db7e773-57b3-474a-95bd-440bb1bb2080")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2c1579c-2372-4c51-bcf3-155afd3785b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d62d998-402b-4505-bc75-384f57228660")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/62d9f82c-cd0c-44b7-973e-820165a4dc43")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3027ae4-8a42-4e86-9b58-5c8f518c2963")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abf24515-8474-4c38-88df-53efaee00249")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2e8434c-fbc5-4b85-bf7c-2e183a08199b")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bb0c493-de82-43d0-a2bd-50743e907f9f")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab77fec0-710a-4a43-a5fa-20fd72ebbdc6")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ddb51b95-bbeb-4539-838d-b5d9ad779114")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4107b4f3-c812-45a3-a113-e3d444bdd1ab")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e953a806-d23c-49d1-b40f-15bb34d1be74")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6474232b-d541-4e74-a6c1-b7abe6511b1a")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "635cb6e1-785f-44af-bc39-7d1737d636d3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "78e6e07d-433f-40eb-8d96-625e1c76f800")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/电源/VRA1")
			(pintype "passive")
			(uuid "63dc98c1-7920-4f08-bfd4-6cf2328da8c9")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "41588d3b-a0f9-4d3d-a1ca-c3f5e6e3199b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "071f6dbc-b573-489d-87ba-f6e242d38e42")
		(at 64.75 117.16)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "3dfdfdef-7e48-452d-9505-5329f633d0ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5f178a28-2e78-4e9d-8afd-9217cad843e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd627241-a845-4c7a-bf5d-2c6ec00c6df3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "538d23f8-e973-431d-ba39-4062dfdc7d15")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/d8dd88d0-edd5-480f-bda4-ba7d12b1eb87")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8a0148f-c647-4d49-92d6-cfe35ff2fbe2")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9afb8eee-035f-4809-94bc-86e660e4cf91")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e79dd5c-e08f-4b28-964a-3b337c2778d0")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37238fae-3119-4af3-b9ae-ffa580cca6c3")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b64ab29-fd48-4964-863e-9f90382382b1")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5377a0e-2239-41ce-a85b-c6a4f9711310")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c4050c8-4cc9-479b-b36e-bc75e698aaac")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbe21b8d-77cd-43d7-94cc-7430227bb676")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e3bc74a-9fc4-40ee-b681-221ec3af4127")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "658e41a8-ee23-4f28-89e9-51985f0b6c99")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eccb9441-ac95-458a-94c3-0ce067482a85")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fe437640-4e89-4aa0-a452-995d56ea5157")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/网口/XTAL_OUT")
			(pintype "passive")
			(uuid "8ac3470d-f6b1-4895-92bf-a40aa67a90b4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "091c77e8-7e10-489a-b8d5-a8fc0a7ae321")
		(at 81.45 115.05)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP11"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "47b607fa-5e4f-49ff-8370-ce37dfa2c0b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BT_UART_RXD"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "3a4dbbff-35d8-4653-a89e-db9f40283b1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0bb2022-d2f3-4946-8261-e600a02d401c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "999b9ce9-b74b-4b6f-bea6-693e3e76d6fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/e74b8d78-3806-4b81-ac05-7186834ca0ad")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "c90143e3-8f9e-4b13-bbd3-5bd6d33c261b")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "adf309e1-c8ae-49e1-a209-3141b5901dc4")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "869b5494-aa2e-4d9f-b4c8-091dd5338c18")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "406a4062-7aa2-4a40-9163-24ac0b04cd0b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "561935e5-9570-4744-b414-d30b93b54128")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "/网口/UART_RXD")
			(pinfunction "1")
			(pintype "passive")
			(uuid "bbcc9d8f-9bb1-46e4-b6ec-e7ac060a864a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "0da0a4a5-2489-41c6-abc5-adab7280d503")
		(at 71.49 83.04)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2d266366-1cba-42f5-982b-886789f7918f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "f46a9ad4-1aec-46ea-8d62-d438f760da4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "07a493af-c8f4-4b76-adab-f8d15bc57b9e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a795cfcb-5cd7-4848-948e-e7774b7c3611")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/83a2d945-063f-44a5-978c-3d3114c881eb")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "529b17e4-a186-47d2-9d98-c83038e825da")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a621f6f6-cdd0-411d-9ae2-1c5387e1fa49")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41f916aa-93b3-40c1-b5e7-d93cffeb1422")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf0a1066-78f0-455b-9cca-b29fa2af4278")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58a97900-d384-4a7e-a2eb-bf93a101c6fa")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9021051-29aa-4597-8aaf-a326c1fda9f0")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03b8269c-2c1d-4949-bbeb-c6c239f7f0ad")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e499c84d-9787-4dcb-9699-f330a7a05332")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "daea820c-a017-4a99-bbe9-51beaffc4760")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a04d0559-4d5a-4c7c-b11f-c422d34e474c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a7d6ca0d-9b92-4bb8-872d-baf7e9b06b44")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "68ae51cb-42f8-4a56-b9e4-1277563a2a0d")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c70c943e-5b2c-4c6c-9b32-6ff8339fb852")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "1293ad40-75a6-4cea-a612-b40dca22c86a")
		(at 72.77 119.67)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "05b8f9a0-febb-4576-8044-5ff30404eed9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "e8a72b02-a234-4015-8838-1b6581e9360e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a78f8c80-904e-4ed2-bd61-a9174f65ef49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66adc2b1-5027-4445-8a5e-c43a480879c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/3545fad9-b4a9-4801-96e0-1bdf1fdca746")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "325c70b9-7890-42e2-abcc-c8fdc4cad49a")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7288397b-6907-4aec-a924-51e23640f936")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b29b14c-43fb-4231-a31e-966991408039")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d8ed3d9-17b6-486c-80b5-74eb73d422b9")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4bbf693-64f2-426a-bd09-9c419f47c475")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc771008-c953-46c8-aa93-4863db7e4964")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a24da69-c8ae-4990-8b76-a8ee463aae85")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dd6a789-7ceb-48f5-ad96-bde5bccb9acf")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7dc052ca-f4b2-41b7-ab8d-a7c9d00dd73d")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd3b563d-90c1-40a4-bc61-b967e39c6bba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c9023bd2-ab20-4040-a508-2d2475e037ce")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "PG3{slash}SDC1_D1{slash}PG_EINT3")
			(pintype "passive")
			(uuid "c775588e-f815-4925-9111-2a278d7f6b13")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "4d58e54d-9701-4686-b6f1-d83dea9d3177")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "15f443ae-33d9-429b-ba8d-2122078c2ef3")
		(at 72.77 117.16)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f2524747-6836-4cd3-8732-c1ebf22d62d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "237815ad-a5a4-40f6-97f8-d41c1e46ec38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56cdfa7c-29f3-48e7-a2d1-79a1a260783c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5328e826-738a-477e-958a-ccc5503d92cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/03572c85-9ad1-4588-974d-986c6add8bb8")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11b0b09a-4f14-45c0-a7c4-59aa9960fa1e")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8e3d97b-c481-497b-b0d7-112a5a505184")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e9bd6e7-84cb-4488-bf3a-cb373c8e34c5")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "092b5dd9-3f9d-47e2-a000-92e582d42e5b")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c55489ed-3271-402c-9591-a2b86ccc5edb")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42559a52-4b2e-46a2-8c89-5d36086d6480")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e044571-86b0-4a82-aa08-24d724ec73c2")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77975383-987e-4fe9-9b5d-712717d1bbda")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b879195e-aa80-4b9b-9e2a-ab9a2cf2d2df")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de668bc7-984d-44e6-b643-cca5c21eb609")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7d1ee8cf-d342-44f0-9d29-bc92fbcd4e28")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "PG2{slash}SDC1_D0{slash}PG_EINT2")
			(pintype "passive")
			(uuid "2714d11f-be93-426a-ba93-68fef3ef02a8")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "2cee015a-5812-484d-b347-3e9080a582f5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "178018e0-db12-4b2c-bda4-f0378f7a6d0a")
		(at 87.75 74.2)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP5"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "6c626c69-9a1e-4623-b744-836b2549afa4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3V0"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "462e94c0-a56e-4b9c-99c4-251cb772b97a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4b887b4-f2e9-47ef-a384-f168cd80e1dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "40c7479d-c9ab-4ac9-970b-52da0e01d691")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/65cc509a-6aa7-487c-bae3-01eadaf167e5")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "2277b909-3505-46ba-b6bc-211420f42169")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a32c467d-725a-4d0d-bd00-dd4e3c23bd94")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c8b4eb2b-88cb-4f3a-9301-d10d9a04f76b")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f346f474-592d-462b-99b9-9dcd8d5ab4ba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "48bba8ef-9d0c-48c4-9072-51abfaf21797")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "+3V0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "e583238a-2ab4-40dc-a499-997132bc92a3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "180bc46d-82ff-4883-8abe-5751e56cb02a")
		(at 77 110.6)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP6"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "f064e061-2909-4b3f-a5be-fcdd58d2fce9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "WL_REG_ON"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "7b75892c-5162-43d5-9be7-7e0a13eb80cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e0caf6d-40e7-4545-9fdf-e6a628fddea1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ae563f38-87a1-44c1-99d4-71820b0d838f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/6846302a-fa98-48a6-9753-b362e83f5a97")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "8deeb5ae-48bb-4976-8224-856302ecf294")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "06e97b8e-b2c9-46c3-aeda-1a5ee1525fbc")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cb6c3983-2211-4d91-8dc9-249cb33631a4")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "45000ed2-31f2-40ec-bfab-19e783987a5a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "67c2266e-9408-48b0-8ae2-592dd59247aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/网口/WL_REG_ON")
			(pinfunction "1")
			(pintype "passive")
			(uuid "8d3adc7c-2668-488f-81f7-135b5ebe8e50")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "190151f1-19be-4993-80d2-ffc18df2d130")
		(at 64.75 124.69)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "342d7f8c-4b2d-4ff5-8a54-420c835a3ede")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3dce6a32-6948-49eb-a8b3-077a84bd2e27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be4fe222-94f4-4e24-92f7-365a24c859d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a21d11ec-8ce7-4e45-8b55-1fa092073470")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/21eb9cf9-253d-456a-a4e0-632949c52c58")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5199ff98-005e-4c85-ab3f-179e6eab9f3c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de6face7-d903-4267-8503-408a280d7fbe")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b597a11-f52d-49f6-88f3-3bcff8bf0ebe")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50b3d3b1-a063-42bd-b8c4-80c583c44e44")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8492b9d2-bc93-421a-bbba-421e414b569e")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4dc0de12-4d1a-49fb-8a45-bdb081e34df3")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70ba65ec-d2c3-49ed-977c-a0f5b60a281d")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bc8cce2-fa31-4645-a128-9b44938416cf")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3d471cb-1b3a-4051-99ed-97abf8b17dc7")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b5df1afa-ee0b-4a18-9b66-9420c1dd6008")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c287a6e9-e948-4d08-ab93-a8a452907642")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "bc261012-db2f-4bbb-a137-972dae17d8da")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6d94b75d-4c75-46a7-b99f-42c6081d6e9d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "1c5ecbd6-10b1-4187-8a4b-b0a331b9ad38")
		(at 83.52 60.45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f1810ae8-0aab-484c-9471-ca115777d241")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "84c15447-67d7-4088-9d70-b902e3f5a5f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65a7a920-90ea-4d6b-8708-3507e623cd8c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca5e6873-ba12-4f33-9d2f-a46f129c0145")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/29d3df5b-ee61-4464-8870-3916288c67b9")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77d19e81-ab96-4a66-8bac-aa58bb91bbd5")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39bdf9a8-28d0-442c-997c-32aeeb195172")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "681e6047-37b6-4059-877f-3f58ca0b8a3d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f976da3a-747e-43ed-a42d-59fbb8508cf2")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72862f21-16a1-4147-b0aa-4e040427922c")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9315bb1-7992-4e2c-87f0-20ef4122140b")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d12c91b-8a2a-42f9-9a1b-52a076db77d9")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "074c3a19-db27-40ec-b5e1-edca5cbe8653")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bd1c091-ab17-4a76-a5e8-475ba5d40d49")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2124f6e1-37f4-42b1-b233-4cc19f0a3444")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dae20aef-b76b-47e9-a24d-3b6c0def8bb3")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(D2-A)")
			(pintype "passive")
			(uuid "dc10a5d9-c928-4660-bfba-fcec8779b844")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "Net-(R10-Pad2)")
			(pintype "passive")
			(uuid "b75bd1cf-e68d-49b9-94d1-5212e02f07ba")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "1da6adcb-2da1-4f1c-a250-da5ef68d2372")
		(at 67.48 55.43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "de167331-f4e7-4113-9e42-73fb696bea47")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "1e332c8c-d239-4e71-af1d-640a2531da33")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68a7b5b6-0688-4bfa-908d-593b9cec7baf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "990f27c2-fa7c-49f5-9ac4-9489f1597503")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/c10550ab-8649-48a3-9b01-d08c2d7516be")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4309d63f-5ec6-4f5e-9ac6-5ab17c1e1694")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e3935e7-47ad-4ddd-b7d6-8fefea02c559")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf7b0f0b-b802-4334-90f4-e342d98bd659")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59a545e4-b56b-4c79-8a38-d45299685457")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86e8b387-4744-40f2-81bd-bcbea35dd0be")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7b13960-2ab0-42fe-9fa0-22dde4aa3975")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fd2d45a-0d7a-44f9-8125-fccde50c11ed")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f5a160c-bd68-44fc-9bdf-304d24025a1f")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87fbd74f-5fbe-441d-827a-43e9d0b61010")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be448bae-9cce-4d5e-8809-348f46893811")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d7883be5-ca8d-42b9-9931-6f27b29415f7")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "9054de00-1f49-4017-8559-bf29396d1425")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "97dbaf67-5d29-45bf-a259-bddd5eda0ccc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "1ebd930a-4c5b-451b-abee-68ac3a0ad772")
		(at 67.48 62.96)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "c7cd950c-4025-4312-bee8-eec8e869da72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "dcc248d4-8ff0-4ca8-a3a3-72f5e96d7caf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af1720af-179b-4cec-970e-744e91f7e157")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "99b7f32c-7c26-4e2e-8dcf-e94f45bcc094")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/9c965528-fbdb-4263-8e35-87aa70f863e7")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c24868d-b47a-4afe-ab9a-96e438b3ff2c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "851ba292-d9b3-4ded-9687-a14ae9f64b95")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8c38a12-fa05-4831-8913-c3f41330b45d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "471d9446-c219-4d44-a2ad-2465d420cf6e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e974939-80e6-4fd0-91f7-394e8e8447fd")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "473db382-e9c2-4e0f-861e-936b60a8fc59")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02780598-5d65-47bd-9bea-5a9b0605b4d0")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3583b4f6-bc4f-4a48-a07d-254f8b6c6049")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcc2f9e3-a565-4565-93cd-76e2e0eae1dc")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f1b0fb1-8aed-4c61-946c-a98170f76717")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "49fe4ff6-4371-4696-92e5-ef1b04e453af")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pintype "passive")
			(uuid "8314049d-9c03-40f6-9f11-e5643fc572ff")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "99ea4c61-3f73-4000-9669-f7bb7e81f30f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "1ff2b71f-fbda-440b-ab37-ab09b12ba349")
		(at 87.68 97.87)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "53207278-69e8-4c1a-a303-fb5c51770126")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3e1b0041-4d4c-4711-978b-ccad33aab212")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cfff2bc3-5168-42a6-bb9c-1b633368d9c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f9637618-7ca7-4735-8107-3b2f1e07d13d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/78febfbe-3e15-4875-8c3b-6219e0f2a097")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34bfaaa8-f5ca-4263-b97d-7535903eb94e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11671da1-0945-41de-95e8-2e2795146c09")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "206cd53a-51dc-4010-b8ec-0c419cf34186")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09f9fc67-a61b-473a-ab13-8f41c6168e3d")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59598989-62ae-40e4-8dbb-8314df233be9")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24609155-46a4-448e-a312-4485d493a9c1")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4de96ee1-3ff8-4c0f-aa31-6f77e4adc56b")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1655529c-fe06-4c79-b882-42708a49c949")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1e40a41-7da7-4e69-acfe-282d79e8628b")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "892ec2ce-b45e-41d5-bb4f-dc1915b09e85")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fb56235f-eaf9-4e92-bfe9-6d0f1feba5e2")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "86bc3c79-1d01-4a5b-abdb-df578d85184b")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d6434495-4394-47d8-8de8-82d2ee1c23f5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "20991c32-5cdc-414b-993c-29946075843a")
		(at 67.48 83.04)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "92e333cd-5550-43d6-b9d6-64259a2abe5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8240d79e-4d1a-4f09-8bed-eeb4b7b40dbc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f8938b11-37d5-4022-894b-21af762c85cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c36988e2-7609-4ae0-9ecf-bc6361affd0d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/03181abc-e528-4076-82dc-fe2dfdf85c4c")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5a3278f-cd39-4c9d-8723-495198df73f4")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cc9685b-132d-42d2-b59e-c684ec9b4ba9")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df65de63-79f5-4e0a-87cd-0f2e62cfe17a")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9d7db11-4d1d-45bb-abb5-dc36ad330697")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fef06f39-7244-450d-ba0e-03d450709be7")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c2d4159-6f4d-46cd-a848-198927147e3f")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3048d66-6bcf-43de-9392-36167d83f6ba")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "060d8ab3-6e9b-41db-8213-d173f04f6142")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f91174a3-6ed9-4647-9fd5-10ba882baf6c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "863f0c58-2b77-40b1-b419-7f926de65c7a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "00626dd3-3afb-4b32-93a9-2cd70e2221b7")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "ecc6a0f9-f20f-4281-bd25-cccb39940a1f")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "11008f4d-b342-4f67-b744-e34193051c76")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(uuid "23329898-cac3-4f3b-befd-6685616a608d")
		(at 92.85 66.55)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -1.9 0)
			(layer "F.SilkS")
			(uuid "93fa656c-ea20-4ff8-b123-32ca5e7406ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2uH"
			(at 0 1.9 0)
			(layer "F.Fab")
			(uuid "dc8cab3e-61d6-44fc-a43e-d6b85fd04b9d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a0453ce-47f7-4267-81a2-e576f4efa715")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45c1440a-a458-4d8b-bab6-77d512ceb756")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/5551f077-86f8-4738-8364-e2b22176b110")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.835242 -0.91)
			(end 0.835242 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02209394-4e77-4fd1-ba42-4e223d0f8000")
		)
		(fp_line
			(start -0.835242 0.91)
			(end 0.835242 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1ffc33e-4830-42fc-8c50-71c156c7fd40")
		)
		(fp_line
			(start -2.35 -1.2)
			(end 2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a51f89ce-b80e-469a-8307-0fec09904e73")
		)
		(fp_line
			(start -2.35 1.2)
			(end -2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af346f1d-c6f4-4625-a53d-6d722dea1b85")
		)
		(fp_line
			(start 2.35 -1.2)
			(end 2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bdd2be7-6ef9-46b8-b4b2-7882a53ceba3")
		)
		(fp_line
			(start 2.35 1.2)
			(end -2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27d7696d-10f5-4f97-9da8-c836ec88225d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7435eede-9562-4f76-9501-47f02b8a2e26")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0caf1c92-42fa-46df-96b7-e2a22555298f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f53d536-d2a5-4d02-9732-64779ba4357b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c079d900-6699-4512-b1a1-b0e2f285d065")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3af54ff3-b307-4f4e-94b2-21b6a46297a1")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 6 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "bb82f5f8-319b-4cc6-a9c5-973ad84ee002")
		)
		(pad "2" smd roundrect
			(at 1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 76 "SW3")
			(pinfunction "2")
			(pintype "passive")
			(uuid "78f8eebb-42d7-4667-aadd-17f69e87139c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "248aa37e-549e-4a64-af94-a676691eed35")
		(at 75.5 60.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2dc62bb4-251c-410c-a1bd-475927a26d19")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "59261831-dc21-4ea7-8b4c-a976ed90973e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e21d383-6fd6-42cc-a716-cc8c2667e34e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d5e413c-ab6e-482f-925b-feee311485d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/ea49db43-4f17-41d7-acef-85ea05e9ec2d")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64291380-e86f-4df2-bab0-0d66af1ecb5d")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97ab669d-5b11-4fa9-870c-09180c03916f")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da450209-e17c-4795-9e22-a1d1ef30c17c")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7af0757b-75a2-429f-a730-babfea02be79")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d5433ae-89eb-4ea3-9a40-eba6d7538f97")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "513d665e-8eb0-4c1b-b1a1-5753a09e6da3")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b6dfeb9-83cd-43ce-a30e-57f27d6d679f")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71b6cc40-077c-4842-a8cc-dfb256cc8b12")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c02be0d7-12ce-4a3b-89c3-ec8c80e2afc7")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5800bfdc-cd9e-40c7-9aee-f7dabeab6fb3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f4c8de7e-533b-49c3-909f-ee76ae33ecea")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "RTC_VIO")
			(pintype "passive")
			(uuid "e4ad4332-d5ac-48d6-a0c2-0132d7ee3470")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "40ff9e8f-a11d-41b4-ba76-4cdfaf5665f7")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "2ad38838-2ce2-4d99-9760-6e3d8d15332f")
		(at 64.75 109.63)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "720fbc71-10db-4e53-8dc7-d65c7bea5039")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9d09e5e4-4c3f-442a-aa18-f25526783a28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1714e5c7-3808-4cc7-8e9c-656e31ecae7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c19f55df-1626-4a78-b63e-63b926b9e85c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/50f81028-9180-4d1f-ac6f-9093c2e1afee")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0780049-7c57-4ea5-817a-5f8f3c02cf67")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5800dc7a-e028-4b03-9eb7-ba2f11463089")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89789594-a2e0-4613-8769-ed1afe759c5a")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfd8c73a-beca-4745-9994-fc3f728a5661")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a0be8a7-fbca-4877-945e-f45bc05b9c23")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1378fbcf-f856-4242-989d-e92f043e13d7")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b34644a0-7f8e-4717-9b51-e8e530237c7a")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6134397-e265-47cc-b548-1e787879c74c")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bae0c41f-3fbb-4240-9786-d823f7b55e3d")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b45619ad-a538-423d-8766-267900645df4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "75c75e61-e227-4f0b-a875-ecd00f072c25")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "33bea161-e394-4ebb-a06b-d35784c4fe52")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "4bf911ce-f4cb-4109-9087-ca82d411fa12")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "2bb53333-2c9b-4a75-a03e-bec8c1c5a1dc")
		(at 71.49 57.94)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "fdb4616e-394d-423f-b4f7-35a094a900f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "1aa2641c-ea4b-4d6e-97ed-dc7158577c64")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f53676e9-daf3-4270-83d2-b2df90ebf8ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "667706a7-880c-493a-a0a4-dfda5ce3703d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/e886c1da-16ce-469d-8064-58d32c52283b")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f4c451f-b952-46eb-a7b1-df6022c354e5")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "070d4f9b-efd6-455f-9d8e-af75afa2c461")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e6e4ace-27d3-4bcb-975f-6cf7e5f1582d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b1e6200-a1fd-4c0b-aa6d-477f3f2413a6")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42531b82-7372-4bab-a7d8-6df11017dae0")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e116e5b-80fe-461e-b330-6ed25f99fc84")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "554429d6-7f19-43da-95de-d464583e5fd8")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bdbae78-54b4-44ce-947f-91e3dd93cbee")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "710c94db-fc9d-40d4-826f-54ada2022956")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e374e326-c06b-40af-998a-40f9bc47882b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ac827aa3-500c-49f1-b533-891cbeb13999")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "25a6c133-0fb2-41eb-bc5e-3ace2a8cd988")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "1ce00212-2416-46ba-8595-5f7679c4ec9e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "2c77e026-7428-4713-a10d-d475192b2747")
		(at 64.75 114.65)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "984ef978-06ce-40a6-b53a-f41a6a7d4b26")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "248730d8-578f-4d9b-8fa9-44ebeebfdd88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "010e6096-75b4-4e65-a406-6ea0a7874435")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98fec5dc-c6cb-48eb-afd0-065ae07c7e33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/4fb7208a-fe17-494e-9fb7-da0171d1349f")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab81a2e4-37a2-48c7-8808-42173716ce9e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b069b7d-b2fa-4d1d-a405-f91e1f6e1425")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f1e3589-65bd-435b-87c5-4b339131ac3f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "195085fd-ee8f-4662-8d60-8e0dd9369562")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4678522-3092-47b4-b371-51e38d3ea504")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "666d7ea0-c07a-468e-99e5-2fa7525ec498")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96777ceb-a017-4d15-9cfa-80af1106eb4d")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd7f6bae-64a2-4a7f-96f9-f7d022d1e61e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ba04889-fd89-4578-a27f-f4ee341c8a1e")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7aeb63e4-3194-4793-96fd-7250a3ff33f4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5b7e49c9-d58c-4f9f-a047-25f01962ef3d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "50010858-4c6f-43c5-bab7-8be368d8a34a")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/网口/XTAL_IN")
			(pintype "passive")
			(uuid "e8908da7-9748-40f4-bce0-f2b6fe30ab16")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "2fdfb89b-4a83-4429-b330-92a50a773d81")
		(at 79.51 70.49)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "c16ed1cd-48fd-4809-88bb-a3be49bd2712")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b65a08de-0d22-4880-aafb-59858a808f65")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e936ba9f-8b48-4484-b5cb-9931d2cceeec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "439533ef-4952-411b-a917-277c64e2705c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3316b7ab-ec5a-4e0a-ae5f-ffc0d5503291")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6567dfc8-7e3b-4c74-b030-5ab4d59063be")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7937b03-8f3c-4704-b672-5281b480b018")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8a5c787-cec1-4c02-96f3-2a6709f5831b")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21f73b7c-357d-4e4b-bfaa-ed420e6bbed3")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1dd712aa-6337-43c8-a2e3-b37811e7ffc0")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12ac7079-cea8-4589-bda5-9ab2eb8fcc4c")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b6bdbfb-0bff-42e5-9eda-35255469626e")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf9a4f4f-a3ad-4d6f-bebe-89a6aabb06e1")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81583833-8bdb-4538-bcbd-e2c47b0f6b2c")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01bd23b6-beb3-4a34-8efb-c40a31ad9693")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c037e9cf-bb09-4c6f-98c4-2ff5bb3c45e7")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "28de0c00-d10d-448b-83b0-d3eea7c23915")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "FB3")
			(pintype "passive")
			(uuid "27f8f46d-1c23-443d-886f-1d5c47423173")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "30e99982-9dc6-442f-9e72-4b8b7fd03524")
		(at 75.5 55.43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "914bf851-9b0a-4970-aeb1-9e8c6279cd03")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "2b16f8b0-bd02-4800-9a23-049730b5ee2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd1faa00-b2cb-4af9-8413-a550c591ef61")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "807fa10e-67d6-43a2-9eb7-49f09ff1c973")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/b5800c6c-aa56-4d7d-9919-4e745f61cb47")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42c57345-c0e3-4383-9b3b-2fdf63f45317")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ea357eb-6642-4909-8ee9-f0b061b72502")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f459301c-d84c-4b2f-a9f6-15d18259c592")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c42e128a-6398-4a74-8d45-1df67fbc3ba6")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "791833d0-1bf7-476c-9a77-adc7d657582e")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50de6015-7d03-4b12-885e-9f3677370d25")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4660c9a4-bc4a-48ea-8c54-b93b36021f9e")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "942e2185-8eaf-46e1-8543-b35138088612")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34de9076-3c58-4d14-9dd9-3c8701296a21")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc5d5fab-bf81-4f98-9a52-b7434bdd98b1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0ea11c06-5faf-42e3-b2f6-c8f1ca9520e8")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pintype "passive")
			(uuid "d881388c-a9fa-4aaf-8a07-e1a1777a1879")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5885a302-6746-4dde-a038-0f08b9fbb7cb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myPCB:FPC-SMD_40P-P0.50_XUNPU_FPC-05FB-40PH20"
		(layer "F.Cu")
		(uuid "31b16b2a-89d5-4b60-b75c-24ba39b8f5b1")
		(at 118 105 -90)
		(property "Reference" "J2"
			(at -0.156 -3.022 90)
			(layer "F.SilkS")
			(uuid "14d00f15-afc1-4f91-b057-33ae5fcb6664")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify right)
			)
		)
		(property "Value" "Conn_01x42"
			(at -0.156 -4.8 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c011ce57-df71-4471-bcc2-ee91694ace11")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify right)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8d1f12e-f43b-4122-8097-919c44e9c6d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "\"Generic connector, single row, 01x42, script generated\""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb7a96a2-b3a4-4170-849e-75426693bb7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/96087d05-830b-4291-bb79-79ecfa65573e/a624cfdd-82e3-40d8-852f-766e772e695e")
		(sheetname "/RGB屏幕/")
		(sheetfile "Display.kicad_sch")
		(attr smd)
		(fp_line
			(start -11.75 3.55)
			(end -11.75 2.756)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffbdb244-54df-4514-b967-59cbff6c9fb1")
		)
		(fp_line
			(start 11.75 3.55)
			(end -11.75 3.55)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c13bb8cb-d81e-42bf-a6e8-8729fc72e577")
		)
		(fp_line
			(start 11.75 2.756)
			(end 11.75 3.55)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "074095c4-3f7b-481f-9bfe-223a3194b6c3")
		)
		(fp_line
			(start -11.75 0.494)
			(end -11.75 -1.1)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d94800da-3fdc-49d2-941e-0dd4a7e3717d")
		)
		(fp_line
			(start -11.75 -0.95)
			(end -11.75 -1.4)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb048928-ca38-41c9-8ab1-5f46c05f28a8")
		)
		(fp_line
			(start -11.75 -1.4)
			(end -11.15 -1.4)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b7ec78f-2781-428a-a1c8-b2564fb5e1db")
		)
		(fp_line
			(start -11.15 -1.4)
			(end -11.15 -1.9)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25ac3a90-e175-4fe4-8bcb-678bbdae4bef")
		)
		(fp_line
			(start 11.1 -1.4)
			(end 11.75 -1.4)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c67bda6b-37cb-47e2-a7e1-c4ef06a8e40f")
		)
		(fp_line
			(start 11.75 -1.4)
			(end 11.75 0.494)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acbca7d9-c72c-49f8-8ceb-9791139a1314")
		)
		(fp_line
			(start -11.15 -1.9)
			(end -10.131 -1.9)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d87f0b9e-b952-45d9-a9d3-02edaa91e8de")
		)
		(fp_line
			(start 10.131 -1.9)
			(end 11.1 -1.9)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91580eed-3107-46ec-ab75-7e7ff2d796c5")
		)
		(fp_line
			(start 11.1 -1.9)
			(end 11.1 -1.4)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1eff4104-4c42-465b-8248-27dff5fd1e03")
		)
		(fp_circle
			(center 10.399 -2.355)
			(end 10.608 -2.355)
			(stroke
				(width 0.254)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "3b947570-e780-4863-88dc-f82008276309")
		)
		(fp_circle
			(center 9.75 -2.05)
			(end 9.9 -2.05)
			(stroke
				(width 0.3)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "2a14856c-49dc-4eab-90ae-8f437d17b203")
		)
		(fp_text user "gge8ba4c923b92839f6"
			(at 0 0 90)
			(layer "Cmts.User")
			(uuid "b88d954f-75b2-465d-9242-ae8908b2bd13")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at 9.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "1aa8ba7f-b629-43e6-8743-6fc5e82685f6")
		)
		(pad "2" smd rect
			(at 9.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "698ae04a-60e4-400e-8989-b8c78cb87087")
		)
		(pad "3" smd rect
			(at 8.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "896391f9-e768-4dfa-a0ad-339dafcc8e0c")
		)
		(pad "4" smd rect
			(at 8.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "3dd2b06f-5bc4-42f7-8cb3-82efbfff964d")
		)
		(pad "5" smd rect
			(at 7.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "PE16{slash}CSI_D12{slash}LCD_D18")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "876ba496-a706-4a01-b5ce-a4340decd891")
		)
		(pad "6" smd rect
			(at 7.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "PE17{slash}CSI_D13{slash}LCD_D19")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "9ad839ce-fc1d-4918-bee8-ce838e89dad2")
		)
		(pad "7" smd rect
			(at 6.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "PE18{slash}CSI_D14{slash}LCD_D20")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "66500033-691d-4c20-a6db-fe3a8e92f602")
		)
		(pad "8" smd rect
			(at 6.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "PE19{slash}CSI_D15{slash}LCD_D21")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "49433e49-4aa2-4f03-8993-33645c42f22f")
		)
		(pad "9" smd rect
			(at 5.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "PE23{slash}LCD_D22{slash}UART1_RTS")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "3945cfcc-da0b-496f-9bff-2bdfbb3a0978")
		)
		(pad "10" smd rect
			(at 5.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "PE24{slash}LCD_D23{slash}UART1_CTS")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "9e9c2d2f-363a-41e7-a1a0-07fb04a2e664")
		)
		(pad "11" smd rect
			(at 4.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "89fba1e3-d84f-4760-a9b7-467203629429")
		)
		(pad "12" smd rect
			(at 4.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "21e3f2b7-a4d0-4746-bc2d-b50b561d448a")
		)
		(pad "13" smd rect
			(at 3.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
			(uuid "202c4ffd-d29f-40ba-a563-2f03e249fa51")
		)
		(pad "14" smd rect
			(at 3.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "PE10{slash}CSI_D6{slash}LCD_D10")
			(pinfunction "Pin_14")
			(pintype "passive")
			(uuid "b9a2cd8b-ef4a-47ea-a4bb-41ef1028d32c")
		)
		(pad "15" smd rect
			(at 2.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "PE11{slash}CSI_D7{slash}LCD_D11")
			(pinfunction "Pin_15")
			(pintype "passive")
			(uuid "9b36fcd4-472e-4155-abb7-6fdb1f1719fb")
		)
		(pad "16" smd rect
			(at 2.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "PE12{slash}CSI_D8{slash}LCD_D12")
			(pinfunction "Pin_16")
			(pintype "passive")
			(uuid "4da62fcb-5aac-43ed-baf1-ab168bd373ca")
		)
		(pad "17" smd rect
			(at 1.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "PE13{slash}CSI_D9{slash}LCD_D13")
			(pinfunction "Pin_17")
			(pintype "passive")
			(uuid "fcb22235-1f2d-43e8-a017-548db711a6e6")
		)
		(pad "18" smd rect
			(at 1.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "PE14{slash}CSI_D10{slash}LCD_D14")
			(pinfunction "Pin_18")
			(pintype "passive")
			(uuid "3b662a9f-74e4-421d-a3e1-d468e38e246e")
		)
		(pad "19" smd rect
			(at 0.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "PE15{slash}CSI_D11{slash}LCD_D15")
			(pinfunction "Pin_19")
			(pintype "passive")
			(uuid "f83161f4-277d-4fd9-bcc0-a9aac339c9c5")
		)
		(pad "20" smd rect
			(at 0.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
			(uuid "096cca05-4c79-4597-99ec-da5dc4675144")
		)
		(pad "21" smd rect
			(at -0.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
			(uuid "6611907f-f590-437e-a41c-55eff0c556c7")
		)
		(pad "22" smd rect
			(at -0.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
			(uuid "3a239e04-714f-48ce-81c5-5251d0279b04")
		)
		(pad "23" smd rect
			(at -1.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "PE4{slash}CSI_D0{slash}LCD_D2")
			(pinfunction "Pin_23")
			(pintype "passive")
			(uuid "d774b9c0-f73a-403e-bc73-0261471ad46a")
		)
		(pad "24" smd rect
			(at -1.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "PE5{slash}CSI_D1{slash}LCD_D3")
			(pinfunction "Pin_24")
			(pintype "passive")
			(uuid "f8d1fb5d-c7ca-4fd2-9b06-3b13621d9f79")
		)
		(pad "25" smd rect
			(at -2.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "PE6{slash}CSI_D2{slash}LCD_D4")
			(pinfunction "Pin_25")
			(pintype "passive")
			(uuid "a8403332-aad8-4156-a28e-5d5fb4d30ce4")
		)
		(pad "26" smd rect
			(at -2.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "PE7{slash}CSI_D3{slash}LCD_D5")
			(pinfunction "Pin_26")
			(pintype "passive")
			(uuid "dfb061b1-071a-403e-883b-068de42492cb")
		)
		(pad "27" smd rect
			(at -3.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "PE8{slash}CSI_D4{slash}LCD_D6")
			(pinfunction "Pin_27")
			(pintype "passive")
			(uuid "340424b7-fa1b-4b79-8271-62db9306c1cc")
		)
		(pad "28" smd rect
			(at -3.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "PE9{slash}CSI_D5{slash}LCD_D7")
			(pinfunction "Pin_28")
			(pintype "passive")
			(uuid "772ef107-8533-4b77-bbd6-c4fa4b80282d")
		)
		(pad "29" smd rect
			(at -4.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
			(uuid "f255a134-c6c1-47f7-85ee-a19a098f75e6")
		)
		(pad "30" smd rect
			(at -4.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "PE0{slash}CSI_PCLK{slash}LCD_CLK")
			(pinfunction "Pin_30")
			(pintype "passive")
			(uuid "23ac39a2-e7e3-4ee8-bae4-692823bdf385")
		)
		(pad "31" smd rect
			(at -5.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "PE2{slash}CSI_HSYNC{slash}LCD_HSYNC")
			(pinfunction "Pin_31")
			(pintype "passive")
			(uuid "8e10a130-ddae-4c6b-86f7-8a7e1ae6c9b7")
		)
		(pad "32" smd rect
			(at -5.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "PE3{slash}CSI_VSYNC{slash}LCD_VSYNC")
			(pinfunction "Pin_32")
			(pintype "passive")
			(uuid "0d9fd83a-f516-47a0-8407-45f8239bbcd5")
		)
		(pad "33" smd rect
			(at -6.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "PE1{slash}CSI_MCLK{slash}LCD_DE")
			(pinfunction "Pin_33")
			(pintype "passive")
			(uuid "8d622bfc-ce7e-4d33-9673-5eb0e9787403")
		)
		(pad "34" smd rect
			(at -6.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "PB4{slash}PWM0{slash}PB_EINT4")
			(pinfunction "Pin_34")
			(pintype "passive")
			(uuid "c0aeca06-5b1d-4cc5-8a43-00c3df780df8")
		)
		(pad "35" smd rect
			(at -7.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "PB3{slash}UART2_CTS{slash}PB_EINT3")
			(pinfunction "Pin_35")
			(pintype "passive")
			(uuid "98f65f59-1665-4295-b038-a2599b5a2b79")
		)
		(pad "36" smd rect
			(at -7.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "PB7{slash}TWI0_SDA{slash}PB_EINT7")
			(pinfunction "Pin_36")
			(pintype "passive")
			(uuid "46c661bf-b6a5-4b96-9bdd-5c99fd262467")
		)
		(pad "37" smd rect
			(at -8.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "unconnected-(J2-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
			(uuid "64ece6b1-8a39-406d-a0b0-ebaba4458a03")
		)
		(pad "38" smd rect
			(at -8.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "PB6{slash}TWI0_SCK{slash}PB_EINT6")
			(pinfunction "Pin_38")
			(pintype "passive")
			(uuid "cb702f65-341b-4ea1-8be5-0c553bca860a")
		)
		(pad "39" smd rect
			(at -9.25 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "PB2{slash}UART2_RTS{slash}PB_EINT2")
			(pinfunction "Pin_39")
			(pintype "passive")
			(uuid "558e5e23-410b-4a95-96ce-39b68e7c9d99")
		)
		(pad "40" smd rect
			(at -9.75 -1.625 270)
			(size 0.3 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(J2-Pin_40-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
			(uuid "0b0e527b-8d3d-444e-a900-491783ea3a31")
		)
		(pad "41" smd rect
			(at -11.3 1.625 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_41")
			(pintype "passive")
			(uuid "df079443-05ab-4fc4-afa0-dd99f1c0af5a")
		)
		(pad "42" smd rect
			(at 11.3 1.625 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_42")
			(pintype "passive")
			(uuid "a06c7309-d081-430e-b1d5-f865dff33599")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "32f7298b-21b8-41a9-b729-34b135a8c3ed")
		(at 71.49 60.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "7800b757-95ed-4f18-9be1-4f6cc540eacd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8f097aad-c2b2-4631-8c11-49c715712fcd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9bbbf41-892b-43e8-9e7d-6350333540df")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d8d7358-d065-47f5-a237-b943c8ab8274")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/4b22c244-6521-45a4-a479-ce9c80d34789")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "311f161c-30f0-4cec-b4ab-7e9010c9818e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efcb2f4d-c4dd-4130-a3d8-16d7946ba6a7")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ba2e615-695f-412c-915e-2158154852aa")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53f28f92-004e-4020-a74f-6be5360620b8")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "551425a2-c24d-434c-8a1f-0647fbe75204")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2f6989b-4b8a-4d40-8311-1b6916d69bb2")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "991cbd33-ec65-4fb7-a693-05d0abfd2b34")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd4c9875-9f11-4c0e-a951-82c512f4392e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f072efc9-b597-4bc3-96bc-e145d5ad2e1c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a93dcf46-c698-4ea1-bc8c-0297ca0a4728")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4d2fee41-ed32-4568-af09-07fcfc996421")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "6fc34492-2acb-4bfa-882d-74414967d4b6")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ed4e27b2-b77b-4ae5-b6f4-c86a4813c042")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "33083a7e-e712-4eb1-b99f-cccdc76588b1")
		(at 75.5 57.94)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "776fb933-179b-4779-a9d8-4db23d430bc6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "fd76deee-f54a-494d-ac32-35bad86240b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3df54c50-62ca-4c6e-8927-f9501bee01ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68f09c4b-97a6-42ab-882f-886fec2fc2ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/39a1d9e3-8e95-43e4-bee1-56711d5dfad8")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "329c0009-efc6-4e96-868a-4fc7f4d8d01d")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e3d29c0-1dd5-402d-becd-182f5c530a62")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b1c650d2-b878-4ab8-a67e-e6f2acf54f99")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a668d5e2-530a-4b65-8203-d3a4b42be308")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0cd3821c-d132-4ebc-bbcc-5e8497891256")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca202ed9-97cf-4e4c-bbc5-0088bef0f138")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39c47525-658c-4d83-a987-6178481011b3")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b63ea141-ba7c-4d92-a59e-5e8f420e0ff2")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89a63457-14f7-4af6-8e40-932fe33452ba")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c804c1eb-7856-4703-9aea-b17a95d28f38")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fddde78d-918f-4b17-8fca-8884fb88faa4")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "HPVCC")
			(pintype "passive")
			(uuid "9ced586d-558c-4e31-8dd5-1fde3b2bbcc6")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9644c4f9-b6b2-4615-a9e6-422c4a5998bb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "332e24c5-675a-41d4-a63d-eb7c3903f4e1")
		(at 68.76 114.65)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "69a6897d-febf-4970-a091-db1e940cea0a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8888e044-94db-42f3-80e0-58c654791dff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "11bbb39d-fd49-4813-b05f-d1a1ffa720a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc26d672-b6fd-40a8-80d2-daa4bdc691aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/94726fe8-7193-4c25-9d51-e25a9f279785")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68353187-915b-494d-bc60-e23bd8047e5d")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa9f5274-9bb4-4539-8a84-a09be0fcabb1")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d941125-a377-40e5-94bc-8c831f6fb8fd")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd3d932d-9fa7-440e-a4ee-b7371e5a9681")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1339af42-2021-49b3-8eaf-09e7f1de5361")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe2d3ed6-0bae-499f-bd51-e46432ba8d75")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da1dec93-0125-4694-9180-19d54d39a016")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57c8c1c5-e98b-41d6-a1a8-77e7a543e8ac")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f99fd89a-5ed7-4fdd-8325-231de724b215")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "174ab48b-8a47-4a5a-82e3-14c554793783")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "448a382d-6cba-4bb9-9b8d-58668626572d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "EPHY-SPD-LED")
			(pintype "passive")
			(uuid "c3ac19dd-5567-4f96-82d7-8470f168cb1f")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Net-(J3-Pad10)")
			(pintype "passive")
			(uuid "6a99bc1d-d072-436c-a29c-1988ddb838ca")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myPCB:QFN-44_L12.0-W12.0-P0.90-TL_AP6212"
		(layer "F.Cu")
		(uuid "349d9610-82f7-436a-8518-5ff2bf2ffb35")
		(at 136.111 129 90)
		(property "Reference" "U7"
			(at 0 -7.112 90)
			(layer "F.SilkS")
			(uuid "b99f05e3-459f-41c4-926f-53d19e616098")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify left)
			)
		)
		(property "Value" "2.4GHz"
			(at 0 -8.89 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a22af10c-76f4-42a8-92aa-93ebe64769a3")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify left)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c48370d-045d-44e9-95b8-5b85c57cd6c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "fab880fb-4b20-467f-a48f-977771f65c97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "AP6212"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5beef099-9a16-4537-905a-2973c9775a21")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "AMPAK(正基科技)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6292ad0f-b591-4e74-ae62-b9f7041d02f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C2798300"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a2320ec-c01c-4c09-b4e3-0b5008cca255")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d1162707-ccef-4549-8e3e-a6f10af8457e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/d2c4a5a5-fd45-46c3-8d89-7446dc0dd064")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start 5.994 -5.994)
			(end 5.994 -4.902)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "736e957f-d506-406c-9bde-8bf819b36a08")
		)
		(fp_line
			(start 4.978 -5.994)
			(end 5.994 -5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db483ab2-1ed0-4735-b5ac-d23d0228212b")
		)
		(fp_line
			(start -5.994 -5.994)
			(end -4.978 -5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d77841f5-950b-4612-bc41-69cc86e4e27e")
		)
		(fp_line
			(start -5.994 -4.978)
			(end -5.994 -5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e084348-9335-4d33-88dd-bab8e5322090")
		)
		(fp_line
			(start 5.994 4.978)
			(end 5.994 5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ff0e522-c3ed-4802-919c-8e5652b4291f")
		)
		(fp_line
			(start 5.994 5.994)
			(end 4.978 5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20c81519-7d19-4c3f-9764-683b4f301417")
		)
		(fp_line
			(start -4.978 5.994)
			(end -5.994 5.994)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d694e6b7-6e30-402c-b6d5-7f2ae49cdb8b")
		)
		(fp_line
			(start -5.994 5.994)
			(end -5.994 4.978)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca77c3da-2b11-4be0-96af-ad2ae3254896")
		)
		(fp_circle
			(center -4.496 -4.496)
			(end -4.14 -4.496)
			(stroke
				(width 0.254)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "3e24bdf3-ecfe-47da-a014-c9b22b807976")
		)
		(fp_circle
			(center -5.86 -4.536)
			(end -5.66 -4.536)
			(stroke
				(width 0.4)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "56638810-15e7-4579-8eef-468ee907169a")
		)
		(fp_text user "ggea42585d30999db3c"
			(at 0 0 90)
			(layer "Cmts.User")
			(uuid "48a3d058-29e7-47a1-bda8-19327f88a8b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -5.889 -4.496 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "29943c2f-d8d3-4d7c-8cfd-d9dde06687c2")
		)
		(pad "2" smd rect
			(at -5.889 -3.607 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "/网口/WL_BT_ANT")
			(pinfunction "WL_BT_ANT")
			(pintype "unspecified")
			(uuid "c4e46712-d58b-4cae-a7c5-895ced1a133f")
		)
		(pad "3" smd rect
			(at -5.889 -2.692 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "c0eacafd-64ea-4d14-810c-351952154da7")
		)
		(pad "4" smd rect
			(at -5.889 -1.803 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "unconnected-(U7-FM_RX-Pad4)")
			(pinfunction "FM_RX")
			(pintype "unspecified+no_connect")
			(uuid "af492871-54c2-4062-af66-dea7fe937355")
		)
		(pad "5" smd rect
			(at -5.889 -0.889 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "unconnected-(U7-NC-Pad5)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
			(uuid "05829a9d-9214-4a8e-b469-047855e83b89")
		)
		(pad "6" smd rect
			(at -5.889 0 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "Net-(U7-BT_WAKE)")
			(pinfunction "BT_WAKE")
			(pintype "unspecified")
			(uuid "b01ae4bb-18d3-42ef-996b-a239a4d07636")
		)
		(pad "7" smd rect
			(at -5.889 0.889 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(U7-BT_HOST_WAKE)")
			(pinfunction "BT_HOST_WAKE")
			(pintype "unspecified")
			(uuid "e5a80ea7-d5cb-4d9f-914a-e99cfc5d03b5")
		)
		(pad "8" smd rect
			(at -5.889 1.803 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "unconnected-(U7-CLK_REQ-Pad8)")
			(pinfunction "CLK_REQ")
			(pintype "unspecified+no_connect")
			(uuid "c68b3f74-956f-432d-8d96-f10ef6fb7aad")
		)
		(pad "9" smd rect
			(at -5.889 2.692 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "BT_3V3")
			(pinfunction "VBAT")
			(pintype "unspecified")
			(uuid "f839d017-8423-4054-b81c-0fcb8440a0f5")
		)
		(pad "10" smd rect
			(at -5.889 3.607 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/网口/XTAL_IN")
			(pinfunction "XTAL_IN")
			(pintype "unspecified")
			(uuid "bb59b9df-ed15-49b9-bf20-89b661edfe01")
		)
		(pad "11" smd rect
			(at -5.889 4.496 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "/网口/XTAL_OUT")
			(pinfunction "XTAL_OUT")
			(pintype "unspecified")
			(uuid "f66883f4-f21a-4afb-ac78-ff15778ccc75")
		)
		(pad "12" smd rect
			(at -4.496 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "/网口/WL_REG_ON")
			(pinfunction "WL_REG_ON")
			(pintype "unspecified")
			(uuid "ceab8076-2bf6-4a54-a12c-273802fec8a7")
		)
		(pad "13" smd rect
			(at -3.607 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "/网口/WL_HOST_WAKE")
			(pinfunction "WL_HOST_WAKE")
			(pintype "unspecified")
			(uuid "bc03d343-0518-4b56-95fb-3c13231ee62e")
		)
		(pad "14" smd rect
			(at -2.692 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "PG4{slash}SDC1_D2{slash}PG_EINT4")
			(pinfunction "SDIO_DATA_2")
			(pintype "unspecified")
			(uuid "3f5e5e41-708d-45bb-a9e2-c2af00f8e8a9")
		)
		(pad "15" smd rect
			(at -1.803 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "PG5{slash}SDC1_D3{slash}PG_EINT5")
			(pinfunction "SDIO_DATA_3")
			(pintype "unspecified")
			(uuid "03999597-7fc9-4b49-be47-59bb4c597c4d")
		)
		(pad "16" smd rect
			(at -0.889 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "PG1{slash}SDC1_CMD{slash}PG_EINT1")
			(pinfunction "SDIO_DATA_CMD")
			(pintype "unspecified")
			(uuid "783d5386-72c2-430f-88e2-d99f66e7e40e")
		)
		(pad "17" smd rect
			(at 0 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "PG0{slash}SDC1_CLK{slash}PG_EINT0")
			(pinfunction "SDIO_DATA_CLK")
			(pintype "unspecified")
			(uuid "a851f578-15b7-4e09-a39a-15780f6eca4c")
		)
		(pad "18" smd rect
			(at 0.889 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "PG2{slash}SDC1_D0{slash}PG_EINT2")
			(pinfunction "SDIO_DATA_0")
			(pintype "unspecified")
			(uuid "7eeb67d8-b248-4f35-abfc-36df561c7476")
		)
		(pad "19" smd rect
			(at 1.803 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "PG3{slash}SDC1_D1{slash}PG_EINT3")
			(pinfunction "SDIO_DATA_1")
			(pintype "unspecified")
			(uuid "540379c0-5205-4f53-9e92-c9213ba54804")
		)
		(pad "20" smd rect
			(at 2.692 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "08cbf975-249c-47a8-bc89-cf4ad083a483")
		)
		(pad "21" smd rect
			(at 3.607 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/网口/VIN_LDO_OUT")
			(pinfunction "VIN_LDO_OUT")
			(pintype "unspecified")
			(uuid "018cefd1-7c85-47b0-bc71-3f5b0f9da80a")
		)
		(pad "22" smd rect
			(at 4.496 5.889 180)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/网口/VDDIO")
			(pinfunction "VDDIO")
			(pintype "unspecified")
			(uuid "7ac00f8f-59b7-4da5-8167-160285bce27e")
		)
		(pad "23" smd rect
			(at 5.889 4.496 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "BT_3V3")
			(pinfunction "VIN_LDO")
			(pintype "unspecified")
			(uuid "ab35ccbf-6c4b-4279-8e85-5941d32bb2da")
		)
		(pad "24" smd rect
			(at 5.889 3.607 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "LPO")
			(pintype "unspecified")
			(uuid "f1584732-97c8-41ca-b9b0-64bfac7aed7c")
		)
		(pad "25" smd rect
			(at 5.889 2.692 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(U7-PCM_OUT-Pad25)")
			(pinfunction "PCM_OUT")
			(pintype "unspecified+no_connect")
			(uuid "5515d531-d995-4a17-8081-9621777a81cc")
		)
		(pad "26" smd rect
			(at 5.889 1.803 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "unconnected-(U7-PCM_CLK-Pad26)")
			(pinfunction "PCM_CLK")
			(pintype "unspecified+no_connect")
			(uuid "0f291606-2887-462f-8c11-e5acbeaa458c")
		)
		(pad "27" smd rect
			(at 5.889 0.889 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(U7-PCM_IN-Pad27)")
			(pinfunction "PCM_IN")
			(pintype "unspecified+no_connect")
			(uuid "3ac31745-837a-4356-8360-f1ba6983b7a3")
		)
		(pad "28" smd rect
			(at 5.889 0 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "unconnected-(U7-PCM_SYNC-Pad28)")
			(pinfunction "PCM_SYNC")
			(pintype "unspecified+no_connect")
			(uuid "ba4fde85-511c-4b91-bd21-9a3a650629d3")
		)
		(pad "29" smd rect
			(at 5.889 -0.889 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "unconnected-(U7-NC-Pad29)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
			(uuid "b575cd74-c64a-429c-8e2b-3b7d242ea0e8")
		)
		(pad "30" smd rect
			(at 5.889 -1.803 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(U7-NC-Pad30)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
			(uuid "5431505d-b25b-4935-bba5-8636b33167b0")
		)
		(pad "31" smd rect
			(at 5.889 -2.692 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "fbb4d606-64fb-4cdd-bb0c-6fc7ee370f72")
		)
		(pad "32" smd rect
			(at 5.889 -3.607 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "unconnected-(U7-NC-Pad32)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
			(uuid "6828656e-2036-416b-970a-2662d4082de0")
		)
		(pad "33" smd rect
			(at 5.889 -4.496 270)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "f92348ff-15b9-40c7-870b-f0c20f89f575")
		)
		(pad "34" smd rect
			(at 4.496 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "/网口/BT_RST_N")
			(pinfunction "BT_RST_N")
			(pintype "unspecified")
			(uuid "f533103a-c837-458b-bf7c-068338162b28")
		)
		(pad "35" smd rect
			(at 3.607 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(U7-NC-Pad35)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
			(uuid "218cf6ad-db33-4d55-bb5d-b800b5fe467e")
		)
		(pad "36" smd rect
			(at 2.692 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "6206ebc1-8681-482c-9cc3-c420d58ad266")
		)
		(pad "37" smd rect
			(at 1.803 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "unconnected-(U7-GPIO4-Pad37)")
			(pinfunction "GPIO4")
			(pintype "unspecified+no_connect")
			(uuid "2100f959-a352-4a7e-ab6b-4667fe20c49a")
		)
		(pad "38" smd rect
			(at 0.889 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(U7-GPIO3-Pad38)")
			(pinfunction "GPIO3")
			(pintype "unspecified+no_connect")
			(uuid "2df39bf4-2c17-4a11-96af-9732a31b42c7")
		)
		(pad "39" smd rect
			(at 0 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "unconnected-(U7-GPIO2-Pad39)")
			(pinfunction "GPIO2")
			(pintype "unspecified+no_connect")
			(uuid "939c60dc-e169-4851-b30f-409421e3b541")
		)
		(pad "40" smd rect
			(at -0.889 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(U7-GPIO1-Pad40)")
			(pinfunction "GPIO1")
			(pintype "unspecified+no_connect")
			(uuid "0377f544-eb8d-457b-895b-efa993c82719")
		)
		(pad "41" smd rect
			(at -1.803 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "/网口/UART_RTS_N")
			(pinfunction "UART_RTS_N")
			(pintype "unspecified")
			(uuid "ccf80876-5b55-4b95-b120-d0245f431c69")
		)
		(pad "42" smd rect
			(at -2.692 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "/网口/UART_TXD")
			(pinfunction "UART_TXD")
			(pintype "unspecified")
			(uuid "b7a7e5a1-a6b7-4cd6-a2c5-1f6d95d85fdd")
		)
		(pad "43" smd rect
			(at -3.607 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/网口/UART_RXD")
			(pinfunction "UART_RXD")
			(pintype "unspecified")
			(uuid "ce3cc914-0b0a-4f73-9782-927af0c39f3c")
		)
		(pad "44" smd rect
			(at -4.496 -5.889)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "/网口/UART_CTS_N")
			(pinfunction "UART_CTS_N")
			(pintype "unspecified")
			(uuid "af7da8bd-da46-4f80-b66a-f47366c561fd")
		)
		(pad "45" smd circle
			(at -2.7 -3.607 90)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "unconnected-(U7-TP1-Pad45)")
			(pinfunction "TP1")
			(pintype "unspecified+no_connect")
			(uuid "58c43126-8296-4640-ba12-7615c8685e97")
		)
		(pad "46" smd circle
			(at -0.9 -3.607 90)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "unconnected-(U7-TP2-Pad46)")
			(pinfunction "TP2")
			(pintype "unspecified+no_connect")
			(uuid "914b008f-31eb-49e6-a7ed-6721a3ad867d")
		)
		(pad "47" smd circle
			(at 0.9 -3.607 90)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(U7-TP3(NC)-Pad47)")
			(pinfunction "TP3(NC)")
			(pintype "unspecified+no_connect")
			(uuid "3d2171b8-259d-4c37-8cd3-896f9716cb57")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "3794a705-2ccd-4450-bb54-998ecd7ff678")
		(at 67.48 70.49)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "20f9f8bd-04b6-467b-a574-8b6baab9b936")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7d6ec92a-734c-467d-b4fc-e464ec7035ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d30a9f5-e680-4799-8233-682a2a407cf0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5cfdd553-1674-4b37-98c1-d0d096d39e66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/887c2232-6efc-45e5-9044-cf89573a8f87")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b0b9455-29a4-421e-a1f4-41cc8431f167")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28dca50b-2465-4cca-ba2c-5dff7ddfef88")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a4e3a92-b5c6-4da6-ae74-8f4f5deadd15")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3738daf-3926-4932-922c-4b080d632535")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1290350a-fdf0-4208-a213-df55b7e0025e")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aeef0860-28e0-4eb9-bb90-9f59255fadb3")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cf8f313-4a99-44f2-960b-0760155234aa")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8a3edcb-c857-49e2-9d52-2e6aef18f2e4")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "093694eb-f6a0-4a82-be13-b1d0f2a12921")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92c92b8c-8a69-41c6-b6b8-7c0c6864e914")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "210ea1d2-6e46-48b5-9e32-20bab2469fb9")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "6eee2e35-4cdd-43e8-8671-19d8c5121eb0")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "1ac06140-95ef-43bd-a4d5-edf39c4ac698")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "39066ae8-b0de-4503-af88-f30f60b57d31")
		(at 98.88 114.93)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "9a607bef-779f-4779-8cad-7a422ecaa729")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "642b3419-a632-4538-80b5-5936359a80a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8236a775-adb4-4d4f-8c6d-fb6be9dc70ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af605944-980d-461c-b3c9-c2c6ef2c28c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aaaf3f24-1f7c-48e4-abd7-3efcb84c2d78/c014be29-d27a-4124-9159-6b43934e5adb")
		(sheetname "/主控/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc825e26-41a9-4270-848b-e4597ec1a1a3")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f8c99dc-9b67-4251-85e6-9f9074f99064")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1af9346c-8e78-4bcd-b825-9ef9302dc8e1")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18a35a23-5668-446a-998e-4470a70efde2")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe542140-7f7f-4d6c-b7e3-d4f6c1c2a34b")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "588b3594-a77c-4f57-9668-f442e1df3e54")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "371ffb42-aea6-4866-9fd7-c0b98ebc31d9")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89682f0d-36da-4f7e-8e56-731276498594")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b7c78a2-e31a-464d-ae67-8610fb6f3a04")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4b621fe-90be-4091-a6d5-fbb19318635d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "66b036e6-c495-4e3a-aac7-ab5de3ff529d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "53178109-9234-431c-9c5a-4038eb5fbf78")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "PB7{slash}TWI0_SDA{slash}PB_EINT7")
			(pintype "passive")
			(uuid "c85f78ce-ed35-462a-a2bb-fa09bcb09399")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "3b0a4335-9cbe-4d78-9695-af74a7047498")
		(at 83.52 57.94)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2bf64035-6b78-43ce-8bed-f35e4b8f0b88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "99d2f51d-f9cf-4437-a215-eb30c1d0aeec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "17d90391-c527-4248-a790-c87dbcd40c58")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c547f67-8ecd-494a-8f25-4f09e0a2aa8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/fe88ca9f-c801-40a7-afc5-eded23858911")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e559aea-4f84-47df-8550-bbd6f5cd34b1")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbe303dc-0a81-4045-8759-37e8a17907bc")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "84cca4fc-4e20-4644-bd4f-be941a78b966")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a92d0649-facc-415e-a79a-3190ec1ad7d2")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fc8f9b2-ab58-4c23-9119-3455b43ab621")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45e02723-305e-43d0-bb46-6a1d734ce26f")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcb4f36e-238e-4ab2-b456-2fa294d87424")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d032dcc5-f1a9-40f4-9e0b-9e08187cb5f1")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcbb756e-d8b9-4b26-98d0-0c12b2eba315")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbf369e3-27f9-46f7-ae4f-d1da3b0a257b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "776d1c04-71dc-439f-be79-5f2e26f9cb6c")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(D1-A)")
			(pintype "passive")
			(uuid "216ae9e1-8230-4fd4-a100-8130671fd30b")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Net-(R9-Pad2)")
			(pintype "passive")
			(uuid "64420c0b-2f68-4c42-80c4-29ca67e674f1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(uuid "3b6e70cf-008b-4604-8800-34d6b8a0f851")
		(at 78.135 100.685)
		(descr "Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal oscillator")
		(property "Reference" "Y1"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(uuid "a8c9fd1e-18c5-4b1b-91f2-c8a4c171b28f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "ASE-24MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
			(uuid "97b01dd5-c7f9-4c3d-8d53-5b0c6ce3c563")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.abracon.com/Oscillators/ASV.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e5b7e04-ec8c-43ac-acdb-d8af53397c87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "3.3V CMOS SMD Crystal Clock Oscillator, Abracon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f95a08b4-612b-437d-b5d0-bf37bc50d431")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Oscillator*SMD*Abracon*ASE*3.2x2.5mm*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3757e8f2-e1e1-40a5-a3d6-251ca23104a8")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.9 -1.575)
			(end -1.9 1.575)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6dc57b9e-0a9e-45ba-8b31-f0d5f98faf18")
		)
		(fp_line
			(start -1.9 1.575)
			(end 1.9 1.575)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "046fd7e5-a856-41d6-9a3c-02154e80fdb7")
		)
		(fp_circle
			(center 0 0)
			(end 0.058333 0)
			(stroke
				(width 0.116667)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "d008f0b4-8e8c-4bf2-958a-d0b1fd29d572")
		)
		(fp_circle
			(center 0 0)
			(end 0.133333 0)
			(stroke
				(width 0.083333)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "31ab8240-59da-4e1e-99c7-f699d68e9faa")
		)
		(fp_circle
			(center 0 0)
			(end 0.208333 0)
			(stroke
				(width 0.083333)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "937de318-aa4c-4956-aec6-62805c3596b8")
		)
		(fp_circle
			(center 0 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "fefca9b6-6f03-4a6d-84d4-a2fcaab07ada")
		)
		(fp_line
			(start -2 -1.7)
			(end -2 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9e3976c-9c1d-4044-a6d5-6570973226cf")
		)
		(fp_line
			(start -2 1.7)
			(end 2 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c17bb0c-48d3-4a3c-b819-f09ec04817bb")
		)
		(fp_line
			(start 2 -1.7)
			(end -2 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8dc820e-5064-4ed8-813a-feebbfd7e609")
		)
		(fp_line
			(start 2 1.7)
			(end 2 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c764c0dd-b76b-497a-9ff7-1495e2239cc7")
		)
		(fp_line
			(start -1.6 -1.15)
			(end -1.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b79f74c9-8c00-4a17-9303-6371df7dce81")
		)
		(fp_line
			(start -1.6 0.25)
			(end -0.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7228f4dd-9e6a-4f7a-a744-fa7f40b7e5c4")
		)
		(fp_line
			(start -1.6 1.15)
			(end -1.6 -1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae5462f0-016a-482f-9911-32d5fb03a9b3")
		)
		(fp_line
			(start -1.5 -1.25)
			(end 1.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51edbb70-1dee-4793-93b8-ef0bef78fd36")
		)
		(fp_line
			(start -1.5 1.25)
			(end -1.6 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96155333-3056-4d3f-a7dd-7ebe25b389d3")
		)
		(fp_line
			(start 1.5 -1.25)
			(end 1.6 -1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54f86941-3dca-4b3a-ba3a-a8679cbb47bc")
		)
		(fp_line
			(start 1.5 1.25)
			(end -1.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af774c18-a973-4fe7-a6e2-56d4702ffa8d")
		)
		(fp_line
			(start 1.6 -1.15)
			(end 1.6 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b521d1da-4ab9-4814-aa04-d7dcafd0333c")
		)
		(fp_line
			(start 1.6 1.15)
			(end 1.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0cb01ba-ef1a-4a1a-8d2c-3e01cce9eb59")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2edeaa4d-a053-4b04-8561-e3b233b3c044")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.105)
				)
			)
		)
		(pad "1" smd rect
			(at -1.05 0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/电源/X24MIN")
			(pinfunction "EN")
			(pintype "input")
			(uuid "54b44359-4fde-4c4a-88d7-f382f87e06da")
		)
		(pad "2" smd rect
			(at 1.05 0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c9f372dd-f70b-4154-8135-155897a65aab")
		)
		(pad "3" smd rect
			(at 1.05 -0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/电源/X24MOUT")
			(pinfunction "OUT")
			(pintype "output")
			(uuid "3be55c06-c4c1-4e8f-b479-1606f477b8d5")
		)
		(pad "4" smd rect
			(at -1.05 -0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Vdd")
			(pintype "power_in")
			(uuid "1419150d-5c0c-4d72-977f-9baa9e3aa87c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "3dda2b9d-4107-4cfc-b664-9b6d7dfca511")
		(at 87.75 56.4)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP1"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "911d0398-5242-4d4f-aeb8-d81429f8ad38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5V"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "d2d32024-a6c6-47e0-b0b4-1b0f85e52c42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de2ec95a-14ad-4da9-93cd-7f373b8a244c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "85c10b0d-088c-4528-93c0-8ccc4d825138")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/40631c01-cda8-4fc0-b076-7ce34bbff584")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "55df1d68-bfc8-4de9-91ab-5a3314cd46ca")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c6448c1f-ee45-4efe-96ee-7093ecbb7c1e")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7b3a90d1-d278-4968-aaeb-a55c077a32da")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5343c939-91b1-41cc-b05b-a81bc2136eea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "2b8fb9e4-0762-48ec-b3ee-30156350d843")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "1")
			(pintype "passive")
			(uuid "400d09c3-a70f-438b-961a-703aa3820bb3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "442fd3c1-cf49-49b4-9498-93ed15296d19")
		(at 98.88 117.44)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f30edc88-b739-4d3b-9dde-dbed421ea96a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3a07b246-0c32-43f5-a5f7-c163b2218088")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3562bc69-4d30-47ae-bbd2-ea50ab19b6f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7cf70b6e-10d6-46a2-9410-70aaa5eb4c77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aaaf3f24-1f7c-48e4-abd7-3efcb84c2d78/2f356166-282c-4272-ae3e-a3ee93561199")
		(sheetname "/主控/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4831c7f-bcff-439c-a0f8-bb7a383653dd")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0fef875e-55d1-454c-aa36-4937dd824c13")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "382a71d7-e197-4e3c-9c74-a40187d084fb")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cdbfc272-3e91-4e75-9da1-775437f31c70")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a2f263d-df60-4a9d-a315-f1d17b868263")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17b655d1-dc6a-43b0-8b5a-7ca288017b78")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3b9e0de-0036-46f1-9de3-b6dd411a50e8")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90bfcb18-8879-4e83-9a3e-76b3e0ff18ea")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa337071-e439-434b-9088-14ad1b45e7fa")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9403107a-e88d-4858-ad39-fccc7e0cb457")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "847c5663-0873-4cfa-aa6c-0644bc614e11")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "38594328-666a-45e1-bb75-94470eca0da2")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "PB6{slash}TWI0_SCK{slash}PB_EINT6")
			(pintype "passive")
			(uuid "b605f907-d92e-4910-bfd5-4791ba26b9a6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4454bba6-cf99-4129-b09b-3b6f1901d19b")
		(at 67.48 75.51)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "be5e711b-ffa9-4765-8505-81176cce938a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "a490831a-6cdd-405e-8145-64d53be6e819")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac4f4523-9784-4e76-81a9-ba6b30a24fca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5abe414-41db-43f8-8ab1-e52e05905e90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/cc777156-21db-4080-8c64-77d698303048")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf17c85c-986a-42a1-85c2-f3a261c1a2d4")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aae038a4-b718-4482-9410-450e54b907d8")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b8aa0a8-5476-4e68-a64c-2b28fb459d06")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3a9668f-b499-4d19-978b-7dcd938c0c75")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bfca06e-d299-4a35-9214-d7edd2f42e11")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3652d0d6-9b6e-4c0a-b0fd-66bfc1b020b4")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06f0365c-dfe5-46e1-927a-624ef6ef81b6")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d0a267c-cd5c-40e6-89e2-7ebfe27ef64c")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f71cd36d-a797-4f53-bf8b-b0a895de9e1c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "053f6f4b-c17c-46e5-8de3-d5e36de79e38")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b488a691-d71f-4c2f-a0cf-b0fb0986f3c7")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "029c1946-a3f9-4971-a0e5-4f41b0efbed1")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "19ea2435-87f1-4641-97ad-b71062a6b46a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "45158d04-ab90-4ae7-ac4a-3f2c0ea89283")
		(at 83.52 80.53)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "d1e180bc-3dde-493b-8dd6-8bf1d3dde863")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "240"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b1a4ffaf-a2ad-4f00-ab01-2883e5e4996c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f1ff7bd3-4041-47cd-a6a4-17aa13c55986")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f6b1d36a-e6f8-429c-bef8-1ab88de52fc1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/4017d3b2-79d6-4f01-b4aa-b13e81dafdd5")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f182853a-27d2-4ef6-ad2f-c3ba875d691c")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7400ca1f-6cdc-4cde-a425-cfee0f93889f")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da9b921b-8def-4ed7-b2b9-e63e04deba6c")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86311beb-05ce-499a-9d65-8165fb1e7f7a")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf73ae3e-43f7-49c8-b73d-9ec879656643")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "891871f4-ee03-43ea-8a10-d951e48e1651")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f13f402-6daa-470a-9339-2cf81f5126aa")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f70480f-dbbe-4c6d-8db4-8d49718bce32")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb641270-2ea6-4140-a8b6-238d6a5bcba7")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aea768db-925c-4c22-9a35-32512205b8c0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "508992b1-afb6-4656-86a3-05398144d716")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(U1B-SZQ)")
			(pintype "passive")
			(uuid "4c411e52-0f89-446f-82c1-0838d38f3b8e")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "290a44f3-e4c4-489d-9669-ca023cdb6e71")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "456e9274-14fd-4bd8-8829-7166feb83d57")
		(at 83.52 78.02)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "d5540cc8-36ad-47b1-a1b4-51937d9e969c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10M"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "70a3cb01-46aa-450f-9869-73fa35b4cb42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5e1c057-7383-40b0-805c-5aa4410329bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1eb22cef-688c-476e-8ecd-0da477dff638")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/2ad65da6-289a-456c-bc8e-6f55c37a7b28")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6375d6a6-a9b9-4caf-a4cc-b18ae8aa24c4")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d862d75b-926a-47cb-8cbf-fb38e44d85f1")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7c619a6-c1c9-40c3-a12d-2416b7e7bba5")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c256c401-7c63-48e1-a274-bc21c5561159")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a45ba79-4673-4243-ab7c-3c080b1f1685")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45b76a03-97cb-46bb-b0f9-671285343e5b")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08792948-e7eb-4f39-96bd-850254e1e10d")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ae209cd-19ec-46a5-9804-c274308354d7")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d13b0f76-29c6-4a9e-8813-ea3a58731a70")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "156f89c4-a839-4c2d-9d5f-7a1d00870e05")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0843d525-5a7d-46f3-bf60-7ca5fdd1cef3")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/电源/X32KIN")
			(pintype "passive")
			(uuid "7d88351d-648c-4a49-bc0d-8520fa531c0d")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/电源/X32KOUT")
			(pintype "passive")
			(uuid "a9e2da0c-63b6-409c-98ac-75b577d5a6be")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "45c1886e-6e3d-4fc8-ba4b-b7f33ed7a884")
		(at 87.68 95.36)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "19ec681a-7038-4113-a007-e63f743d9324")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9653afd6-472e-4244-a566-14e2880757f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "731fc77b-018a-4789-8092-1deffba17ae9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "df7bbe5d-5ba2-4d14-b4d4-9bec14f50dac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/e295260b-9fdd-4d68-8b44-c25971cd15f1")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f9ede20-290f-4082-b4fa-2d2572eb2197")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad94e38d-2fa6-48bd-a080-cc2cf9acb00e")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29b65317-04f5-4bc5-ace0-2dcd0a4fe5f7")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf542c89-e8c8-432f-ab0a-a44d4eb7efb7")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24a864df-0811-4678-8704-fde04f52a849")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e8cd79b-5eae-4cbd-ba26-6407b19152c8")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80a20e23-2af5-47f4-bdd9-9e7bcae70aa5")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26dfbb57-6704-420d-bdd9-66e1c6ea0428")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "93eb6eaa-8d76-4f12-88a7-d6d4703b36c5")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6e4da67-c380-473f-a54e-f01fa7ded3e6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "706ea1ae-f111-41f5-bae0-5943862f4566")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "784e6c7b-0e15-4c30-9642-ea6d80d66ceb")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e76aa517-62e0-44fc-9b11-e86026a78f4d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4b6239c9-5558-469e-9fec-ece91bd2ee04")
		(at 68.76 122.18)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "6298b96d-47a0-4679-89fd-bc6c84632f90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c8cf3d0b-160c-45ce-8879-a6a912aa24f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43dcb29e-3fc5-4ea7-a19e-8dc64b4737c4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf20c1b2-3a7b-4c81-af9c-c5c7fccce1b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/79e3ebe6-5eff-4af7-97cc-b8aba81359a4")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d71d6838-8526-4491-aea2-43c4c910bf4b")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "913e79cd-ee42-418f-aaad-ba5eb848bfc9")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f77b02c3-4242-4161-bdec-472e0c867673")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12bfb1a2-56b3-4678-9732-cc11885203a0")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b60a4bf-cc0e-4fe0-aea4-f4e5d9c9b5a7")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "127beffb-d5f1-4402-b8b2-cbed1def361d")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eea17bc7-8035-4c8f-b330-9778f4dae75d")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3149cb6f-bcf4-4e01-bbfc-a37f5c1ef261")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83118dbd-1bb4-4d03-b0d5-353cd21469c0")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "074650f4-7093-4f3a-a7fa-2462310e98db")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "88a925fa-62aa-4c0b-80d3-b985e965b59c")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "11dba6ef-17b4-4bbf-b7a8-253c787b22cf")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U7-BT_WAKE)")
			(pintype "passive")
			(uuid "e844f603-24e6-4dd5-904e-5b8956be164b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4bbdf4a3-5fa6-4844-851b-fbb8f0e5d1d8")
		(at 87.57 84.3)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "1780d90a-0352-4d20-a004-f5b974fc4f0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "64b38b40-1b18-4460-965d-ca256f7cbdf9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b252bcca-a2b9-4bbf-9fe8-4d9b2766ed7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "81578d8b-5a92-4602-94f6-177c9f9eda39")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f4097d9-e1f2-4fd1-9ef2-768232369f60")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/31af7ee9-3bf2-4fe9-8699-5f88488a0663")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.485 -0.735)
			(end -1.485 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79e5f317-be9d-4305-9e21-338794ce9cc4")
		)
		(fp_line
			(start -1.485 0.735)
			(end 0.8 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eee0138e-590d-419c-9089-b88f8bf56991")
		)
		(fp_line
			(start 0.8 -0.735)
			(end -1.485 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0abf19d-71a0-4400-a55b-61d73a8c4dcc")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9deb8ec6-3dcd-48a3-8a6b-e7831df2637f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5257d9b-472a-4e93-97ba-0277851c3c1e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7dbd127-ef72-4cf8-a071-6aa7033b6367")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d00b5c0b-eb25-458e-b0b4-dbe765d57bf6")
		)
		(fp_line
			(start -0.8 -0.1)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cface34c-3b12-4af8-9d3f-7dcf88c1af3a")
		)
		(fp_line
			(start -0.8 0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77055f1e-246e-4351-8640-5fdd27a0bb31")
		)
		(fp_line
			(start -0.5 -0.4)
			(end -0.8 -0.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8234654-19b6-4edb-9cea-43a02b4fad6e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end -0.5 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94706126-a4ce-453e-a66d-8fc5476cd448")
		)
		(fp_line
			(start 0.8 0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d4bdb07-6ba6-4b51-b6e9-0317ecf27e52")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "45e2df0f-7c3c-49f1-a059-60a668ebe51e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "57ab02d7-9172-48fa-8d55-4e489886fcb9")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "81b875f8-a893-4900-b315-1c5e88fb0ee8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4c28f8e3-53aa-4eff-bb3e-8d4acf3ee33f")
		(at 63.47 62.96)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "00feb81b-90bd-4a0c-bf48-90b8d669f6da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "309a4315-3d99-46a3-bc33-2f987bc884e5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ffb41fd-8659-44d3-83cd-5f608209780e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "908cef68-be04-4f37-b0ff-08b07bc3ee6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f928013f-3e4e-4b27-974e-b9ae8b1835fc")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6084fa2-872c-4e09-a7fa-3ec38ab96425")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c0d2c14-1cb3-4cb4-84b1-eae5a0687a05")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f67311ea-681a-412a-89cc-420fafb0a135")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87ef6ce8-2104-4f46-9c68-3d1aedb5323e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0c2e687-d599-47af-945b-cec3d1d53a1a")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6338d0ac-2412-4f72-a0ae-56d228fe5e82")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f52ef6a-090e-4d92-999e-4c18d1f4ae0e")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86010c8c-e244-4dda-902f-68eaf07cfdeb")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56cc0867-d33c-4fbe-b4d0-b89e6f068bdb")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d594f5a-6d31-4fda-90b3-cf0c6d924940")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "44fc40a2-223a-4287-912f-ed9284910d3e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "1dec2f0e-3f86-414f-ab51-0e8906f7900b")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "50a5ec50-3ed0-4720-b76c-47da0a3cb229")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4fed9218-16a1-4eee-9c2d-93cb49004f0e")
		(at 75.5 80.53)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a8bed67f-5d10-498b-89cd-1783f55768e5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "45b16aae-2942-419f-89fd-51b4f5238e2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c071993-c54d-4998-8a10-ad3cb236ab15")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f4bb204-5891-4fe3-bbfd-51bb1ca94e3b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/9e8e8c5b-7256-4f57-9e52-b690073fdd44")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2559cf82-0fda-4eca-b41b-f02a96c19a93")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e05e10f8-1574-4f28-a089-89a0ce94ebaa")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "243823f5-7a52-41a3-9cec-b0f083aa491c")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a31d5a60-5f78-44da-959c-fad5aa0862f5")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d859dd2-197d-4b5e-9e98-18a8aa2cfdce")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13f2cbdd-8b06-42ce-a377-66e4df002562")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3be559e1-1a6b-4549-a470-3ac6ce004d5a")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1824ac87-c171-425f-a28c-961abd268277")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23b4d46c-5a01-47b8-93a4-bb911bc5f723")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15451d5b-9ba2-4eb3-b39a-534e2e3606a0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "890f6142-89a9-422c-93b9-7f6cf4a95dcc")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/电源/VRA2")
			(pintype "passive")
			(uuid "ccb746d5-3939-4c5e-82e8-0995c9077a53")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "90f9b46b-a3ef-4c9f-b6cc-98276a64e25f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "530f58be-8add-4b14-96b3-6ab0e2f0dbb6")
		(at 87.68 105.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "893a76aa-2761-4f6c-a571-5cbb36c3b343")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "40cfa907-21b9-4a7c-a44a-75d549d342af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "95638b21-010d-434f-8f8e-587fa43e5e86")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "393a9a8b-cc1f-47bc-87b9-55418153f8a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/143804dc-6950-42ee-9fe9-63cb067206ec")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "077fcf95-4bb4-4904-bcdf-542f675999e8")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8efabba6-307a-4006-916e-4be389fa708f")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a16e109f-514a-4a5a-8190-96a98216ca06")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a27db154-fb0e-4c03-ae6c-5e429918cbd6")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5670b91a-d53f-4893-a853-49f449825947")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d63e225-7d5b-4ef1-9e08-3a4307881c73")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de6f7124-51a5-4161-a1aa-01f3e1124e0a")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84ec7232-656d-4021-a335-e22b02eb2dcc")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5d0455b-502b-4b63-95cd-8b89b33ecd05")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64593c2f-a852-49bf-9853-526db37e81e8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "908296de-0e05-4b48-b955-be8f32b5becf")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "b1e003a4-6850-478f-a923-e5a971cdf70e")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "PF3{slash}SDC0_CMD{slash}JTAG_DO")
			(pintype "passive")
			(uuid "24b97583-ed01-4a90-93af-8f913de6479d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "54e378b8-aed3-4ffa-87f2-d68bb253bcb5")
		(at 83.52 83.04)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e2d41418-29db-4ecd-b0dd-fd8c1125bb7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3491e879-192e-4bb6-b249-242624f70c12")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db85aab1-3068-4c8a-97c2-0b53aec28606")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0713baf7-fabb-42b8-8b5a-1ec414451225")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/0fd1ef5d-9e94-4c18-a14d-df965fea58cf")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39c8996b-9b8e-46f0-9504-cdbc51ce220a")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb6b6dbd-dfce-4c5a-8057-71ca8818dc20")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "faf28f9a-83c4-48d9-a19a-d6f5726b04c7")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6dc21f1-c48d-4fab-b768-ff4915054bce")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de6df5f7-d107-4afc-a8b8-dd2cb9e2fa41")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99ba7463-5790-482b-b300-3884afd45f9d")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c135fb7-86df-414b-be13-e76e10230dde")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29033e15-d301-42d0-a461-b8b6e9618615")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec6be3a6-f1fc-4ca0-93da-5737eac77155")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ae91ce6-a894-4b14-9f84-1e84d9f3e679")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "04b26883-cb03-48a3-accc-e159d918d064")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "584460d6-5527-4518-b624-f95e4f2cc786")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/电源/RESET")
			(pintype "passive")
			(uuid "10fdbd98-d7b0-4339-966e-ac1e46cfb2de")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "57f47989-f5a3-4f6a-8c94-e486f2b78c70")
		(at 63.47 70.49)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2047547c-ddb0-4a5a-a13e-efb239d6de99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7c75d53b-1b89-4971-bde0-6f62409bfc45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56636d86-6d6c-425b-94e0-5b0e21692a2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff3b96bd-26b0-4ede-9140-48821fb3d347")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/ef1148a0-11bd-4e2c-a731-9c818b7c8a8e")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d5f3a48-c870-4215-953a-7fcd556da818")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d973db5c-27c3-4e86-87e4-59b940fc09ee")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cee6a0e0-bfd0-4f56-8c01-f1ce33c42379")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b57a4a49-7a5e-4f0f-aafa-158a9b6713a9")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d69336c-f41f-4a25-99e1-4edfeea18a77")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03d3a55b-d491-4908-b852-6b133a07099e")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4e30e4e-d5ea-4738-9237-02c8a6a59a62")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15daf2d6-fb9d-4ef0-9485-6bfd78b90535")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82dc6a99-e40a-4620-a0dd-366ffb01501d")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9c7596c-41a2-4fd7-b1bd-8bb47e1fb2ad")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b476b2b3-23f2-463d-90b4-98e80867b1b1")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "05d0207a-13e8-49ab-bb6f-0d46f0a232d2")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "50caa8c3-ab38-4a40-be67-91919bca909b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "5864b576-09a4-4a2d-99b8-a3a794271bac")
		(at 79.51 60.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "c11f555a-e86b-4383-9de1-f0e5bdb0f195")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "6pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7a21bce5-ca14-455f-bcfd-e50537bca18b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f043044-01ce-4967-bb63-560383d52e87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "36bacd01-66b5-4860-9c57-3b1131c086a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/36cd3a3e-279a-4c8a-9e63-828507dab707")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f164f77-a013-4870-ad86-5c343d5a440e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b8fb600-6ae2-4149-9cc1-4ef800cd6fcb")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4830d51d-8a4b-4785-a859-ff6503b1fd45")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e1605fd-4cb1-45f1-a517-2b621da8232d")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "abcee4f0-2011-4d98-98df-cbf30fa3190a")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d46aeb34-05e0-4456-a6e9-5435f9cc8af1")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4191fe1-744c-4e0b-b7b7-9c777172887f")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0b7b57d-85b7-4b45-92ba-5446176cb04f")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fb56722-70f0-4aca-ad0f-d03021e3eddb")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "615eb73a-5721-488d-bfff-b2420d7a5358")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f929f43f-9d43-48a6-adfe-065d5ec1a5d8")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "64a4042f-d217-47cb-8e8a-9be12179e52d")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/电源/X32KOUT")
			(pintype "passive")
			(uuid "681e6741-e8ef-4c59-8291-b4284e9b7f25")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "59b08ca2-b1f5-455f-b1c9-1645aacd137b")
		(at 87.68 102.89)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "33ba856f-89a8-4faf-adba-c252e5fe2d0b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c23773e0-1e08-453b-80ea-d7423c3c2b63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a265a5c3-0077-4f19-8cca-6fd2f6e1525c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1080039c-3060-4e74-99ff-90daaca770a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/a8847df2-a51a-4802-9aff-8713655a357a")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eec275d0-fcdc-4470-95dc-5c876efcda84")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b3120ce-ef1d-4095-b44b-08242359dcb5")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "84b8691c-1d6c-4cda-9de2-065105d33407")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "086c3e62-0299-42a4-b8f2-1784acb45b46")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aae54246-7bf5-48ba-9a32-db2dbb60b078")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58bcc11b-89dc-4216-bc25-8f86947733bc")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71f01023-3df2-4913-b73a-6e4076d585ea")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00a27a21-7a2b-41c9-87b2-d34a598cda2e")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c724fff4-c782-42bd-b8cf-29dc4844e431")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "389343d0-b28d-4b28-a76c-1ba906145cc0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2c316342-788e-416a-8185-a3324c1acec0")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "ee67dff1-0b81-466c-8f7c-738238e63db5")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "PF4{slash}SDC0_D3{slash}UART0_RX")
			(pintype "passive")
			(uuid "eb2eb2fc-6b57-44c8-9ed4-c78a23aea6bc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(layer "F.Cu")
		(uuid "5b0f4573-c911-47f6-b425-91938def71a0")
		(at 91.395 86.68)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "D4"
			(at 0 -1.3 0)
			(layer "F.SilkS")
			(uuid "84c526fc-7128-4e37-b17d-a90dadc77633")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1N4148WT"
			(at 0 1.4 0)
			(layer "F.Fab")
			(uuid "afccd6e6-f6d1-483a-8380-a9ed07130f0d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "621a1f00-6e90-4029-9dc2-bea061a7ca09")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f85233c1-6fac-4b7a-b688-13547cf4f18b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e81e12e7-cfbb-479d-a432-85ec15db600b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f2fae80-4bdf-4fc6-b654-ca360f07e1f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "D*SOD?523*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/5da9d235-79aa-4422-b61f-ba212eef3da6")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.26 -0.6)
			(end -1.26 0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22d4ed82-6b08-403b-840d-2dca5679e4b0")
		)
		(fp_line
			(start 0.7 -0.6)
			(end -1.26 -0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2260e27c-5561-4224-963e-8cbe4b0a83b0")
		)
		(fp_line
			(start 0.7 0.6)
			(end -1.26 0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "194324a8-365e-49b8-83e6-0f179458af39")
		)
		(fp_line
			(start -1.25 -0.7)
			(end 1.25 -0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b805caf5-000e-411d-b535-216e8ed7ffbb")
		)
		(fp_line
			(start -1.25 0.7)
			(end -1.25 -0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4c1c448-15a5-4e85-8d4b-a79e5bb677d3")
		)
		(fp_line
			(start 1.25 -0.7)
			(end 1.25 0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c30dcfb-a176-47d1-a15f-d3a5770d6231")
		)
		(fp_line
			(start 1.25 0.7)
			(end -1.25 0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2145e058-d41c-40a1-beb9-e8e9ef428674")
		)
		(fp_line
			(start -0.65 -0.45)
			(end 0.65 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b46ab66-a720-45f4-b6b9-9fc82e782ae9")
		)
		(fp_line
			(start -0.65 0.45)
			(end -0.65 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "792e2a3b-1034-4f04-a399-2c7e7f673c54")
		)
		(fp_line
			(start -0.2 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1374116-c7ad-43c7-8508-287ee6dc4682")
		)
		(fp_line
			(start -0.2 0)
			(end 0.1 0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c39ba03b-b87d-4892-b6db-ed237f68f7ae")
		)
		(fp_line
			(start -0.2 0.2)
			(end -0.2 -0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0651152-f054-45f6-9924-11cdb6b35877")
		)
		(fp_line
			(start 0.1 -0.2)
			(end -0.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cdcfb34-bb4a-48c9-8b21-8e7dae8edf20")
		)
		(fp_line
			(start 0.1 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dda68994-150b-4a6e-9985-36047f8bca8f")
		)
		(fp_line
			(start 0.1 0.2)
			(end 0.1 -0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a998be87-0a54-4ec9-b83f-349cc909f5d1")
		)
		(fp_line
			(start 0.65 -0.45)
			(end 0.65 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8a6b4e7-271b-49c6-b239-67ca6ef76777")
		)
		(fp_line
			(start 0.65 0.45)
			(end -0.65 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d17a4dd4-0273-4b0f-b1e0-943a458b71b8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 0)
			(layer "F.Fab")
			(uuid "dc6eb5e4-96ec-4b39-8a87-29e356c6b1c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "VCC_RTC")
			(pinfunction "K")
			(pintype "passive")
			(uuid "3a8a0f7d-4060-4dc4-9d7b-ac2fc5cafff4")
		)
		(pad "2" smd roundrect
			(at 0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "VBAT")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8505c135-c3c9-4809-bca3-d061ef23cd31")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "5eeb8e75-c804-4570-a312-6ea6cca66c55")
		(at 87.68 107.91)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "8eae3ed5-5eb0-44d1-a43c-b5c355bef5cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "073a71c6-685b-4341-bc4a-bde5938a79f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9420669b-1eda-43cb-a239-30ef4f490797")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d551386-35a5-46a0-bfd3-a25f170d1217")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/65f53e2b-983e-4b76-a710-2b01ec802bfe")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f7d4f71-f2b7-4775-ab3f-9c2eeef3f12f")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4e1391c-c0f2-430f-b38d-bea7470454ee")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90886811-a071-42a7-add1-93ef295e2869")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70013670-5c6d-4709-bebc-4b170b0be6d9")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e63ba70-a453-4705-bb27-187ec6af8dc4")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fe2a2b4-87ea-4057-a55e-962e2790f0a9")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcdab2c8-aa6c-4401-830e-14de320ecde4")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8153ed8f-3e18-43ac-8c80-d98071bce3b7")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d23c18f-021d-48c2-ade7-a9431c017d96")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2798b67c-535d-451f-9433-1639422da4a4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e8662991-61a0-45a4-83bf-75583435e6da")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "a22addf4-3428-49c1-918c-58cbab114346")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "PF1{slash}SDC0_D0{slash}JTAG_DI")
			(pintype "passive")
			(uuid "c2d01ff5-aac3-4d03-b90d-5954112a433e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "5fceb14a-43ee-44df-a81e-0af7d9836a73")
		(at 71.49 75.51)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e0876fd2-4060-406d-bad4-10bb8cb9ffbc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "2c201822-9a5a-4e2f-a635-2488d2ba2f3d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5bcd3dc4-5f72-4a5e-b452-87215fbfdba9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3bdb731-86d1-4d09-8ae7-b55072030b1a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/12c37996-ceec-4b4a-9391-7643b10c7d4d")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a1ea733-6426-4940-b54d-8bffd59eaff6")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cbdfee9-a83d-49eb-91ab-381164a5eddc")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b367fe2-906e-4aff-be66-6f6854846ced")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b3f5ac1-495b-48cd-84c9-c914b24adc67")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7266a932-e59b-4799-89b5-adbd9e4cdeae")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e9c2fec-2fac-4206-8bd4-4d023114952b")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f120be55-f8a5-4b7a-9bbf-1a4a7634bf6c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "415e99a4-156e-4fb0-9c47-23a277c010e2")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99edf155-57eb-4336-b0da-54c7f5501f18")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1985afe-8a28-4dc1-bab6-a1dd07951623")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c1de1544-01fe-4462-a4b4-c47f35426d20")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "48891566-e20e-45b8-b441-d41fba9b264d")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "87a283cd-55a6-4460-ab1c-377bb85496e3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-523"
		(layer "F.Cu")
		(uuid "5fdf8d89-37cf-42bf-a19c-c905affb9bee")
		(at 91.395 84.23)
		(descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
		(tags "Diode SOD523")
		(property "Reference" "D3"
			(at 0 -1.3 0)
			(layer "F.SilkS")
			(uuid "4c56e450-4be8-4277-8161-33c831931151")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1N4148WT"
			(at 0 1.4 0)
			(layer "F.Fab")
			(uuid "157867a9-5093-41ef-8beb-86bbd348107a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9892adb-7bcd-40bc-ab50-9dfc8fcab733")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ceb725e1-8ed3-4005-9462-15e8453fbe6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "46b2deb8-d54c-457d-b980-23d240cdcc18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8e70627-b80b-4434-8356-a269a1e0e579")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "D*SOD?523*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/ddf96e4d-9bcb-4b0a-b5e3-76b8902d5acf")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.26 -0.6)
			(end -1.26 0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb5b37f5-44e1-45ab-8bc7-51f0cc122b39")
		)
		(fp_line
			(start 0.7 -0.6)
			(end -1.26 -0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e659aae9-6662-498c-bb47-4119b1d65998")
		)
		(fp_line
			(start 0.7 0.6)
			(end -1.26 0.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe55ca56-bed3-465a-963c-b4b274895c20")
		)
		(fp_line
			(start -1.25 -0.7)
			(end 1.25 -0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbb3557a-a969-4d33-8d00-334c091f506e")
		)
		(fp_line
			(start -1.25 0.7)
			(end -1.25 -0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06d59534-c0b8-4926-aca4-cb042d199ee8")
		)
		(fp_line
			(start 1.25 -0.7)
			(end 1.25 0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c448506e-3936-4d0e-8fc6-5add563ed135")
		)
		(fp_line
			(start 1.25 0.7)
			(end -1.25 0.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "31d5f502-8b98-4dc2-b1c7-9a31c8599da3")
		)
		(fp_line
			(start -0.65 -0.45)
			(end 0.65 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2756a6a5-01cf-42a7-ac96-02f0c99b9f5e")
		)
		(fp_line
			(start -0.65 0.45)
			(end -0.65 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bec5223d-7279-438d-9035-b9d319e8ed91")
		)
		(fp_line
			(start -0.2 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cdb00ce-7f69-4732-8e87-fa335558a6a7")
		)
		(fp_line
			(start -0.2 0)
			(end 0.1 0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55363171-72ef-4bcc-b840-8f4735e3b761")
		)
		(fp_line
			(start -0.2 0.2)
			(end -0.2 -0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd84994a-327a-4f35-b431-e9108f78fd88")
		)
		(fp_line
			(start 0.1 -0.2)
			(end -0.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae724c09-1d8c-4a13-8a44-424419c7ce20")
		)
		(fp_line
			(start 0.1 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b02b5b9-35d1-4a5b-9eac-834ad34788fa")
		)
		(fp_line
			(start 0.1 0.2)
			(end 0.1 -0.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57240d34-3e18-4e71-a73a-6ca84a8e1a0b")
		)
		(fp_line
			(start 0.65 -0.45)
			(end 0.65 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79c32140-688b-40e9-ac61-4af07a784908")
		)
		(fp_line
			(start 0.65 0.45)
			(end -0.65 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad2ce857-bbba-4ba2-8470-4149eeb0367f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 0)
			(layer "F.Fab")
			(uuid "cecb3fac-3ddf-4da0-b4d1-ef8184348d87")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "VCC_RTC")
			(pinfunction "K")
			(pintype "passive")
			(uuid "c7622246-5f6f-4589-a14b-f69c04a68bde")
		)
		(pad "2" smd roundrect
			(at 0.7 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "A")
			(pintype "passive")
			(uuid "31ecbca3-a9f1-482c-beae-2ed352bc6fd3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "60fc3de8-c8c7-43e7-b915-8aa0603b5089")
		(at 178 112.475 -90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 -3.4 90)
			(layer "F.SilkS")
			(uuid "23369269-85e6-4120-a5b1-21165a38cfbb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LM393"
			(at 0 3.4 90)
			(layer "F.Fab")
			(uuid "31b8136e-6b1d-4466-a32e-4819c8596af2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm393.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea66c7d8-2b46-4f85-a3a8-a97385bfed29")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Low-Power, Low-Offset Voltage, Dual Comparators, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "746be5da-450e-4059-89cf-7fd1c4eb1076")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* SOP*5.28x5.23mm*P1.27mm* VSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/63931c4a-8231-419a-8663-5ea1d92ee592")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c21ee082-3eaa-4413-adf8-8015ec7e2846")
		)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5fb0713-cb94-4392-a6c8-94b037812c8f")
		)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5443e5a7-9b81-4ef4-9c7d-07aa2f3817d7")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99806403-48ca-4847-be82-a579c187ac50")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "1182114e-e664-462d-b653-46ee6a381521")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30021742-f110-401f-bb1b-949156e89d0d")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85736bef-74e1-449d-a98d-e6a72b723670")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12f91fcc-a8d5-480f-9ec1-eb2c913b446e")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80c420af-c010-4413-9ce1-f4bcbbd2156a")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b958367-7560-4a89-8e72-a63332f0d73f")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8f821e6-92c6-4064-aa26-e8caef789824")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d944e29-f8ed-4c4e-b634-bbf94194f74a")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "531527a7-b169-43e7-a67c-bd1dc9d22bed")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36a386d6-c4f8-4dbd-9f8a-3af2ebbb8323")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "19e2bbd7-e3bd-4e7f-bb2c-4c1fed375728")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "Net-(R10-Pad2)")
			(pintype "open_collector")
			(uuid "81d63a8b-f7e2-47f1-88fd-adaaf7f4a5a4")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "input")
			(uuid "1fd3ad1a-fcc9-4e34-b659-55f8d33e3c12")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/电源/CC1")
			(pinfunction "+")
			(pintype "input")
			(uuid "b32b1b99-7e5a-41da-a940-10fbe9e0d6b0")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
			(uuid "29b68857-9fd4-4251-8324-6863bda52ecb")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/电源/CC2")
			(pinfunction "+")
			(pintype "input")
			(uuid "859cbd85-b40e-49f8-8c93-1a63a96f2b8a")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "input")
			(uuid "5e9885cf-a7d2-4a2b-b4e8-4cc24082a7d2")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Net-(R9-Pad2)")
			(pintype "open_collector")
			(uuid "ef637977-8701-443a-9359-58d7c6f845bf")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "V+")
			(pintype "power_in")
			(uuid "2aa3db08-abf5-4295-bb7e-4d294a4739e8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
		(layer "F.Cu")
		(uuid "61395588-530b-4940-af70-3daf0ca2e572")
		(at 173 124.5 -90)
		(descr "SOIC, 8 Pin (JEITA/EIAJ 08-001-BBA and Atmel/Microchip, 208 mils width, https://www.jeita.or.jp/japanese/standard/book/ED-7311-19/#target/page_no=21, https://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23, https://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=162), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO P-SOP SOP SOP-8 SO SO-8 8S2 S2AE/F K04-056 CASE-751BE SO8W 8-Pin-SOIC PSA W8-2 W8-4 W8MS-1")
		(property "Reference" "U6"
			(at 0 -3.6 90)
			(layer "F.SilkS")
			(uuid "e86ddfb9-74c0-405d-b828-abeeaf0a1563")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "W25Q128JVS"
			(at 0 3.6 90)
			(layer "F.Fab")
			(uuid "01d8b73d-2d30-4484-99ad-6d6d8ad5b4e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "71c98c20-89b7-42c7-b161-0812a89130de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "128Mbit / 16MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3de46f3-fda8-4376-9782-bf517dd0a5d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*SOIC*5.3x5.3mm*P1.27mm*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/417d2395-e60b-4902-aa82-c4bd968db076")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -2.76 2.76)
			(end -2.76 2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9cad4c02-e247-461d-a5e6-9a4004eac0a6")
		)
		(fp_line
			(start 0 2.76)
			(end -2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ed5b513-1f95-4caa-ba6f-a7a380dad3ee")
		)
		(fp_line
			(start 0 2.76)
			(end 2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63de8669-3f40-4ea2-96fd-f627fe7da30e")
		)
		(fp_line
			(start 2.76 2.76)
			(end 2.76 2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3adb037c-c7ea-4c8d-8ec6-f6ae26adfd5e")
		)
		(fp_line
			(start -2.76 -2.76)
			(end -2.76 -2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a70371a9-65b4-4c1c-a721-926078d56d1b")
		)
		(fp_line
			(start 0 -2.76)
			(end -2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30ceeaf8-3264-4922-aa8c-6fe2d6ac0265")
		)
		(fp_line
			(start 0 -2.76)
			(end 2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e80e6052-b275-42c7-9cb4-89c9398edc4e")
		)
		(fp_line
			(start 2.76 -2.76)
			(end 2.76 -2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc0c24ae-f709-42f6-be9f-df7c2fc45334")
		)
		(fp_poly
			(pts
				(xy -3.525 -2.49) (xy -3.765 -2.82) (xy -3.285 -2.82) (xy -3.525 -2.49)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "75260fed-0f32-4577-a31a-b4f2093d8b57")
		)
		(fp_line
			(start -4.65 2.9)
			(end 4.65 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f7482f8-8cff-4ca1-8c0f-90f84c23a1e2")
		)
		(fp_line
			(start 4.65 2.9)
			(end 4.65 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc3babfa-c890-41c8-9a8b-f48976eb7873")
		)
		(fp_line
			(start -4.65 -2.9)
			(end -4.65 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53bcbe03-d11c-49e8-a39b-06b25d874e8a")
		)
		(fp_line
			(start 4.65 -2.9)
			(end -4.65 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7a97a93-9402-48c1-8795-c984669a530c")
		)
		(fp_line
			(start -2.65 2.65)
			(end -2.65 -1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "775c5e9a-14ed-4316-894b-a74e7891dec0")
		)
		(fp_line
			(start 2.65 2.65)
			(end -2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6730f246-50ef-4b59-a4fe-8e4b95bd6b46")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -1.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49ca2309-6712-42c9-84e0-87cb1db8796b")
		)
		(fp_line
			(start -1.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a93e0670-2483-4eb9-a8d5-cee472fd4211")
		)
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b083d50c-a120-47ca-94bf-395c8b479d5d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "99dc6c0f-e26d-4dcb-ba5d-600905bf33b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.5875 -1.905 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "PC2{slash}SDC2_RST{slash}SPI0_CS")
			(pinfunction "~{CS}")
			(pintype "input")
			(uuid "b63cda82-97a3-4157-a77d-882498a45079")
		)
		(pad "2" smd roundrect
			(at -3.5875 -0.635 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "PC0{slash}SDC2_CLK{slash}SPI0_MISO")
			(pinfunction "DO/IO_{1}")
			(pintype "bidirectional")
			(uuid "a70f4f90-2f54-406b-b6ce-43b320d3a4e9")
		)
		(pad "3" smd roundrect
			(at -3.5875 0.635 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "~{WP}/IO_{2}")
			(pintype "bidirectional")
			(uuid "fc757859-f0ed-4624-8961-8ee230b50e8f")
		)
		(pad "4" smd roundrect
			(at -3.5875 1.905 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "unconnected-(U6-GND-Pad4)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ccce4f58-bcf8-45a8-9a00-bf03d02ee6e5")
		)
		(pad "5" smd roundrect
			(at 3.5875 1.905 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "PC3{slash}SDC2_D0{slash}SPI0_MOSI")
			(pinfunction "DI/IO_{0}")
			(pintype "bidirectional")
			(uuid "7e62f82f-a842-4a04-a142-f61a93ec09ff")
		)
		(pad "6" smd roundrect
			(at 3.5875 0.635 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "PC1{slash}SDC2_CMD{slash}SPI0_CLK")
			(pinfunction "CLK")
			(pintype "input")
			(uuid "6e19b391-8930-4874-84dc-462ac9147be3")
		)
		(pad "7" smd roundrect
			(at 3.5875 -0.635 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "~{HOLD}/~{RESET}/IO_{3}")
			(pintype "bidirectional")
			(uuid "e2380a42-3453-4e83-9177-67d448ddfa98")
		)
		(pad "8" smd roundrect
			(at 3.5875 -1.905 270)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "076f5710-1e47-4c30-b5e5-03267e2114fa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.3x5.3mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(uuid "615843a1-f070-4b29-968a-8a0d53b9bc82")
		(at 92.85 70)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 0 -1.9 0)
			(layer "F.SilkS")
			(uuid "bc668979-0019-4148-b0e2-d506bcd1c506")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2uH"
			(at 0 1.9 0)
			(layer "F.Fab")
			(uuid "d8c17cf0-b6fe-4dde-81d5-f92cd8a4f039")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5fa2e89a-1499-43ac-b8a2-766a091ff4bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "518f379d-5edd-4d2f-9a8a-00359087d6b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/0f7c5b13-c56b-43ae-953d-9d74cb8736a1")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.835242 -0.91)
			(end 0.835242 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d1c4b1f-afa5-47c6-b05f-4b109263fe44")
		)
		(fp_line
			(start -0.835242 0.91)
			(end 0.835242 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "053e1230-8ff1-4bfd-9cdd-0a0382039e89")
		)
		(fp_line
			(start -2.35 -1.2)
			(end 2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f7a4cc6-1040-4cde-b1ba-5e7af081a1c1")
		)
		(fp_line
			(start -2.35 1.2)
			(end -2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6533178f-a985-4339-9797-3ae8cc520a78")
		)
		(fp_line
			(start 2.35 -1.2)
			(end 2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b56b8e3-0c83-4f9d-9adf-dbb93201025f")
		)
		(fp_line
			(start 2.35 1.2)
			(end -2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ad3efbb3-1584-4ccc-8e9a-b4403a42a916")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33936e5c-d43c-405a-baec-6e041999af00")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da7230a4-7b1f-46a7-bb55-b2f8151973d1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "458d922e-c360-44eb-a738-e1fc3738080c")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d888a27-50d3-4201-8c3e-d9ec34b23662")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "28996376-afc6-4d7f-97a7-51d17b6e2e88")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 7 "+1V8")
			(pinfunction "1")
			(pintype "passive")
			(uuid "fae48634-84ce-411d-9f57-9d42f8745a84")
		)
		(pad "2" smd roundrect
			(at 1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 79 "SW2")
			(pinfunction "2")
			(pintype "passive")
			(uuid "6c8bbec5-45c8-4b45-aa72-090ec24cd602")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6260ae5f-2d47-4556-b126-2374f9525e7e")
		(at 79.51 78.02)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "ab81101b-49c9-44de-acc0-0103a2eda15e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "80e2e656-21f9-4a6e-a527-13aeddeef044")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ae1e440-d763-4641-aa43-4cb59ceabb7b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c6e4759-17e7-4d82-87c6-5c864d431288")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/e8eddc46-fb33-4ca7-bc43-7d5aa6f4f7d8")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3aab49b8-efab-49f7-aaf4-81c49a2bf7fa")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f368fa9d-2b6e-4981-af18-0a0640abe075")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7278c13c-b52e-46c4-8804-b89760b70ccc")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc22df62-2d47-461b-a1d4-8da1653e5743")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4678d14-6eb2-48ab-9101-2fedf02d1b1c")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb230f5b-008a-4b78-9c24-625800e56a1f")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1cc609c-ce42-4bc7-badd-4e81a64b15b7")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57f76f5d-da20-4daa-ae4d-46cf63344f2d")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49685511-9782-4f5e-aba5-f0eb21ec195d")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b6b666c-85fd-413b-aa52-d775d70f0e4d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f231d8e3-8c0e-4a76-830c-a3f533efd8ad")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b30df941-d254-4295-85c3-97d6a97fb2cf")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "FB1")
			(pintype "passive")
			(uuid "033d89e1-1629-4dca-b625-ed9082e9a9b1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6481272c-6a29-40a3-a289-153534ebb2c4")
		(at 83.52 73)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "1ad11f50-a680-4208-8b4b-585ebd9107d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "95071ffd-60ee-4f72-b398-73345aa29e50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f11ff90-c416-4258-99f2-10d14c88905c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1d3e3c9-bd6a-4e6d-a331-c1ea023d2235")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3347519f-ae4b-4a33-af1a-c24ac7daff76")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef998511-4b0a-4029-b79f-79882c4950bb")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fdeb64c2-6d6c-4b7c-bd46-eb67073a7050")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94d5e5c5-1186-4c57-bd3d-2198b4d97bf8")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f16fd3d-f888-428e-91af-e1df4c7d0e4c")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b37381b-1b42-484f-9094-0792f154a6ea")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6853fac-48f3-4f56-b137-9eb8f1c0c39f")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1bacba69-80d7-43ed-bf75-b66639db72fe")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "284d7905-3f21-4b39-ab3b-9358c766697f")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbe9b530-1cad-41dc-a58a-75ed32041d4a")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "623ff341-2151-48df-a6c5-8589bd3426c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fd612391-b05e-471d-aabc-f8bbe0b341fc")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "4ae17f39-1c70-4cc9-a85b-0e902b0cc78d")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "24b8f702-52f5-4a1e-98e6-5adc412ef991")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_SPST_NO_Alps_SKRK"
		(layer "F.Cu")
		(uuid "667d72e1-3ecb-4a47-9a11-b5f199747527")
		(at 101.52 59.074)
		(descr "http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKRK/SKRKAHE020.html")
		(tags "SMD SMT button")
		(property "Reference" "SW1"
			(at 0 -2.25 0)
			(layer "F.SilkS")
			(uuid "514f8bf2-2641-4bb0-bac0-c369e50af6ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2.5 0)
			(layer "F.Fab")
			(uuid "27bb535a-1ea4-43d8-8750-484f9c29b728")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd06eba3-0721-41eb-bfa9-d853bbc71c09")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "553eb767-ff23-433a-9b67-ced4bc5c66ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/1438734a-8b49-4271-9715-3246df660f68/4ecf51fe-6b5d-49c1-a0f2-dae5c2927475")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.07 -1.57)
			(end 2.07 -1.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f24f260-3548-406c-b07a-52e1c6465355")
		)
		(fp_line
			(start -2.07 -1.27)
			(end -2.07 -1.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e5a0577-85b9-442b-bc41-c63958fc9211")
		)
		(fp_line
			(start -2.07 1.57)
			(end -2.07 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2386b36a-bd28-4302-8d78-07b2479cdf21")
		)
		(fp_line
			(start 2.07 -1.57)
			(end 2.07 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a423d1b2-6303-4b43-9619-ef58d7ac636f")
		)
		(fp_line
			(start 2.07 1.27)
			(end 2.07 1.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7769d51c-fc98-452e-b2c9-c1bce9bf4e47")
		)
		(fp_line
			(start 2.07 1.57)
			(end -2.07 1.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47eecdc7-0679-45e1-be3e-e4d7a16c1dd8")
		)
		(fp_line
			(start -2.75 -1.7)
			(end 2.75 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a506875d-1d82-426e-b94d-fa416751065c")
		)
		(fp_line
			(start -2.75 1.7)
			(end -2.75 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0fed873-d4a1-4a50-a034-c95c44b3df6c")
		)
		(fp_line
			(start 2.75 -1.7)
			(end 2.75 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6574c300-c05d-4e01-a700-71f8a0fa3324")
		)
		(fp_line
			(start 2.75 1.7)
			(end -2.75 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4bb3719-129a-4d6f-8ce6-39bfc1c6dee7")
		)
		(fp_line
			(start -1.95 -1.45)
			(end 1.95 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf408e69-e35b-4382-a5e0-5255120c9bdd")
		)
		(fp_line
			(start -1.95 1.45)
			(end -1.95 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2ea05fe-5bb9-4423-a3b0-bfd808d54dd5")
		)
		(fp_line
			(start 1.95 -1.45)
			(end 1.95 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e39633d-86dd-443b-898c-c45ba745727a")
		)
		(fp_line
			(start 1.95 1.45)
			(end -1.95 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b6a02e0-7ee3-48be-911c-a5f1063849d4")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "39aa25ed-d950-47a2-80cf-f8ba45270815")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "75a18c69-2a52-4dae-9b2d-f77359312081")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.1 0)
			(size 0.8 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "c648ae31-5a04-408e-93fc-89efedd5a2d6")
		)
		(pad "2" smd roundrect
			(at 2.1 0)
			(size 0.8 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/电源/RESET")
			(pinfunction "2")
			(pintype "passive")
			(uuid "3ef73e8a-60ca-41d0-b052-f9e364f7adc9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_SPST_NO_Alps_SKRK.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "68943df2-fd59-41af-9c48-7762f7bbc55a")
		(at 75.5 67.98)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2e1fb6fe-db7d-4662-90ca-b0a69e3682f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "6bd0bf85-3ef4-4f27-964f-f69d3c2ab4a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bb41f4c-c59f-451d-bb03-8811d202654f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9dd39c9-52f9-41c0-ba07-f9059205f309")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/6e5e43a8-db4d-4915-bde5-6a94dfa09ca9")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48f73259-3688-4f36-b8cc-b8d9f6ae50fe")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c94b2604-c158-446b-acbe-50fd20af9c9d")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "31821fbd-395c-45a5-92a4-f0421fe008ac")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6eed353c-ed82-48d9-ad70-ff2b633608d3")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13d4bab7-aa17-4a34-aaaa-0bc5627b0ad9")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f844905d-2d28-4724-93c3-e26e703409ad")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb2bdf52-ca97-41ce-9935-a8c6effacffe")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e11d0bc-8ebc-45a6-a114-c922375a03b3")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d142569d-96ee-4f51-93cd-744184ab1e80")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb6b3142-e268-4680-a683-d688aee052bf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "16fdef34-6351-4b96-898d-0b894d6423cf")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fb22a7c2-f2df-44ac-bfd7-a4fc8b270268")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "VCC_RTC")
			(pintype "passive")
			(uuid "57b2fbea-c9af-4b7d-afda-750ed8563c7b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6c5bb00e-e1d5-4fdc-8c8d-b677efa9110d")
		(at 63.47 60.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "6bc2fc30-4f56-422a-85b8-fe8c9616cfe9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "ad1aa891-1960-4eb6-8a79-3b3a88994082")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ea6d906-8172-4d47-b1fa-90afd81d805b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "766ec905-a3ba-4754-af04-b39d510115b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/2a7a3e0c-97eb-459d-8ac1-76a340f1a91e")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2064be7c-6852-4014-a7c9-23d13a8f4ea1")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed7d6a4f-f717-4bb4-994e-0b86b5706982")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a3f73b4-dc34-4a30-8e88-83596277dc45")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44817df9-8a63-4261-b14a-ae76337be34e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c048f35-13b9-447e-a831-26fd6fd7635c")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50e550d6-0e82-4f57-ad75-d3a9e6e93de3")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "875e9ca7-bfc1-4c39-9cc0-a6cc0e11e7ac")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "747bccba-ff61-4289-a8ad-05f3d29f4677")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "500e17a2-50a3-444f-8425-6347bc5a4a46")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0400f9c4-9e98-4c2b-bd38-d4cae56c13c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0f4d77fe-0d36-4580-8663-b07168829f73")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "5e5abe7e-f948-4b93-b36a-7623ccc5dbe5")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7c4c8a1e-de79-4e15-b5a8-964c043a701b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6db6a116-c030-4e85-b6ea-4a8ee01673d4")
		(at 72.77 114.65)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2a3dcd74-181c-40c3-8bbc-9f233aa58545")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b628024e-4a72-43de-85c1-9e5bca188017")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e19c0437-5f44-4bba-9935-e49ab104b717")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf63b267-d88e-42c8-b309-f66c5f69bcc8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/d7e5919b-93cb-46b7-9488-a3ac48f8288a")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c54f30fa-f2e0-430d-9d51-4adf1b370133")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa34483d-fa20-4599-9f31-0926757eef54")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c26b29e2-1af6-4856-8610-96bb50891849")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "098ec295-45b3-4115-9ca1-308ef28de862")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bf777fc-3994-4bd4-9fd2-5785e87f155d")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52668809-19da-48f3-be61-4308e54defd5")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c53d9c1-9c2f-485c-9576-2a35d541c1bd")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "301324ed-4a19-42b9-b092-2672f2656594")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b946b386-85d9-40a5-a240-476702695d0a")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ebf9400-6aaa-4539-8a3b-eea05e09d031")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3e887f43-68f1-4619-8708-8bdd55f314c1")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "PG1{slash}SDC1_CMD{slash}PG_EINT1")
			(pintype "passive")
			(uuid "4da80fac-f0a7-46d6-a95e-b94f8fef8c51")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "198cc239-2196-4769-bfd7-a7ab9542eb43")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6e087a06-1131-4727-a6e2-e8a4e95ba813")
		(at 67.48 57.94)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e1f78d91-2bd8-4937-855c-febb20be9be2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "ac944ee6-09d9-4c49-bfb3-3574dd57d740")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e50b917-cb3f-4a4b-a74d-f487c3820a81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d4a19fc-254a-47b1-8309-9053cb1621e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3bf1c02f-4998-4d1b-b50e-fab06b71ad9a")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43f3030f-350d-45a8-ab98-6e0e90cb5fa7")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7bc73a0-b099-49a3-9ca1-63fed17fa060")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b50cca7-dee6-4cc5-bca9-9d0de25ae710")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04eb87b3-b2d9-4666-8e9b-3ccb219df634")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a730d7f-005f-4cbc-9d2f-172c0d7029c1")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "874854a3-161c-4e70-8e73-3e4b4ae2dd72")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba7d111f-ac54-4740-a00b-cfbceb348153")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3abe9c3-cf22-48a4-9057-e9d215f849ac")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4b250ed-0229-478a-b2e8-b307ab9c7eaa")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87253128-6305-49f2-b568-832861b1bad2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7f7601f7-8d7f-4ecd-9e3a-ae00b05b975c")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "6db45390-e7e2-4fbd-a825-798ec02c9099")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "4a09fd19-4b9c-4a2b-9a89-ac7d350f4481")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6e215435-674f-47d3-988c-24b499d12124")
		(at 87.68 110.42)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f9ef5176-3298-48d3-b313-b460c221a8d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7d0cf41c-7ee7-4f65-852f-fa26117bc545")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bda35312-5fb2-4a5d-9f63-a65a5e83a6c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3336537b-f926-4494-bdd5-329cf4186cac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/15d80d2f-5257-4f58-af9e-2a83b9392310")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d61a8c3-04f4-4ca5-b12f-da15962c10f8")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c961958-2f3e-43f0-8d0f-d77c1b8b8ac4")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d4a04fe-8b37-4630-a9bc-2fbe8ac5132f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc6dcde3-9523-4652-a5a4-8975bccbf211")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dba5c34a-afff-431a-9d8a-55a57ec78a3a")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "361bde92-f6c2-453f-8fcd-9e8915212e2b")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59df6901-862f-4061-93ea-19c65fe69091")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "402bb790-dac1-42f0-b283-d4b1779a285d")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "107a0b51-21c5-4db4-abe4-4c281e2309b0")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c31baf42-ef54-41e2-a324-c5f39ad4c1c7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "212656d1-e678-4b60-a884-cdfc38a9ed6f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "766f60a5-f00d-43f5-85ec-f324ef469ba7")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "PF0{slash}SDC0_D1{slash}JTAG_MS")
			(pintype "passive")
			(uuid "41f62b69-644d-4f8a-a119-37243f74989e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6f80cc06-3e91-485c-b443-31cd162cd3d1")
		(at 64.75 122.18)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e7bca948-b3e3-4cf7-9da8-93acce7a1f27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "56e0f7f6-d224-41b9-a952-654b8343c440")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "425b4fc3-c80b-4fa7-a235-0c80ef87b517")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e675bb7e-3987-492a-8605-67408c7fe4f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/74e21e40-8d06-46f5-862a-f5c1b8abb8c2")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a1f52ef-3969-49b6-ad86-4f4cbc83266b")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26ea4cd6-2c39-4d8b-8c21-37ad1c885291")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be41ab8e-7c3a-4f07-8663-d92aef08909f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03304bdb-cbf9-4e8f-8f04-c44e2a771be3")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8d7f596-0912-45ec-9b65-03e49e678ef8")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5670848-9a5d-4b3d-a597-52a426a1ae44")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c609b79-2860-498d-8733-4839de4286a4")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae43e6ae-c46b-4936-b3c9-e1a264a946f9")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82b51010-5586-4ce4-8256-c1b89ee4a2db")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b2abc17-e195-4a07-8e3e-3b7f5e50c7c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4a05fce2-3de5-44c7-8bc3-2fbdc5450ebc")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "78e3d6d4-a3d8-4733-8ce8-c8c7e5fee32c")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9aa5f4da-3401-4188-b0a8-870281e0265f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "7223a0c1-0a7a-4065-b60d-f181d7b315ea")
		(at 71.49 55.43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "7447bc27-30f8-410a-85e2-9e3fdb84da31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "ec61ad0d-8cf2-4486-aeb1-abebf0cbe9a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3eee56f-f3e7-4b85-8cfa-114c22588bd7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a5bdacd-98ec-46e8-8732-64d9f7495ae7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/114745ee-972d-465c-b92b-a75a2f95da88")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ed53799-23df-41b6-b0d8-111dfceb4a5b")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7576ac3-630f-4d85-9157-a41634cad0ea")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7caf0347-536f-41a0-a9d5-04c21c613512")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fc7d4a1-5afd-4fbe-8200-2b7290affa7b")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3780bd5-bffd-4931-8515-f4a578a660c0")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4e96e2f-9cb9-425b-8ac5-8e28396a43a4")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ee89263-4601-43f4-be33-88ed8cbe205c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1fca825-0abf-44db-b647-c3c3c50a8d57")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50d1532e-53c4-4e62-ab0f-639e91dd5fde")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9bafd49-5981-486f-a7b2-66835cdc6dbd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cb08727d-f26b-4727-a5db-7ed52cc64a3d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "b32d4e0a-0e63-4671-b033-62eb24c35ad8")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "111df63f-5a09-4904-be20-e63bf232969c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(uuid "75f4e224-39ba-4073-8977-49d7b9e5a97f")
		(at 92.85 73.45)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at 0 -1.9 0)
			(layer "F.SilkS")
			(uuid "5a70574d-0d6a-41c8-94f8-697dfad1e881")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2uH"
			(at 0 1.9 0)
			(layer "F.Fab")
			(uuid "88a8034a-e6c7-4d32-9376-41a13b96442b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfd95546-b6ce-4e99-8562-623d6c9d8852")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f8ce5ee-a118-47cb-abe2-6f8685613532")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/7b9002c8-7f63-475f-b485-36761096b962")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.835242 -0.91)
			(end 0.835242 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5f5f621-9ee3-4695-8126-f8ed21979262")
		)
		(fp_line
			(start -0.835242 0.91)
			(end 0.835242 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc16a25a-4896-4579-ba74-264d548317b6")
		)
		(fp_line
			(start -2.35 -1.2)
			(end 2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bcffd787-940b-40d0-a455-41a8c5deddd9")
		)
		(fp_line
			(start -2.35 1.2)
			(end -2.35 -1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47eb0081-c58b-4b32-8ca7-ebfac67573f0")
		)
		(fp_line
			(start 2.35 -1.2)
			(end 2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d822e956-c44c-423c-bac4-0205bb6b7627")
		)
		(fp_line
			(start 2.35 1.2)
			(end -2.35 1.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fde6ca7d-a4d4-4db4-8320-493ca89f0fc3")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cb59f69-2c57-4309-9346-5315bfb73b3b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "085787d4-8aec-43c0-8cba-8a2f73090bb9")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49c424f8-882f-459a-b051-aa9a95a8ddb8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d202d549-e05c-467f-af8d-5d6ed3c2ef9e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "df8d52f1-3e55-4ab4-b2b0-70fc4d78f1d2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 17 "+1V2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "a682da20-32b1-4f3a-b709-69ec9fdf1f7d")
		)
		(pad "2" smd roundrect
			(at 1.575 0)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 80 "SW1")
			(pinfunction "2")
			(pintype "passive")
			(uuid "16ae381a-e6a8-497a-a029-1466a423785a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "767d0b1e-20f9-4447-ac31-0a5ddef46a7b")
		(at 71.49 70.49)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "5e7a4996-9b90-4a4b-b28a-6c09dc31f397")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "47a49930-0583-4df2-b6b3-e193480aee70")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "77f6788b-6b58-401a-938d-f9adbfda7ad1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1fce9ebe-c21a-4846-87de-39ecd12b9514")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/4fb6e9d4-e961-4a94-9773-e1c4aaa9c96b")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04970478-7218-4b0a-ad1a-2886d891be2b")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "125b6bf7-64d1-4c2b-81ba-1951f371a9a6")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7158f498-9566-4a0f-96cd-54388b53f022")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b13c50d-d2d1-4967-a5b9-bb8a3e7d29ff")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41456d75-19a8-4323-8525-dca3a6ba4596")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b487b79c-2022-4401-82c2-4ebf0d13872a")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bf87c1a-14ca-4034-b658-543b34af2743")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46ec1963-a689-4587-b2af-4b3714d5513a")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28392937-1cb8-412f-8e4d-bf7056a28575")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00f5997b-0212-475c-adba-65686170fce6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d51ada69-73d7-4000-a2f8-a41b5532b8d6")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "0c3ad64e-d349-4a29-8fcf-388882980b36")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d8390030-1af7-4a43-8ead-a3fe7158e612")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "791195a5-4c66-4de3-98b3-d02a8c45cd04")
		(at 72.77 109.63)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "41ede3f0-7d44-4946-9d24-731a6adca938")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9288b17a-473e-4aa5-9c4e-95623b2c8e4a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "331cfd9f-8122-4899-921d-9be40548cb55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf6ab6c2-75f4-4ac5-bd3a-19104676d7d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/3830a484-6098-4c54-ad74-0d210a005479")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c944ae30-f59b-4126-b183-9d408e4ef058")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2205d658-c236-4930-b02a-acb93ce26e82")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "664a1809-f5cb-4d0d-88b2-050d1a1e3c95")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f22b9bfa-efc7-4a0a-92fd-a0be2ce169b7")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2db81eeb-c8b8-4770-aabf-ca3698f30df7")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c6d5c00-aabf-4ba0-bdb7-0c0c25324d75")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b988d853-1881-448a-9eeb-c647597b5eb8")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b14a78e-774f-4328-8f7d-763501c5d1fb")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5abd74bf-67e2-4f37-ac88-2cc07aca9f9f")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb99b2fa-d62c-4125-99fc-83eabf61baa7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "04110e3c-0373-4eb6-b50a-5db2b50cff5e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "PG4{slash}SDC1_D2{slash}PG_EINT4")
			(pintype "passive")
			(uuid "8d30a23e-1a21-47cb-8461-32bed5436faa")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "39db4094-40ea-422f-a659-1c0ef58e22e8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "7b91eedf-a080-4cc9-89b0-f59d89888c0e")
		(at 87.68 100.38)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "cb68491b-3254-48ca-96fc-a6f576842769")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "06d50d88-92ec-47c5-93b5-cde4183c570d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5472c6d-5216-4a59-9f99-9e70f5f129fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f83d794-6dfe-4aa9-b5b0-04704c951e31")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/f7ea2437-7e3f-448d-a570-938ba5075758")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f4cb280-c4bb-4409-85e1-6ea86f34b744")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a8e4173-191a-44fc-89df-407528aab4b9")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d82525ae-7cc5-4363-873a-4f38c28c3d26")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91c4918d-a0f9-4018-b7b5-c965bf168102")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ef2136c-a9d9-4d8d-b60c-371caa535d2f")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d84391c4-a712-454c-86f9-6c2cd3bc1943")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27969801-98d1-4fe1-a952-20424fd79903")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a51e6234-1ab5-4aba-bf20-0671276ed52f")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31d311e5-e9c4-469d-92c4-d06e0763a463")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8875c8a-6830-43db-9897-e369cd747fd2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eacce7d0-b64f-4081-b9a4-bc2391cb75b4")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "b40331a0-ba7a-4c12-b3fd-3002585e2604")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "PF5{slash}SDC0_D2{slash}JTAG_CK")
			(pintype "passive")
			(uuid "271a98ae-26f7-4f11-abca-8bd6a930e1d1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "7cbdb5f4-27c7-4079-95c7-a18b21ecd228")
		(at 87.75 60.85)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP2"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "2e709574-43ed-43f4-84fd-97530678dca8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1V2"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "a5b85fc6-e68f-4871-a50b-74c6f6b09c21")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf831f48-922b-4b38-81cf-74b06ef6927b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf7709dc-6d5c-4607-984b-75679542cb9d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/a2367509-3f78-4325-b8b6-8ea9ee7bd7a4")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "baf53209-e64e-484e-b8d8-c64f9b845b0a")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b19faf78-05de-42a6-9799-4b49798d6058")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6033401d-89af-4a5c-9476-2bed9405ef88")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "78e4d377-afcc-4565-a41a-2389c5ce4876")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "17811f76-ebda-4dfb-93a5-00e609e0705b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+1V2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "dc363fa0-36aa-4559-a426-f89d4124aa4c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "7fe31556-2589-42a1-b249-8b3acf319a2d")
		(at 81.45 119.5)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP12"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "28c80b18-4491-4e68-94a3-245391b511ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BT_UART_CTS_N"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "3b8fee72-89cf-40dd-8c92-057ce1d3d78d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88fd863c-5cf1-4ac1-a0f9-8aaaa2798f04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2436b88b-0fee-427e-ba73-c13e9d271db8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/a3b2b02f-0cc5-4a30-8678-039a43e51403")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "a69459be-65c8-4dca-9a31-3ba8794f1fd0")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b51c4b09-ff96-441a-a744-fc51de1ab53c")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8ea48d4f-9254-478f-a8ba-c63fdd8caae1")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8a90502d-5352-4216-a033-1ac23bb16f8b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "13040ce2-3c5e-4155-9c9b-3178aee42cf5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "/网口/UART_CTS_N")
			(pinfunction "1")
			(pintype "passive")
			(uuid "5d903def-0d25-4f0e-b50a-319ba3f1dd7b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "80337e1d-a21b-479c-8bd3-a565a79439d4")
		(at 63.47 67.98)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e4657247-e975-4b2a-9cdc-26769a991470")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "53814a5c-03de-40de-af8a-1ebdd25b3c5f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cdc0471c-91e9-446e-9f88-d509a6e09063")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2cbfe90-f80f-48a5-aecb-c033995c232a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/161da55d-5f38-4614-b0f8-741c340e3cf8")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "228ccf85-a5b0-4182-b1b7-30c93c824490")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28a09c86-8bfe-4fe2-91e7-07323233c6d1")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4210207-224e-4123-9708-4fdc8edfd8ec")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2207da02-ebea-426d-b2cb-a64858b72d96")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47d2203c-eff9-479e-acb2-bc108faf8084")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "076352b2-f7c4-4738-98c3-b1533d978944")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81d9d58e-4bbb-4f08-aa6e-507e31ee61aa")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4798fc8c-4db9-4261-b8c1-b1360146864d")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a54ca921-f92c-4e60-9eb5-89f09d1e3e85")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab2b02b8-64a6-4707-9518-dd5488d7fd3b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f0022db7-f2b9-43f7-9fa7-895c161293ae")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "037f99e4-1a8e-45c7-bc05-51065b70c1bf")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "883ed076-32af-4749-a405-fd475e7c9e89")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "80537634-2658-40bf-a640-fe89a2d72c0a")
		(at 68.76 124.69)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "d6bc65de-41d2-4edb-a314-467f85177403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "22195079-b304-43cd-8e53-b7273fdaf7b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de99f63e-e3b9-4163-b91c-b54812e965d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4671b385-8510-4626-a42b-dff134cb0072")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/8f3875c5-2fe6-46ad-9576-220d4042be14")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06874914-47d7-4037-ba90-c8e5b85bed9b")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a8413ba-160d-4de8-8f4d-6a33691c5d58")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "990668a2-03af-4fa9-9f5a-5753797a09d5")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f737cef0-fc44-4f39-b9d6-caddd181fde4")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4cda378-fd03-4af5-8fe1-a0619a6b4fd9")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0645063f-37fb-45f5-a518-5d0bf765e6e8")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7ae2a06-b279-4767-90ca-fdc8cd270a2d")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31c8a870-c94d-418a-ac96-f4d0833dbb5d")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f19ebf65-138a-4c60-bfcf-1ddca73ab733")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1aa416eb-8a84-4f84-8b23-66a131a86cc5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "374b7e8d-26d2-48ec-9771-0037de4af01d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "cf785875-de34-4d24-b961-21b5b4f4384f")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "Net-(U7-BT_HOST_WAKE)")
			(pintype "passive")
			(uuid "f3f3d93a-c969-486d-9a16-fe7e8ec759bc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(uuid "81473659-02ea-4cae-8383-25fa3e33d003")
		(at 69.135 99.86)
		(descr "Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal oscillator")
		(property "Reference" "Y3"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(uuid "05b65c37-f6a2-4636-bbe6-0df0e09fea31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "ASE-26MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
			(uuid "6ab02a89-c659-4bc7-aa7a-e55cf236cae8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.abracon.com/Oscillators/ASV.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1ea7191-463f-4b8f-ad44-3134fa4f33f1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "3.3V CMOS SMD Crystal Clock Oscillator, Abracon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dff86204-c86b-4dc7-90e6-31f98e8c52a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Oscillator*SMD*Abracon*ASE*3.2x2.5mm*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/15824582-87f7-4375-98a4-a29eb0b457d0")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.9 -1.575)
			(end -1.9 1.575)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bbccf41-628d-475f-a5a9-2ac185727329")
		)
		(fp_line
			(start -1.9 1.575)
			(end 1.9 1.575)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9d3795b-2306-4391-bb1a-dfb962301cea")
		)
		(fp_circle
			(center 0 0)
			(end 0.058333 0)
			(stroke
				(width 0.116667)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "cdd39bfb-4f58-4bdc-b2e7-1e5a1fa24da2")
		)
		(fp_circle
			(center 0 0)
			(end 0.133333 0)
			(stroke
				(width 0.083333)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "4bdd284f-732b-42d0-8041-027b2ef3be57")
		)
		(fp_circle
			(center 0 0)
			(end 0.208333 0)
			(stroke
				(width 0.083333)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "17e19b04-ceef-4bec-afc0-b8577b5c50ab")
		)
		(fp_circle
			(center 0 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Adhes")
			(uuid "fea064db-7db8-43ba-a851-0f6311f4e558")
		)
		(fp_line
			(start -2 -1.7)
			(end -2 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "547c6f33-e10f-41d2-a887-ee040c245855")
		)
		(fp_line
			(start -2 1.7)
			(end 2 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a016817a-2865-4f2f-9409-718a3b2fadb1")
		)
		(fp_line
			(start 2 -1.7)
			(end -2 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64793482-7a19-4f86-8857-4630a821c7c7")
		)
		(fp_line
			(start 2 1.7)
			(end 2 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19d0492e-c2fe-4939-9c89-c1e8a54e3912")
		)
		(fp_line
			(start -1.6 -1.15)
			(end -1.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "406bcf8a-0573-43f9-a888-acf99e31f584")
		)
		(fp_line
			(start -1.6 0.25)
			(end -0.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e313e3a-6b8d-4912-9c43-364b48c686a7")
		)
		(fp_line
			(start -1.6 1.15)
			(end -1.6 -1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e736a100-203a-4d84-aebf-de2136f1f5b6")
		)
		(fp_line
			(start -1.5 -1.25)
			(end 1.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1e2a568-4e22-4cba-8d7a-8de6b7514bab")
		)
		(fp_line
			(start -1.5 1.25)
			(end -1.6 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb5835af-54ed-496a-bea6-089bac7fe792")
		)
		(fp_line
			(start 1.5 -1.25)
			(end 1.6 -1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d7ef2ed-2f75-4c80-a707-f6dc23cd0779")
		)
		(fp_line
			(start 1.5 1.25)
			(end -1.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18489413-7e15-40c5-b8d7-913ab0813714")
		)
		(fp_line
			(start 1.6 -1.15)
			(end 1.6 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d264f1d-dcf6-4619-b720-2ab3d07a09ad")
		)
		(fp_line
			(start 1.6 1.15)
			(end 1.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06c7d77a-961e-4077-bd48-4b0441f19ccb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f7e5c82a-120c-41dc-a83b-a77f59dac6f7")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.105)
				)
			)
		)
		(pad "1" smd rect
			(at -1.05 0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/网口/XTAL_IN")
			(pinfunction "EN")
			(pintype "input")
			(uuid "6cae36d1-d084-43d8-89e7-72e54fdecd96")
		)
		(pad "2" smd rect
			(at 1.05 0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "56a4a41c-cdaf-40e0-9620-a205fd932a78")
		)
		(pad "3" smd rect
			(at 1.05 -0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "/网口/XTAL_OUT")
			(pinfunction "OUT")
			(pintype "output")
			(uuid "ef75578d-24da-4b4d-9f54-348852a656bd")
		)
		(pad "4" smd rect
			(at -1.05 -0.825)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Vdd")
			(pintype "power_in")
			(uuid "3f390f3f-82e3-4822-8607-b259f3b40179")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "8490bea7-3e6e-4dc9-af2f-acceabcd81e4")
		(at 79.51 75.51)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "96dd20f7-62d8-4db1-9e95-957ce5b6accc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "200K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "d7761447-04e0-4fa1-aaf5-733c6db1a11b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6a9926e-e152-47ef-97fa-84c957366967")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b223ba0-1f7e-44f1-8d59-6ac2a32fcccf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f075e83d-e531-458f-ad3f-e84847ca3cff")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bf3b01a-c21a-40be-b42e-2387f100bc1b")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9221c0ab-c2a9-41b5-956f-ac6bc59f4773")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe0329b4-458c-4da6-8533-54aea0d3a372")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af36fac6-c122-46e3-8bf0-25316e30c6bc")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3aa2aa8-ec44-44e8-a6f0-caf70cc0a1a7")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "784d77aa-ab2d-4969-a24a-08a22ec9ee32")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d0f30c2-fe15-4548-8298-be6dc0828d57")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6b36509-e251-4981-9238-fe1659ea1b54")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae98eb91-2d0f-4b8f-850d-7c426eba8e43")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06e42099-389b-481c-88b5-46cb275e0ff3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bbc13954-4409-47d9-9bcb-0a0c6d9869ec")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "fa17b415-9d4b-4822-ac55-940b188a4f9a")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "FB2")
			(pintype "passive")
			(uuid "3fee6510-398b-4e07-b9cd-7638ee110a7f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Allwinner_SiPs:eLQFP-128_14x14_Pitch0.4mm_EPAD_6.60mm"
		(layer "F.Cu")
		(uuid "856f43ef-a490-4019-a4a7-711f5b0580e2")
		(at 153.75 108)
		(property "Reference" "U1"
			(at 0 -9.25 0)
			(layer "F.SilkS")
			(uuid "443eebda-ead1-46f6-a1da-7e84d64ecbc4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Allwinner_V3s"
			(at 0 9.25 0)
			(layer "F.Fab")
			(uuid "7dae4d2f-0f3e-43cb-9d05-87aa5f06fbc8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://linux-sunxi.org/images/2/23/Allwinner_V3s_Datasheet_V1.0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "23468900-e479-4b65-b404-c0e5482559cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ARM Cortex-A7 CPU with 64 MB DDR2 RAM in a single package (SiP)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4ed06b0-5e84-4f17-ba55-75bc25d51b1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LQFP-128")
		(path "/aaaf3f24-1f7c-48e4-abd7-3efcb84c2d78/f03ba8cb-ee07-4cd3-8bb2-6af23df471e0")
		(sheetname "/主控/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_line
			(start -7.15 -7.15)
			(end -7.15 -6.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29a95a81-5552-4fb1-81a5-f129c904c2c2")
		)
		(fp_line
			(start -7.15 -6.6)
			(end -8.25 -6.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9a48845-b39c-4b55-b421-3bf89cecbda6")
		)
		(fp_line
			(start -7.15 7.15)
			(end -7.15 6.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "356dec7c-95ff-4a0e-9a3e-b8a984223903")
		)
		(fp_line
			(start -6.6 -7.15)
			(end -7.15 -7.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18d9fc51-49d9-4ffa-939b-f4de163ca7dd")
		)
		(fp_line
			(start -6.6 7.15)
			(end -7.15 7.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "527c9bed-2217-4230-ad97-82d761cc11e0")
		)
		(fp_line
			(start 6.6 -7.15)
			(end 7.15 -7.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cbd3690-c615-4491-b9d5-e48bb776ff2e")
		)
		(fp_line
			(start 6.6 7.15)
			(end 7.15 7.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82fc869e-e190-441c-97e6-6e02c2d45e5e")
		)
		(fp_line
			(start 7.15 -7.15)
			(end 7.15 -6.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d3f6299-95dc-41e3-a273-de6ad18c0f4f")
		)
		(fp_line
			(start 7.15 7.15)
			(end 7.15 6.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e4adb0a-e841-443d-ab8f-ff0d528341a8")
		)
		(fp_line
			(start -8.5 -8.5)
			(end 8.5 -8.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1501c178-6c19-43f4-b52e-2ef74541366f")
		)
		(fp_line
			(start -8.5 8.5)
			(end -8.5 -8.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf1ec903-fd31-4f66-9892-b5216d01b1ed")
		)
		(fp_line
			(start 8.5 -8.5)
			(end 8.5 8.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9faba70d-98eb-4bcb-963b-717fbc12f847")
		)
		(fp_line
			(start 8.5 8.5)
			(end -8.5 8.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a6e80d4-bded-444a-89d2-0d88c4bdd91a")
		)
		(fp_line
			(start -7 -6)
			(end -7 7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20af14f0-f0c9-462b-b330-f361dc5f0df1")
		)
		(fp_line
			(start -7 7)
			(end 7 7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "722a8ab9-9219-46d6-a2cf-848d27d42809")
		)
		(fp_line
			(start -6 -7)
			(end -7 -6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7197774f-e9c6-43e2-b6ac-124337cc34cb")
		)
		(fp_line
			(start 7 -7)
			(end -6 -7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84e3eb39-3de1-4b17-9dd2-9e7ecba317bc")
		)
		(fp_line
			(start 7 7)
			(end 7 -7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ae8a618-f51e-45e7-9252-659e47d9cdba")
		)
		(pad "1" smd rect
			(at -7.625 -6.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "PG4{slash}SDC1_D2{slash}PG_EINT4")
			(pinfunction "PG4/SDC1_D2/PG_EINT4")
			(pintype "bidirectional")
			(uuid "45d26521-0f9f-403d-b5b8-1a5a1a2a8ef6")
		)
		(pad "2" smd rect
			(at -7.625 -5.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "PG3{slash}SDC1_D1{slash}PG_EINT3")
			(pinfunction "PG3/SDC1_D1/PG_EINT3")
			(pintype "bidirectional")
			(uuid "b40dddfb-b11a-4914-85d1-b4e74fd9117b")
		)
		(pad "3" smd rect
			(at -7.625 -5.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "PG2{slash}SDC1_D0{slash}PG_EINT2")
			(pinfunction "PG2/SDC1_D0/PG_EINT2")
			(pintype "bidirectional")
			(uuid "cc5063db-6be7-4b41-bd83-65dedef88c60")
		)
		(pad "4" smd rect
			(at -7.625 -5 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "PG1{slash}SDC1_CMD{slash}PG_EINT1")
			(pinfunction "PG1/SDC1_CMD/PG_EINT1")
			(pintype "bidirectional")
			(uuid "dbc0766b-e2dc-439c-8557-d5ec0b9db4d4")
		)
		(pad "5" smd rect
			(at -7.625 -4.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "PG0{slash}SDC1_CLK{slash}PG_EINT0")
			(pinfunction "PG0/SDC1_CLK/PG_EINT0")
			(pintype "bidirectional")
			(uuid "f8692c7a-907c-434a-9bb8-92eb2f20b57e")
		)
		(pad "6" smd rect
			(at -7.625 -4.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "PE24{slash}LCD_D23{slash}UART1_CTS")
			(pinfunction "PE24/LCD_D23/UART1_CTS")
			(pintype "bidirectional")
			(uuid "f3366c1c-0960-4ef4-90d3-54181dea51a5")
		)
		(pad "7" smd rect
			(at -7.625 -3.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "PE23{slash}LCD_D22{slash}UART1_RTS")
			(pinfunction "PE23/LCD_D22/UART1_RTS")
			(pintype "bidirectional")
			(uuid "5f055d3d-0245-4081-90c4-e3ced7ef1b39")
		)
		(pad "8" smd rect
			(at -7.625 -3.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "PE22{slash}CSI_SDA{slash}TWI1_SDA{slash}UART1_RX")
			(pinfunction "PE22/CSI_SDA/TWI1_SDA/UART1_RX")
			(pintype "bidirectional")
			(uuid "e8814629-90b8-40e4-8da9-2cda51bb0dda")
		)
		(pad "9" smd rect
			(at -7.625 -3 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "PE21{slash}CSI_SCK{slash}TWI1_SCK{slash}UART1_TX")
			(pinfunction "PE21/CSI_SCK/TWI1_SCK/UART1_TX")
			(pintype "bidirectional")
			(uuid "855a36ec-ab5d-4ef2-b48c-22d06d4c004b")
		)
		(pad "10" smd rect
			(at -7.625 -2.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "PE20{slash}CSI_FIELD{slash}CSI_MIPI_MCLK")
			(pinfunction "PE20/CSI_FIELD/CSI_MIPI_MCLK")
			(pintype "bidirectional")
			(uuid "88e75d84-c802-42ad-94cf-f08110f06bc5")
		)
		(pad "11" smd rect
			(at -7.625 -2.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "PE19{slash}CSI_D15{slash}LCD_D21")
			(pinfunction "PE19/CSI_D15/LCD_D21")
			(pintype "bidirectional")
			(uuid "21f0f401-f0ce-4f07-b125-99e0230e5339")
		)
		(pad "12" smd rect
			(at -7.625 -1.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-PE0")
			(pintype "power_in")
			(uuid "bf2b7af1-f7c2-41a7-be3c-9a9f4d9a3d1f")
		)
		(pad "13" smd rect
			(at -7.625 -1.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "PE18{slash}CSI_D14{slash}LCD_D20")
			(pinfunction "PE18/CSI_D14/LCD_D20")
			(pintype "bidirectional")
			(uuid "613a5073-753d-4458-a43b-c6ea278f9339")
		)
		(pad "14" smd rect
			(at -7.625 -1 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "PE17{slash}CSI_D13{slash}LCD_D19")
			(pinfunction "PE17/CSI_D13/LCD_D19")
			(pintype "bidirectional")
			(uuid "6531c5b1-656a-4007-9650-59fcd640ce1b")
		)
		(pad "15" smd rect
			(at -7.625 -0.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "PE16{slash}CSI_D12{slash}LCD_D18")
			(pinfunction "PE16/CSI_D12/LCD_D18")
			(pintype "bidirectional")
			(uuid "9448da6d-8c1d-4ad4-ba81-f6eef678e7d7")
		)
		(pad "16" smd rect
			(at -7.625 -0.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "PE15{slash}CSI_D11{slash}LCD_D15")
			(pinfunction "PE15/CSI_D11/LCD_D15")
			(pintype "bidirectional")
			(uuid "e5760628-b1ba-4d11-9f59-00311fdb0486")
		)
		(pad "17" smd rect
			(at -7.625 0.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "PE14{slash}CSI_D10{slash}LCD_D14")
			(pinfunction "PE14/CSI_D10/LCD_D14")
			(pintype "bidirectional")
			(uuid "939cad2c-6cc4-476c-ae69-610de72dcf7f")
		)
		(pad "18" smd rect
			(at -7.625 0.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "PE13{slash}CSI_D9{slash}LCD_D13")
			(pinfunction "PE13/CSI_D9/LCD_D13")
			(pintype "bidirectional")
			(uuid "bd81d1a2-c41a-4e46-8aef-f6107e7e3493")
		)
		(pad "19" smd rect
			(at -7.625 1 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS3")
			(pintype "power_in")
			(uuid "941c133b-e5d3-40a7-82fc-81c807f49fcb")
		)
		(pad "20" smd rect
			(at -7.625 1.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU3")
			(pintype "power_in")
			(uuid "981b2a04-1812-469c-a4f3-888a41d427b5")
		)
		(pad "21" smd rect
			(at -7.625 1.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU2")
			(pintype "power_in")
			(uuid "ccc29519-7b33-46e5-a0a7-97631e5026de")
		)
		(pad "22" smd rect
			(at -7.625 2.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "PE12{slash}CSI_D8{slash}LCD_D12")
			(pinfunction "PE12/CSI_D8/LCD_D12")
			(pintype "bidirectional")
			(uuid "c6c71b29-595c-4ac6-88d6-f0d867594b14")
		)
		(pad "23" smd rect
			(at -7.625 2.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "PE11{slash}CSI_D7{slash}LCD_D11")
			(pinfunction "PE11/CSI_D7/LCD_D11")
			(pintype "bidirectional")
			(uuid "7931f098-cce2-4a0b-b188-15a74c96762c")
		)
		(pad "24" smd rect
			(at -7.625 3 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "PE10{slash}CSI_D6{slash}LCD_D10")
			(pinfunction "PE10/CSI_D6/LCD_D10")
			(pintype "bidirectional")
			(uuid "c8965294-6854-4538-b371-29a7a3ce0585")
		)
		(pad "25" smd rect
			(at -7.625 3.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU1")
			(pintype "power_in")
			(uuid "f1ed15bc-e3d1-474d-acd8-efcd8ff60223")
		)
		(pad "26" smd rect
			(at -7.625 3.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU0")
			(pintype "power_in")
			(uuid "50f6dc51-4ac1-42b7-9b80-6573fad211fc")
		)
		(pad "27" smd rect
			(at -7.625 4.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "PE9{slash}CSI_D5{slash}LCD_D7")
			(pinfunction "PE9/CSI_D5/LCD_D7")
			(pintype "bidirectional")
			(uuid "4c701306-7503-4830-808a-5b314b2e1276")
		)
		(pad "28" smd rect
			(at -7.625 4.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "PE8{slash}CSI_D4{slash}LCD_D6")
			(pinfunction "PE8/CSI_D4/LCD_D6")
			(pintype "bidirectional")
			(uuid "8d6bbb32-ecf1-4040-97a1-89fd2b06315e")
		)
		(pad "29" smd rect
			(at -7.625 5 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-PE1")
			(pintype "power_in")
			(uuid "19b64711-fc27-46ea-a567-07ce1e5cd2e1")
		)
		(pad "30" smd rect
			(at -7.625 5.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "PE7{slash}CSI_D3{slash}LCD_D5")
			(pinfunction "PE7/CSI_D3/LCD_D5")
			(pintype "bidirectional")
			(uuid "d27a5daf-5713-4f8e-b58f-fb53432076f6")
		)
		(pad "31" smd rect
			(at -7.625 5.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "PE6{slash}CSI_D2{slash}LCD_D4")
			(pinfunction "PE6/CSI_D2/LCD_D4")
			(pintype "bidirectional")
			(uuid "1c11a520-f56f-440f-8565-58a726790828")
		)
		(pad "32" smd rect
			(at -7.625 6.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "PE5{slash}CSI_D1{slash}LCD_D3")
			(pinfunction "PE5/CSI_D1/LCD_D3")
			(pintype "bidirectional")
			(uuid "8ff96a4a-3f9e-497f-b9d0-2a12aee21e75")
		)
		(pad "33" smd rect
			(at -6.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "PE4{slash}CSI_D0{slash}LCD_D2")
			(pinfunction "PE4/CSI_D0/LCD_D2")
			(pintype "bidirectional")
			(uuid "407a300b-de5b-4c83-8b62-f1bc8486651b")
		)
		(pad "34" smd rect
			(at -5.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "PE3{slash}CSI_VSYNC{slash}LCD_VSYNC")
			(pinfunction "PE3/CSI_VSYNC/LCD_VSYNC")
			(pintype "bidirectional")
			(uuid "cba34d6c-0add-42e0-bfc7-0dc4e2f3d5a6")
		)
		(pad "35" smd rect
			(at -5.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "PE2{slash}CSI_HSYNC{slash}LCD_HSYNC")
			(pinfunction "PE2/CSI_HSYNC/LCD_HSYNC")
			(pintype "bidirectional")
			(uuid "146f9f1f-56db-43a8-ad27-b712d9a9f879")
		)
		(pad "36" smd rect
			(at -5 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "PE1{slash}CSI_MCLK{slash}LCD_DE")
			(pinfunction "PE1/CSI_MCLK/LCD_DE")
			(pintype "bidirectional")
			(uuid "ed5078c1-fab9-4111-a638-d8272f70e8ff")
		)
		(pad "37" smd rect
			(at -4.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "PE0{slash}CSI_PCLK{slash}LCD_CLK")
			(pinfunction "PE0/CSI_PCLK/LCD_CLK")
			(pintype "bidirectional")
			(uuid "b6e44f77-ef79-40c5-b746-bc818a22ab76")
		)
		(pad "38" smd rect
			(at -4.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU4")
			(pintype "power_in")
			(uuid "f2eb891c-e418-428d-9af7-bd98634b494c")
		)
		(pad "39" smd rect
			(at -3.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "PB0{slash}UART2_TX{slash}PB_EINT0")
			(pinfunction "PB0/UART2_TX/PB_EINT0")
			(pintype "bidirectional")
			(uuid "160ffa76-9b92-4b7f-bf8f-6ca70b641459")
		)
		(pad "40" smd rect
			(at -3.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "PB1{slash}UART2_RX{slash}PB_EINT1")
			(pinfunction "PB1/UART2_RX/PB_EINT1")
			(pintype "bidirectional")
			(uuid "215f6591-0740-4513-9838-a7ff7ee3a472")
		)
		(pad "41" smd rect
			(at -3 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "PB2{slash}UART2_RTS{slash}PB_EINT2")
			(pinfunction "PB2/UART2_RTS/PB_EINT2")
			(pintype "bidirectional")
			(uuid "bbed55ed-5e87-4c8b-b637-023c88df1279")
		)
		(pad "42" smd rect
			(at -2.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "PB3{slash}UART2_CTS{slash}PB_EINT3")
			(pinfunction "PB3/UART2_CTS/PB_EINT3")
			(pintype "bidirectional")
			(uuid "6e5ad035-38f5-4759-849d-d3b9be60991d")
		)
		(pad "43" smd rect
			(at -2.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "PB4{slash}PWM0{slash}PB_EINT4")
			(pinfunction "PB4/PWM0/PB_EINT4")
			(pintype "bidirectional")
			(uuid "df424135-2cd4-4b34-8c05-027a19dc7017")
		)
		(pad "44" smd rect
			(at -1.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "PB5{slash}PWM1{slash}PB_EINT5")
			(pinfunction "PB5/PWM1/PB_EINT5")
			(pintype "bidirectional")
			(uuid "0af963c1-1cff-444e-b49a-6b1f61423eb9")
		)
		(pad "45" smd rect
			(at -1.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "PB6{slash}TWI0_SCK{slash}PB_EINT6")
			(pinfunction "PB6/TWI0_SCK/PB_EINT6")
			(pintype "bidirectional")
			(uuid "95fefd08-9889-401b-87d4-96c1e739d775")
		)
		(pad "46" smd rect
			(at -1 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "PB7{slash}TWI0_SDA{slash}PB_EINT7")
			(pinfunction "PB7/TWI0_SDA/PB_EINT7")
			(pintype "bidirectional")
			(uuid "be3f8f8b-0e12-4dff-9e6b-6f8023a23656")
		)
		(pad "47" smd rect
			(at -0.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU5")
			(pintype "power_in")
			(uuid "00dbf57c-db83-4f70-9092-258c618650df")
		)
		(pad "48" smd rect
			(at -0.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "PB8{slash}TWI1_SCK{slash}UART0_TX{slash}PB_EINT8")
			(pinfunction "PB8/TWI1_SCK/UART0_TX/PB_EINT8")
			(pintype "bidirectional")
			(uuid "4d835ca4-c199-4a42-b25f-a80bca349b6b")
		)
		(pad "49" smd rect
			(at 0.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "PB9{slash}TWI1_SDA{slash}UART0_RX{slash}PB_EINT9")
			(pinfunction "PB9/TWI1_SDA/UART0_RX/PB_EINT9")
			(pintype "bidirectional")
			(uuid "f082209d-c5e3-4753-a2c1-11c97b536eca")
		)
		(pad "50" smd rect
			(at 0.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-IO3(PG)")
			(pintype "power_in")
			(uuid "7e3c6c4d-bb2e-4005-ae78-c10888446f74")
		)
		(pad "51" smd rect
			(at 1 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU6")
			(pintype "power_in")
			(uuid "8356130c-4df3-4caf-9387-ac12a562f309")
		)
		(pad "52" smd rect
			(at 1.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "PC0{slash}SDC2_CLK{slash}SPI0_MISO")
			(pinfunction "PC0/SDC2_CLK/SPI0_MISO")
			(pintype "bidirectional")
			(uuid "dc46b75c-f060-4042-8a88-1e82929920df")
		)
		(pad "53" smd rect
			(at 1.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "PC1{slash}SDC2_CMD{slash}SPI0_CLK")
			(pinfunction "PC1/SDC2_CMD/SPI0_CLK")
			(pintype "bidirectional")
			(uuid "528071b5-5b6a-4e85-9124-2f0537273754")
		)
		(pad "54" smd rect
			(at 2.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "PC2{slash}SDC2_RST{slash}SPI0_CS")
			(pinfunction "PC2/SDC2_RST/SPI0_CS")
			(pintype "bidirectional")
			(uuid "d4b6e9dd-5ee2-452c-962c-4da97b0631ed")
		)
		(pad "55" smd rect
			(at 2.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "PC3{slash}SDC2_D0{slash}SPI0_MOSI")
			(pinfunction "PC3/SDC2_D0/SPI0_MOSI")
			(pintype "bidirectional")
			(uuid "a2a8bc93-4a8e-40cf-9510-b94d1ecb4083")
		)
		(pad "56" smd rect
			(at 3 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-CPU7")
			(pintype "power_in")
			(uuid "affbbe32-8153-4498-b54a-202c4b59f71a")
		)
		(pad "57" smd rect
			(at 3.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-IO2(PF)")
			(pintype "power_in")
			(uuid "0a55f912-80b1-43e4-a6c6-2b44ff42560c")
		)
		(pad "58" smd rect
			(at 3.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS4")
			(pintype "power_in")
			(uuid "9a15db9d-2692-4d53-9464-680a7e885279")
		)
		(pad "59" smd rect
			(at 4.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM8")
			(pintype "power_in")
			(uuid "b33aa2e5-12b3-4a1d-a18b-c3b993f6c352")
		)
		(pad "60" smd rect
			(at 4.6 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM9")
			(pintype "power_in")
			(uuid "3498bb3d-0f4c-40a1-b29d-5d275ec8fe5e")
		)
		(pad "61" smd rect
			(at 5 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM10")
			(pintype "power_in")
			(uuid "97f9140a-5f67-4ed2-843f-c65fb5bc231d")
		)
		(pad "62" smd rect
			(at 5.4 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM11")
			(pintype "power_in")
			(uuid "3db817c6-330b-4cca-a520-8828fdba6b4c")
		)
		(pad "63" smd rect
			(at 5.8 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "SVREF")
			(pinfunction "SVREF1")
			(pintype "input")
			(uuid "8e80c9ba-b637-4e97-a0e5-f93c74be7d3b")
		)
		(pad "64" smd rect
			(at 6.2 7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS5")
			(pintype "power_in")
			(uuid "b3ce27c1-6d04-4b6b-9738-4c0ec49fdf95")
		)
		(pad "65" smd rect
			(at 7.625 6.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM0")
			(pintype "power_in")
			(uuid "3f9954df-18f9-4288-940e-a857f668d0b2")
		)
		(pad "66" smd rect
			(at 7.625 5.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM1")
			(pintype "power_in")
			(uuid "04165eee-8363-48f6-901c-2d1057bcb19a")
		)
		(pad "67" smd rect
			(at 7.625 5.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM2")
			(pintype "power_in")
			(uuid "5f2ea7fa-e82a-45de-b0ca-308d271ff56b")
		)
		(pad "68" smd rect
			(at 7.625 5 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM3")
			(pintype "power_in")
			(uuid "d18aea9a-d718-4a63-ac38-be4f4a36f9d0")
		)
		(pad "69" smd rect
			(at 7.625 4.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM4")
			(pintype "power_in")
			(uuid "76fd44b5-7fff-419c-9ea2-fb611abaada8")
		)
		(pad "70" smd rect
			(at 7.625 4.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM5")
			(pintype "power_in")
			(uuid "a724cc37-4b5d-4a49-a4a9-55e0d5c15d1f")
		)
		(pad "71" smd rect
			(at 7.625 3.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "SVREF")
			(pinfunction "SVREF0")
			(pintype "input")
			(uuid "e3aa0031-347b-4fef-bb18-3aba52d71026")
		)
		(pad "72" smd rect
			(at 7.625 3.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM6")
			(pintype "power_in")
			(uuid "605a6245-764b-4e45-ac0f-25f69ef180ef")
		)
		(pad "73" smd rect
			(at 7.625 3 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1B-SZQ)")
			(pinfunction "SZQ")
			(pintype "input")
			(uuid "603eac0d-2a7d-4852-8770-a3203796eb83")
		)
		(pad "74" smd rect
			(at 7.625 2.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/电源/X24MOUT")
			(pinfunction "X24MOUT")
			(pintype "output")
			(uuid "c0fe48c5-a0d7-46df-8dbb-ee56f3ee16a7")
		)
		(pad "75" smd rect
			(at 7.625 2.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/电源/X24MIN")
			(pinfunction "X24MIN")
			(pintype "input")
			(uuid "ca0af3ac-ea8e-4b9a-915d-5180bd785c63")
		)
		(pad "76" smd rect
			(at 7.625 1.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "+3V0")
			(pinfunction "VCC-PLL")
			(pintype "power_in")
			(uuid "d7d6ea52-4194-47fd-affc-22ae66513584")
		)
		(pad "77" smd rect
			(at 7.625 1.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "EPHY-LINK-LED")
			(pinfunction "EPHY-LINK-LED")
			(pintype "output")
			(uuid "6593e325-846f-4e3c-9b88-697fd59d7060")
		)
		(pad "78" smd rect
			(at 7.625 1 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "EPHY-SPD-LED")
			(pinfunction "EPHY-SPD-LED")
			(pintype "output")
			(uuid "af0a2caa-299a-49f3-8ac2-fc871cc56bb6")
		)
		(pad "79" smd rect
			(at 7.625 0.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+1V8")
			(pinfunction "VCC-DRAM7")
			(pintype "power_in")
			(uuid "1099ed9f-6326-4be6-afd8-27bfb3d9d74a")
		)
		(pad "80" smd rect
			(at 7.625 0.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS0")
			(pintype "power_in")
			(uuid "a1931e43-1eeb-4b46-bd41-7bdd3a0292b0")
		)
		(pad "81" smd rect
			(at 7.625 -0.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "MCSI-D0P")
			(pinfunction "MCSI-D0P")
			(pintype "input")
			(uuid "dabb52a2-ec2b-4edd-a8f1-9a73f1468f2f")
		)
		(pad "82" smd rect
			(at 7.625 -0.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "MCSI-D0N")
			(pinfunction "MCSI-D0N")
			(pintype "input")
			(uuid "a83dbf76-7e90-4cab-ba85-c8d9a5bf31af")
		)
		(pad "83" smd rect
			(at 7.625 -1 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "MCSI-D1P")
			(pinfunction "MCSI-D1P")
			(pintype "input")
			(uuid "8a337eb9-1a78-4df4-b7bb-cad0f86a45bc")
		)
		(pad "84" smd rect
			(at 7.625 -1.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "MCSI-D1N")
			(pinfunction "MCSI-D1N")
			(pintype "input")
			(uuid "c4ac21d7-faa0-4e59-803d-473286458cc5")
		)
		(pad "85" smd rect
			(at 7.625 -1.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-MCSI")
			(pintype "power_in")
			(uuid "699159bf-fa61-43b9-8d3a-e659fecf9659")
		)
		(pad "86" smd rect
			(at 7.625 -2.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "MCSI-CKP")
			(pinfunction "MCSI-CKP")
			(pintype "input")
			(uuid "515515f1-3338-4cc0-9911-42a303aa6e4e")
		)
		(pad "87" smd rect
			(at 7.625 -2.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "MCSI-CKN")
			(pinfunction "MCSI-CKN")
			(pintype "input")
			(uuid "96d79f00-1885-4b99-b950-3b2014b0b2c1")
		)
		(pad "88" smd rect
			(at 7.625 -3 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "EPHY-VDD")
			(pintype "power_in")
			(uuid "9613d43a-9393-4cb7-ad1c-d9fbc59577c2")
		)
		(pad "89" smd rect
			(at 7.625 -3.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "EPHY-RXN")
			(pinfunction "EPHY-RXN")
			(pintype "input")
			(uuid "b4331d2d-bd63-4137-b0af-269ffeef5f41")
		)
		(pad "90" smd rect
			(at 7.625 -3.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "EPHY-RXP")
			(pinfunction "EPHY-RXP")
			(pintype "input")
			(uuid "a61ad7e3-29dd-4ec7-9e3c-4f79f6005355")
		)
		(pad "91" smd rect
			(at 7.625 -4.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "EPHY-TXN")
			(pinfunction "EPHY-TXN")
			(pintype "output")
			(uuid "6142065e-9c34-4342-a62f-a41aa34b3863")
		)
		(pad "92" smd rect
			(at 7.625 -4.6 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "EPHY-TXP")
			(pinfunction "EPHY-TXP")
			(pintype "output")
			(uuid "c23f27b0-dcc8-4296-839b-21994f8cadd8")
		)
		(pad "93" smd rect
			(at 7.625 -5 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "EPHY-VCC")
			(pintype "power_in")
			(uuid "a730abca-2d15-47fb-9658-72ab877214ec")
		)
		(pad "94" smd rect
			(at 7.625 -5.4 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "EPHY-RTX")
			(pinfunction "EPHY-RTX")
			(pintype "input")
			(uuid "2c5ae496-0554-4774-94ac-5c57d004f4dd")
		)
		(pad "95" smd rect
			(at 7.625 -5.8 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/电源/X32KOUT")
			(pinfunction "X32KOUT")
			(pintype "output")
			(uuid "c94b280b-7d10-4e7c-a093-738105441641")
		)
		(pad "96" smd rect
			(at 7.625 -6.2 90)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "/电源/X32KIN")
			(pinfunction "X32KIN")
			(pintype "input")
			(uuid "49a8ff03-fe2e-4cf4-9d60-2b66601fb2ac")
		)
		(pad "97" smd rect
			(at 6.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "RTC_VIO")
			(pinfunction "RTC-VIO")
			(pintype "power_out")
			(uuid "1240c049-8561-4455-a320-27d0410d396e")
		)
		(pad "98" smd rect
			(at 5.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "VCC_RTC")
			(pinfunction "VCC-RTC")
			(pintype "power_in")
			(uuid "5e1deaa0-b8a5-4eb6-896c-64cd9b5df76e")
		)
		(pad "99" smd rect
			(at 5.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/电源/RESET")
			(pinfunction "~{RESET}")
			(pintype "input")
			(uuid "8e5a8c35-72ef-4edc-9c93-9158ee631305")
		)
		(pad "100" smd rect
			(at 5 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "PF6")
			(pinfunction "PF6")
			(pintype "bidirectional")
			(uuid "53e8c0b8-423d-4ca3-9375-c7d40e581b81")
		)
		(pad "101" smd rect
			(at 4.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "PF5{slash}SDC0_D2{slash}JTAG_CK")
			(pinfunction "PF5/SDC0_D2/JTAG_CK")
			(pintype "bidirectional")
			(uuid "55656885-70e6-4486-8fd1-15214c9c4387")
		)
		(pad "102" smd rect
			(at 4.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "PF4{slash}SDC0_D3{slash}UART0_RX")
			(pinfunction "PF4/SDC0_D3/UART0_RX")
			(pintype "bidirectional")
			(uuid "6a20cd78-e101-44e8-aa3a-9a737cf9c652")
		)
		(pad "103" smd rect
			(at 3.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "PF3{slash}SDC0_CMD{slash}JTAG_DO")
			(pinfunction "PF3/SDC0_CMD/JTAG_DO")
			(pintype "bidirectional")
			(uuid "05b39413-eeef-4256-a409-3ea6faedf1e2")
		)
		(pad "104" smd rect
			(at 3.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-IO0(PB)")
			(pintype "power_in")
			(uuid "79c52395-de64-4faf-979e-0503d1aceb66")
		)
		(pad "105" smd rect
			(at 3 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "PF2{slash}SDC0_CLK{slash}UART0_TX")
			(pinfunction "PF2/SDC0_CLK/UART0_TX")
			(pintype "bidirectional")
			(uuid "6e0ebc28-f784-4be0-8be1-44f3493e12f2")
		)
		(pad "106" smd rect
			(at 2.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "PF1{slash}SDC0_D0{slash}JTAG_DI")
			(pinfunction "PF1/SDC0_D0/JTAG_DI")
			(pintype "bidirectional")
			(uuid "1f2597ab-c3b6-40ae-873c-f489baccb34e")
		)
		(pad "107" smd rect
			(at 2.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "PF0{slash}SDC0_D1{slash}JTAG_MS")
			(pinfunction "PF0/SDC0_D1/JTAG_MS")
			(pintype "bidirectional")
			(uuid "97275848-9322-4013-a693-64547ae80c23")
		)
		(pad "108" smd rect
			(at 1.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS1")
			(pintype "power_in")
			(uuid "57db90f1-3698-4238-860a-dd3a2b955fc8")
		)
		(pad "109" smd rect
			(at 1.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-USB")
			(pintype "power_in")
			(uuid "59104e18-29a6-40a5-964f-cc65ce3acdaa")
		)
		(pad "110" smd rect
			(at 1 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "USB-DM")
			(pinfunction "USB-DM")
			(pintype "bidirectional")
			(uuid "cbca5e84-478f-4fd1-acc6-32d9323d4b24")
		)
		(pad "111" smd rect
			(at 0.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "USB-DP")
			(pinfunction "USB-DP")
			(pintype "bidirectional")
			(uuid "2a1ab270-cfd6-4606-ada2-61d48fb8ddca")
		)
		(pad "112" smd rect
			(at 0.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "LRADC0")
			(pinfunction "LRADC0")
			(pintype "input")
			(uuid "7bd6b14a-2f50-46d9-b1f7-6fcf930dc662")
		)
		(pad "113" smd rect
			(at -0.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "MICIN1P")
			(pinfunction "MICIN1P")
			(pintype "input")
			(uuid "d75b850c-67d5-4cea-8aa7-7fb3ad6afdd8")
		)
		(pad "114" smd rect
			(at -0.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "MICIN1N")
			(pinfunction "MICIN1N")
			(pintype "input")
			(uuid "5aef5450-dfa0-4942-a615-807584026225")
		)
		(pad "115" smd rect
			(at -1 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "+3V0")
			(pinfunction "AVCC")
			(pintype "power_in")
			(uuid "c96b5ca6-ca9b-46b0-81ee-49f3ff05dc5e")
		)
		(pad "116" smd rect
			(at -1.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "GNDA")
			(pinfunction "AGND")
			(pintype "power_in")
			(uuid "3572ce59-d77f-4a5d-adea-51b5ded8c274")
		)
		(pad "117" smd rect
			(at -1.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "VRA1")
			(pinfunction "VRA1")
			(pintype "input")
			(uuid "960c5a80-6720-4ad7-83e0-a26010f8f6b2")
		)
		(pad "118" smd rect
			(at -2.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "VRA2")
			(pinfunction "VRA2")
			(pintype "input")
			(uuid "abfdba08-1f88-4936-ad88-f8b85d39f9e0")
		)
		(pad "119" smd rect
			(at -2.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "HBIAS")
			(pinfunction "HBIAS")
			(pintype "input")
			(uuid "e2ed5c89-b20b-4850-9b65-7b50078e7870")
		)
		(pad "120" smd rect
			(at -3 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "HPOUTR")
			(pinfunction "HPOUTR")
			(pintype "output")
			(uuid "cc5ef70b-f3d4-4d71-bcca-380655ae51fc")
		)
		(pad "121" smd rect
			(at -3.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "HPOUTL")
			(pinfunction "HPOUTL")
			(pintype "output")
			(uuid "887ab26a-e56a-4f76-a2b9-9498cd98128b")
		)
		(pad "122" smd rect
			(at -3.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "HPVCCIN")
			(pinfunction "HPVCCIN")
			(pintype "power_in")
			(uuid "3e5abc65-f8c2-4452-9de9-a0f47b47ba67")
		)
		(pad "123" smd rect
			(at -4.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "HPVCCBP")
			(pinfunction "HPVCCBP")
			(pintype "input")
			(uuid "5c885461-85b6-411e-8585-6c988d6f1be5")
		)
		(pad "124" smd rect
			(at -4.6 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "HPCOMFB")
			(pinfunction "HPCOMFB")
			(pintype "input")
			(uuid "fc58e7d5-d213-4b85-9159-e22f5d2228d5")
		)
		(pad "125" smd rect
			(at -5 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "HPCOM")
			(pinfunction "HPCOM")
			(pintype "input")
			(uuid "b4542ed5-a783-44f2-ba18-2b4499f13bcc")
		)
		(pad "126" smd rect
			(at -5.4 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "+1V2")
			(pinfunction "VDD-SYS2")
			(pintype "power_in")
			(uuid "3778891c-91c5-4607-9c75-f27f8d12a474")
		)
		(pad "127" smd rect
			(at -5.8 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VCC-IO1(PC)")
			(pintype "power_in")
			(uuid "4204a3b1-1f0c-46fb-a96b-0b636e86cb45")
		)
		(pad "128" smd rect
			(at -6.2 -7.625)
			(size 0.23 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "PG5{slash}SDC1_D3{slash}PG_EINT5")
			(pinfunction "PG5/SDC1_D3/PG_EINT5")
			(pintype "bidirectional")
			(uuid "3cfeb7fb-594f-4427-b02c-49c2983982e0")
		)
		(pad "129" smd rect
			(at 0 0)
			(size 6.6 6.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "EGND")
			(pintype "power_in")
			(uuid "1d26c17f-590b-4c88-a7fa-f82e8cbacf1a")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-128_14x14mm_P0.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "87a5cccc-7e43-47d3-8220-c59bc6ebafee")
		(at 63.47 73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2f2ca5ae-64d5-4228-9aa6-dd0f06689b1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9212df3a-cb20-41bf-947a-1e335cb209a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c2c8b86-bd5e-4599-9b7f-3f1c29bb2849")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54ca375d-aac5-4473-a221-37a9db8aaf83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/98cb49b5-db3a-47dc-8244-a34943090835")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70f7966e-ce26-42e5-88de-b52296b31d51")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10d618ba-f551-45c0-8ebd-2093debebbf0")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4388b97-906c-4353-bce1-1c1f59d2efe1")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "705bfc7f-c0c5-4837-8c0f-c3b25d646ae0")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e55f4a31-4ec4-4c80-ae92-f9b9b4514628")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d3c414f-3062-4766-bc43-b3f32e753c11")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d8165a5-0cb2-408c-aa9d-c246ed8e33a9")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3e166e3-20b7-463c-8b3b-9b1771885f3d")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00b40914-cc54-4372-bc00-db35cb010748")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81a1cee3-53b3-42fa-8b06-c40ab49f7a19")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8c2f91fc-1654-47da-94cb-f9fd7c6998fa")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "f17dc663-dd79-48e4-9b31-fe68b58d79e9")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "FB2")
			(pintype "passive")
			(uuid "4c3c53ad-75a9-42a2-aada-6c54bb3b76ca")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "87e9e86f-4b0c-4907-9a53-e85c5929d051")
		(at 67.48 80.53)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "6e279221-fd1f-443e-a2d4-20329763baf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9c16a93a-c00a-41b1-ae90-03fad3eb53f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4a6c2e2-1b33-4eec-be11-91195ae191ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5ff58db-4e53-43ac-9334-960c422da5a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/cebcda28-0bf6-4949-bb74-afac15895c1b")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71f00f94-4fd9-4f5c-baea-0bf8f1c5cca6")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6eaf9be-4859-4fa7-aa7d-3f7e6a4c2249")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9397cd41-1b81-4302-a519-e38e2346d8df")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "959c7b25-4658-48fa-a5c0-04ea4ef79d27")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db739984-4934-4cba-9dba-e73d28ac8348")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e6ed4d5-e06f-4961-8802-4479173ed69a")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7d89a5f-85de-44b2-a1bf-557a5d7107fb")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f966b0cc-988d-4834-a51c-728071f072f8")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d07f28b-7d8e-4139-9504-ca2f1830b37a")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6714e82-97b2-44d5-83bf-7d8f37933ae8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f35c999e-8c1c-4409-a3ab-7717116f755a")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "3f2c1665-fbad-4223-b7f4-555ca4b9c020")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "46f79c37-34a2-4d22-a252-087c825d98bf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "886594dd-696c-4b27-9f29-75c559add300")
		(at 71.49 67.98)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "9ffdf986-edf7-424b-a837-fa9619614b34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "98faa40c-3144-4624-be16-5f881f38166d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "da10babf-9419-4713-90e7-509492daea6d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3efb27fd-a398-4d9a-b21e-bb07258037ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f6cdf52c-1b8f-4d71-a178-6512d3a0c355")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9ee5f55-1dd5-42d2-b069-0bcfbad41b6c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3ab774d-97ea-470d-bb58-d19a382a36bb")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76bf120f-d398-45ff-9335-4af6428f5384")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f999e9f1-dfec-4846-8084-3bce3e526ae7")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0091c83e-aeed-4dd7-8fb2-83739d758e2b")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0cb33bbc-138d-4c77-a82c-0c480ace4921")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8eeadce-0df8-486c-8010-e50cbc631511")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6265c086-653e-417b-8ad1-e7fa4883f5be")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ade0208a-7a8b-493c-9462-6610588d2743")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48e0f093-ea16-4f92-ba3f-8384651f43a6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "215596d0-ab07-41a5-ae45-8e749b564f3f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "bd5edac9-da22-45dc-b24c-fc5c20caa78e")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "cd48609d-39e6-4ad5-ac24-2e5c14eaab02")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "89f743db-8a62-45fc-828a-27e6eef1e888")
		(at 79.51 67.98)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "aa820765-85bc-4352-95d9-13d329456519")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "680K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "a3c8771d-0b49-4535-b0d7-7c3f79bb40a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "47e058da-6cbc-4b1c-9193-414ac6d1ba64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbb03d15-d96a-42df-b3dc-1c1837cbae08")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/2d0f9722-9065-4985-96e7-5be53cb18a90")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccd27b51-2a81-4ba7-9de0-6b39b07f587c")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3770117d-7f0e-4b2a-9f46-9ad456a1375f")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b85f0355-6ebc-4489-90b0-a5ea0f33cb74")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ddd2ac4-0619-4850-b722-91416b7df16f")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22077073-872c-4c17-a2dc-426b7f93e156")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "291d03a9-0934-4a5a-883a-b9c8a8f58c72")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "146d80dc-a058-47a5-87bd-f20d866474dc")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00fac2af-043d-48c2-878f-f6327ebfd3e6")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2157033-a354-4de8-a7f2-fe98ba327b4e")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c805fa2b-550c-4156-bc9c-de69df77bf99")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5d089319-c5d3-402c-92e2-1871c107665f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "881be464-aba4-4a9e-877a-e38269eff93b")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "FB3")
			(pintype "passive")
			(uuid "44abf97a-ff9f-4fab-9d1e-56f771b60b9b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "8b2eff5b-2f33-425c-b247-8a89b2f41df6")
		(at 83.52 55.43)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "58751296-b6db-4d3c-a832-7936b7f54d09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "6bb8896b-a285-4c5a-9e66-deec6f3bdd63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "665cd01c-da23-4502-89cc-5cddcde4294f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "564729ca-4217-4943-8c88-1173c6440583")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/642ba4af-b4bb-46ac-bfce-34abc1ab32c4")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "904409a2-56db-4b9b-9604-351add84be1d")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71bf29aa-3af9-4e2f-870b-b30224ed5057")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "62b1887c-d82e-4ba2-95de-60e71036b819")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4fb31b6-cbe6-40af-a801-37d6be6d33ae")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "327e331b-2fb7-491b-81c6-408cb83a475b")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9251e1f4-f625-4932-8284-d3a7df26ada9")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d14419a7-fcec-4e00-9f10-64996f8daa91")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2c161ea-8b2e-404d-8348-6e5dce097921")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a82aabe6-faf6-40da-9086-ab833c7516c2")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed35a1ee-9738-46c6-a3ec-2526c71f7138")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "511e2135-f280-4623-9499-f8a41fd32eb4")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bb885dcb-45da-44b7-84ab-4cb2dc998fc7")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/电源/CC1")
			(pintype "passive")
			(uuid "b9179f1a-d734-4dec-aa18-498e45a17a49")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "8b7add4f-5899-4009-8199-3b22ab550daf")
		(at 75.5 65.47)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "306a50e1-064a-4046-812e-b2e76e568352")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "505f6153-28ca-4b9d-9900-77c3520ea42d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94fae129-b33c-4577-acf5-ee1744fb3b08")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef9cefb4-cb6d-4b11-8250-389c4c148877")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/b7dd1bc7-19ae-438d-bb7c-80fd4c84a9ed")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd9a1832-0a71-41f2-9053-2a962d77d558")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45bda35d-94e4-499b-8c2b-2ba22ee9daf0")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4c81878-3d13-4f81-be30-c710be95ff31")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ed59afcf-401c-45bb-914a-c6f8bf209e3b")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07a6db17-6094-4141-8abd-76236576de32")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fbb182a-e90a-4f17-95fc-418591ed144d")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8db5c96d-c3e2-4494-b078-a5ea3d0b95b8")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58cdc986-a374-44cd-b427-a860c0ec9a10")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef39ae19-3e6d-41ff-a9c0-7a0679878e60")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0aecb091-4126-404b-bd21-093794df5d97")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b2ae05fd-60b4-4936-ab89-f9814ea726b7")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "HP_VCCBP")
			(pintype "passive")
			(uuid "0c061e9e-c235-4626-aa4a-ca541d9f8551")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "68e91a72-4a76-4036-8149-abf03ac2e76b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "8c8c0714-e6c4-4412-b5af-3765822fcf3e")
		(at 87.75 65.3)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP3"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "5d95a2b9-bade-4be5-b501-f9a5427cfac0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1V8"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "58450a15-afc6-470a-a23c-35e880283f54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c336275c-54b9-43f7-aa31-c930ccec8c43")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64c6a6bb-dfee-4120-8081-cefa8b2e51e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/c88f0957-dfde-4b0f-b03c-f36f0df7ae33")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "26634319-de31-4982-b9bd-816b1b7c23b5")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "013b6e05-50f3-4463-9e97-8751f0fe1905")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "294dddb3-643c-4938-914a-42f372533c18")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "31b1cd83-0f18-4e85-a833-568e45d04438")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "d972f7f1-e56f-463c-a246-15ff5cf2fce2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+1V8")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9a3abe2a-a6e4-4c49-b96c-fb77dd799ca6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "8e142960-773f-43b9-b63f-04ebcf6c158f")
		(at 230.5 67 180)
		(descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U2"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "bca25815-033d-4287-8b5f-266fbf59831c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CH340N"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "22dae31f-d4a2-4fa5-bde2-2afd3ac9c550")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://aitendo3.sakura.ne.jp/aitendo_data/product_img/ic/inteface/CH340N/ch340n.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eabc6cff-37ef-4023-a376-23ae0635e8d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "USB serial converter, 2Mbps, UART, SOP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d04f9b26-7472-4d96-987b-39ae7f8b3487")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOP*3.9x4.9mm*P1.27mm*")
		(path "/bd45533a-bb41-4498-93a2-e6a98ad47a53/9583b07c-d2b6-4793-9580-d8d41502663d")
		(sheetname "/通讯/")
		(sheetfile "Com.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c2b6448-ef9e-4325-a1c0-3e43d499fe3b")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4af2950e-7442-42f3-b9ad-1054ad0d5846")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "277a8d6c-fc66-4b7d-bde4-e97e1c3b45dc")
		)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20422f1d-a1c1-4e8d-a3ca-886dc8970a12")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "cbbaaf1a-d27f-4fa1-abf3-2aa58d22c671")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06978b27-6f1e-4436-b22d-1b065f7f654d")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e1b0a76-15a0-4b92-9903-e6516b939b8a")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22cf02b8-28ea-4ccc-8038-8fc226ea0bf6")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67f91d06-0941-4d83-b52c-96ffaf8ef6c2")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c354260-c43f-42eb-8bb6-3406eac27001")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f2baec2-6f0f-49bf-a393-4179b872c649")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "492013a9-fb9a-4409-8fc0-0632c4c7261b")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c107ee8-da42-4b89-8822-fabd4df61986")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c8a1d1b-c812-44eb-b01b-24e638750dfd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "51edc3c8-a6ba-4c86-b8b8-7e98572cc720")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.625 -1.905 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "DEBUG_DP")
			(pinfunction "UD+")
			(pintype "bidirectional")
			(uuid "1e06bddd-b077-459a-8a23-cdc09d3e6499")
		)
		(pad "2" smd roundrect
			(at -2.625 -0.635 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "DEBUG_DN")
			(pinfunction "UD-")
			(pintype "bidirectional")
			(uuid "86ce1468-2db8-4cca-b7d4-40eba38c7f8e")
		)
		(pad "3" smd roundrect
			(at -2.625 0.635 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "5f5a3e37-0b0f-4190-b328-7b3a8f7de915")
		)
		(pad "4" smd roundrect
			(at -2.625 1.905 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "unconnected-(U2-~{RTS}-Pad4)")
			(pinfunction "~{RTS}")
			(pintype "output+no_connect")
			(uuid "68d3b28b-542a-4160-a3e5-3a862764692f")
		)
		(pad "5" smd roundrect
			(at 2.625 1.905 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "a0ddf302-6a3d-4ca2-a376-43ec22f9fe8f")
		)
		(pad "6" smd roundrect
			(at 2.625 0.635 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "PB9{slash}TWI1_SDA{slash}UART0_RX{slash}PB_EINT9")
			(pinfunction "TXD")
			(pintype "output")
			(uuid "9a174674-0c89-41dc-83b3-0c1a92225c56")
		)
		(pad "7" smd roundrect
			(at 2.625 -0.635 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "PB8{slash}TWI1_SCK{slash}UART0_TX{slash}PB_EINT8")
			(pinfunction "RXD")
			(pintype "input")
			(uuid "c6fd2ca5-76b3-41b3-8ec9-b50bd3add594")
		)
		(pad "8" smd roundrect
			(at 2.625 -1.905 180)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-V3)")
			(pinfunction "V3")
			(pintype "passive")
			(uuid "d3c13d6e-617a-4850-9232-fc2fe0d31a9a")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "8e4d9a24-364a-451c-afde-c68f506db533")
		(at 72.77 112.14)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "fe4b3b57-ba50-4914-9dff-7cc98fc7def1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "10247b70-5b31-4627-9e0e-37680e39dae3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "553c16ea-6ea5-4460-b044-8fbdb70d2fe1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cec0718e-c491-4b06-b758-659a5e2866fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/ca9e5ca3-c246-49ff-b02f-43b428e5301b")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "137fcb5c-b4c7-462a-87c6-7a9d976306c8")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f96d59e-40be-42cf-8b24-57d472aeb53a")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a16dc5af-702b-4886-a3db-3cc16c48acb1")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4135438e-aa83-4b36-8309-e072e5934c31")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3602591e-b24f-4b77-9b66-64867664b35d")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef32fe74-89cb-42f8-9b6f-796f717e5322")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "edbb3aa6-7b9a-43af-8f85-d5d024865579")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79d3684a-f69b-46fa-89cb-6dc69a8048a6")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1bd286c5-7cb9-4bcf-9b04-96fcc06daf77")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6250080-4186-49f0-a799-14b6dee94d7d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "936286f5-3b65-4339-a319-8d9df732fca9")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "PG5{slash}SDC1_D3{slash}PG_EINT5")
			(pintype "passive")
			(uuid "5d79b4d6-96c5-43a3-a5eb-7ddb8e6a3e7c")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "3690a34e-ff0c-4e60-8ec4-36c0b0062c4f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myPCB:RJ45-TH_RJ45-202-007-02"
		(layer "F.Cu")
		(uuid "8fca425a-f593-41fa-b190-f059050f00bb")
		(at 153.95 90.8 180)
		(property "Reference" "J3"
			(at 0 -4.955 0)
			(layer "F.SilkS")
			(uuid "6796ca87-6c15-44d6-bfee-bae3d5175250")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify right)
			)
		)
		(property "Value" "RJ45_LED_Shielded"
			(at 0 -6.733 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d0c683e-3df0-4f43-930a-71ea7bfa0739")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify right)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c282cef6-a901-4d98-a87c-b0b3ab38b5ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5f5f53f-4e56-4c4d-b8a4-a5ed47fa2349")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "8P8C* RJ45*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/36e36162-74ae-47b8-90a5-5167c9bfb53d")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.18 11.24)
			(end -8.18 11.24)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11011805-01c1-4d0f-9690-52094b570f2e")
		)
		(fp_line
			(start 8.18 3.74)
			(end 8.18 11.24)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3684e77-032e-467b-95e2-bc7ce86cbc30")
		)
		(fp_line
			(start 8.18 3.61)
			(end 8.18 3.74)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff646bf6-b3c6-470b-a866-3f68122562a5")
		)
		(fp_line
			(start 8.18 -4.48)
			(end 8.18 0.95)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6086c48c-3720-4d8b-ab99-b084a806ce3e")
		)
		(fp_line
			(start 8.18 -4.48)
			(end -8.18 -4.48)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f53621d-ed06-4e71-a56e-44a79226d5a5")
		)
		(fp_line
			(start -8.18 3.74)
			(end -8.18 11.24)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6982642b-5c2e-4cfe-a631-12d9f4c9b391")
		)
		(fp_line
			(start -8.18 -4.48)
			(end -8.18 0.95)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d39428fa-15b4-438e-a249-e6a1dd3342b3")
		)
		(fp_circle
			(center 6.35 5.84)
			(end 7.1 5.84)
			(stroke
				(width 1.5)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "59e143c5-45c9-4cd9-8ea8-90a57b5ab30f")
		)
		(fp_circle
			(center -6.35 5.84)
			(end -5.6 5.84)
			(stroke
				(width 1.5)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "32b134e4-42b2-4b12-99e2-51fda0d75c77")
		)
		(fp_text user "gge573552d11986f63c"
			(at 0 0 0)
			(layer "Cmts.User")
			(uuid "8f4bff90-6a56-4fc6-9b41-f75fdb130f95")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -6.35 5.84 180)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "622a4aca-5528-4771-a2fa-8522d93658d4")
		)
		(pad "" np_thru_hole circle
			(at 6.35 5.84 180)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "f4b839ba-782c-4dad-bc98-9fe100c5e02b")
		)
		(pad "1" thru_hole circle
			(at 3.57 3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 96 "EPHY-TXP")
			(pintype "passive")
			(uuid "e0f9a85e-1933-405f-be65-b27661025189")
		)
		(pad "2" thru_hole circle
			(at 2.55 1.52 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 44 "EPHY-TXN")
			(pintype "passive")
			(uuid "e7808a5a-465e-44bc-a115-06b0de10e591")
		)
		(pad "3" thru_hole circle
			(at 1.53 3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 78 "EPHY-RXP")
			(pintype "passive")
			(uuid "03d5a7a5-75ca-40c5-830c-c4e95539c732")
		)
		(pad "4" thru_hole circle
			(at 0.51 1.52 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 157 "unconnected-(J3-Pad4)")
			(pintype "passive+no_connect")
			(uuid "24f3345e-3aa8-4ace-858c-be3cd3dcc6b5")
		)
		(pad "5" thru_hole circle
			(at -0.51 3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 160 "unconnected-(J3-Pad5)")
			(pintype "passive+no_connect")
			(uuid "d812f965-f5ac-498c-b4da-b65d18985254")
		)
		(pad "6" thru_hole circle
			(at -1.53 1.52 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 88 "EPHY-RXN")
			(pintype "passive")
			(uuid "cb244384-8663-478c-bad9-e81ae9d6b19c")
		)
		(pad "7" thru_hole circle
			(at -2.55 3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 158 "unconnected-(J3-Pad7)")
			(pintype "passive+no_connect")
			(uuid "47903c1a-28d5-4858-a9a9-5a29add53864")
		)
		(pad "8" thru_hole circle
			(at -3.57 1.52 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 159 "unconnected-(J3-Pad8)")
			(pintype "passive+no_connect")
			(uuid "65de631c-a5f2-43ee-ba37-1cc762ce42cf")
		)
		(pad "9" thru_hole circle
			(at -6.86 -3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(uuid "00989c20-e7ac-457d-b124-74fa0f1c7503")
		)
		(pad "10" thru_hole circle
			(at -4.57 -3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 101 "Net-(J3-Pad10)")
			(pintype "passive")
			(uuid "38890de0-6049-4526-912e-fd4d8276c72b")
		)
		(pad "11" thru_hole circle
			(at 4.57 -3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d754186d-a537-45c9-9469-8cad5407f554")
		)
		(pad "12" thru_hole circle
			(at 6.86 -3.3 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 102 "Net-(J3-Pad12)")
			(pintype "passive")
			(uuid "5c52cd88-b542-4808-9ae1-0cdc84783625")
		)
		(pad "SH" thru_hole circle
			(at -8.025 2.28 180)
			(size 2.2 2.2)
			(drill 1.6)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 161 "unconnected-(J3-PadSH)")
			(pintype "passive")
			(uuid "b6b512b8-bcbc-4e8d-9dda-bf6844b2bc42")
		)
		(pad "SH" thru_hole circle
			(at 8.025 2.28 180)
			(size 2.2 2.2)
			(drill 1.6)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 161 "unconnected-(J3-PadSH)")
			(pintype "passive")
			(uuid "8f240980-f082-4719-811b-0c6a451b31b8")
		)
		(embedded_fonts no)
	)
	(footprint "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
		(layer "F.Cu")
		(uuid "929705ea-90ba-46e7-b641-95ea2d3779fd")
		(at 162.55 60.7)
		(descr "QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U3"
			(at 0 -2.83 0)
			(layer "F.SilkS")
			(uuid "26632170-f614-4011-b2a4-2d58543012d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RY1303A"
			(at 0 2.83 0)
			(layer "F.Fab")
			(uuid "673e9d86-6382-4935-abc4-252800335366")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "58f00749-bf6d-4f8e-9ddd-85c2fac91d77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "56739b66-5925-490c-8c1c-35a27631dc17")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "RY1303A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2ae1847-5de0-4af5-8af7-b612d704e64c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "null"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c1e53de9-f40e-40e1-b179-dca74c74009b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C2836412"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67f87307-149d-4eeb-9501-c4a00c9276a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0791468c-72f6-4173-82e5-584fda40c49b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/1438734a-8b49-4271-9715-3246df660f68/c4d00e5b-7a1c-4cfd-9443-084ae4f8d887")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.61 -1.16)
			(end -1.61 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "181167f7-f795-477f-a678-ecb1a3d3e2d4")
		)
		(fp_line
			(start -1.61 1.61)
			(end -1.61 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78bcda0a-a2f8-4ad3-bfd3-472802fc3e91")
		)
		(fp_line
			(start -1.16 -1.61)
			(end -1.31 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4289d425-dd80-46c6-a151-4a4f5da27f87")
		)
		(fp_line
			(start -1.16 1.61)
			(end -1.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5e0e3b7-ef03-450d-86f7-50cfebd91520")
		)
		(fp_line
			(start 1.16 -1.61)
			(end 1.61 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96e42bd8-503f-40c7-8a82-5ef246ad2f95")
		)
		(fp_line
			(start 1.16 1.61)
			(end 1.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1701c3c-3b7e-4af1-bae2-29ef4e366b1f")
		)
		(fp_line
			(start 1.61 -1.61)
			(end 1.61 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8422e6d5-b13e-489a-9a4a-bb870c75d6d6")
		)
		(fp_line
			(start 1.61 1.61)
			(end 1.61 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb3fe2bc-f0e6-47fa-91c3-536a760082f3")
		)
		(fp_poly
			(pts
				(xy -1.61 -1.61) (xy -1.85 -1.94) (xy -1.37 -1.94) (xy -1.61 -1.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "79a502fe-d681-4c9b-aa2e-74fa8e9bfa84")
		)
		(fp_line
			(start -2.13 -2.13)
			(end -2.13 2.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71a2e29f-7d74-45f4-8c8f-dfea0981384e")
		)
		(fp_line
			(start -2.13 2.13)
			(end 2.13 2.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5033972-391a-4132-bc08-ba96a440c85e")
		)
		(fp_line
			(start 2.13 -2.13)
			(end -2.13 -2.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c8efd16-9eac-4707-be8c-ba5bf6f6b79a")
		)
		(fp_line
			(start 2.13 2.13)
			(end 2.13 -2.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ddb77d6-4a34-4903-b86a-26e073e5b7e1")
		)
		(fp_line
			(start -1.5 -0.75)
			(end -0.75 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e055cbef-8c8c-475a-ae9b-30735106439a")
		)
		(fp_line
			(start -1.5 1.5)
			(end -1.5 -0.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80154c70-bd7c-4d78-9c94-e4227887db6d")
		)
		(fp_line
			(start -0.75 -1.5)
			(end 1.5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8931388f-28df-4dd9-839e-8687f65ee0a4")
		)
		(fp_line
			(start 1.5 -1.5)
			(end 1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1888a170-05fe-4554-8aab-3924c3f9bf51")
		)
		(fp_line
			(start 1.5 1.5)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9a92ef1-59fc-473c-96a9-b011973d25e6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b05951d6-08b5-484b-83d1-9428008ab29d")
			(effects
				(font
					(size 0.75 0.75)
					(thickness 0.11)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.41 -0.41)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "19cd70cf-c862-459f-9dcf-ec39d0a86aa6")
		)
		(pad "" smd roundrect
			(at -0.41 0.41)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "562f1223-004f-40e7-8a7a-da8293f6c30b")
		)
		(pad "" smd roundrect
			(at 0.41 -0.41)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "2897a865-ab28-4ba6-a11a-870fc7ef02d3")
		)
		(pad "" smd roundrect
			(at 0.41 0.41)
			(size 0.67 0.67)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "af5222b4-abf6-4594-8a39-278c8c0ad11c")
		)
		(pad "1" smd roundrect
			(at -1.45 -0.8)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND3")
			(pintype "unspecified")
			(uuid "a4850742-a852-48b1-893b-c21ee6ca230d")
		)
		(pad "2" smd roundrect
			(at -1.45 -0.4)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "FB3")
			(pinfunction "FB3")
			(pintype "unspecified")
			(uuid "34ddbb45-a0aa-48e9-a2d4-cf0cb15b5579")
		)
		(pad "3" smd roundrect
			(at -1.45 0)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "FB2")
			(pinfunction "FB2")
			(pintype "unspecified")
			(uuid "ec502270-566b-49a1-b04e-7131b6d29d7c")
		)
		(pad "4" smd roundrect
			(at -1.45 0.4)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND2A")
			(pintype "unspecified")
			(uuid "0c835202-80f5-43be-98cf-cb15fda35bbc")
		)
		(pad "5" smd roundrect
			(at -1.45 0.8)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND2B")
			(pintype "unspecified")
			(uuid "2b87a7f6-7eda-4401-bd38-9dd4ca264fa7")
		)
		(pad "6" smd roundrect
			(at -0.8 1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "SW2")
			(pinfunction "SW2")
			(pintype "unspecified")
			(uuid "0232aa23-1153-4ba2-a21e-44ae46031000")
		)
		(pad "7" smd roundrect
			(at -0.4 1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VIN2")
			(pintype "unspecified")
			(uuid "9b2d8b0f-ea9b-4eca-8859-cea673d994dd")
		)
		(pad "8" smd roundrect
			(at 0 1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "EN2")
			(pintype "unspecified")
			(uuid "0fb9492b-5869-437d-985f-2c0f20b108aa")
		)
		(pad "9" smd roundrect
			(at 0.4 1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "EN1")
			(pintype "unspecified")
			(uuid "0b7acf82-df46-4e7d-a3ce-8ddca036a9e4")
		)
		(pad "10" smd roundrect
			(at 0.8 1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VIN1")
			(pintype "unspecified")
			(uuid "13f920a7-49f4-49eb-8c66-a5fe428cdef6")
		)
		(pad "11" smd roundrect
			(at 1.45 0.8)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "SW1")
			(pinfunction "SW1")
			(pintype "unspecified")
			(uuid "79dbbcf1-0f32-4617-a0b3-8722d1ef991f")
		)
		(pad "12" smd roundrect
			(at 1.45 0.4)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND1A")
			(pintype "unspecified")
			(uuid "d214c7dd-5fde-408b-948a-773b9c0e8beb")
		)
		(pad "13" smd roundrect
			(at 1.45 0)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND1B")
			(pintype "unspecified")
			(uuid "42a9936e-ba43-40ce-b06d-68ff0caf5dfb")
		)
		(pad "14" smd roundrect
			(at 1.45 -0.4)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "FB1")
			(pinfunction "FB1")
			(pintype "unspecified")
			(uuid "58ea41f6-85b3-4437-b62d-22d99777bf43")
		)
		(pad "15" smd roundrect
			(at 1.45 -0.8)
			(size 0.85 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGNDA")
			(pintype "unspecified")
			(uuid "10e9a94e-bf19-490e-af4a-0a3a29c1fb0f")
		)
		(pad "16" smd roundrect
			(at 0.8 -1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VCC")
			(pintype "unspecified")
			(uuid "803db41c-60cb-4a6a-8b86-26aaccaca5a0")
		)
		(pad "17" smd roundrect
			(at 0.4 -1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGNDB")
			(pintype "unspecified")
			(uuid "78f72dc6-a386-405e-9e04-1799fa2e1262")
		)
		(pad "18" smd roundrect
			(at 0 -1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "EN3")
			(pintype "unspecified")
			(uuid "44cbb2b0-3cd0-4bdc-8532-1c925d90c720")
		)
		(pad "19" smd roundrect
			(at -0.4 -1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VIN3")
			(pintype "unspecified")
			(uuid "fc354f44-08f0-4c62-9e7c-1dc1a15fcf47")
		)
		(pad "20" smd roundrect
			(at -0.8 -1.45)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "SW3")
			(pinfunction "SW3")
			(pintype "unspecified")
			(uuid "99ecdd86-c7be-4272-b17e-c5f9c202822d")
		)
		(pad "21" smd rect
			(at 0 0)
			(size 1.65 1.65)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "unspecified")
			(zone_connect 2)
			(uuid "070b9b5f-2b19-4383-98d9-c9c3d2382033")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "9304b047-a036-4bbe-a80d-dbe9c918aa9b")
		(at 92.6 116)
		(descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x03 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.77 0)
			(layer "F.SilkS")
			(uuid "f2fecdca-ed04-4044-9690-9cf9bf0ccd5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x03"
			(at 0 7.85 0)
			(layer "F.Fab")
			(uuid "db3b9464-4cf5-4ace-ae43-edeb92d930e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6afb8ea1-fd23-4194-9438-81baabd5c6db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "70515c26-720f-41fe-997f-2c767989ca8c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/bd45533a-bb41-4498-93a2-e6a98ad47a53/996cc5cd-ef5c-4462-a8c7-3c41a55ba569")
		(sheetname "/通讯/")
		(sheetfile "Com.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00ac0664-94d9-4dc0-9b4c-0063c833f904")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78489225-8a0b-46bf-94d8-de52228ca4f9")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07f88877-e35f-4a6f-8cfd-2f5600788847")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98a8edf6-bed8-482d-8840-cd35bf4a49d9")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43724fb4-9af9-4304-ab72-1c17a2c2e986")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "981985fe-44c5-42e0-a905-698b599c56e0")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff9e1d23-99d9-46b4-8bbb-cbe01eb84e1d")
		)
		(fp_line
			(start -1.8 6.85)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35df19b4-c7d9-4b95-86e1-d016dce580f6")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91d4f395-d27b-4675-b253-58b4eec9f5d7")
		)
		(fp_line
			(start 1.75 6.85)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33bbafb3-6f9f-4ce1-b690-ab7ea1673b30")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f851f52-7501-4e42-b050-20ad8c62c4a4")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "430972f4-d893-4b98-aee7-eaf3039a8557")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9035323d-9f83-4828-9df8-ba4b4cefb9d8")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1fc76b0-7203-4205-8ff5-e980f00392b1")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e48a6b16-08fa-4a6c-bb7b-4dd71e89a662")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "f50ef30d-25f5-4e5b-b50f-3ad4c11cd7a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c8ad5dde-df7c-4b6c-b8e0-cef8bcbcf2c1")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "PE21{slash}CSI_SCK{slash}TWI1_SCK{slash}UART1_TX")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "d6cdcf9a-317b-4dbb-898d-ad225426d717")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "PE22{slash}CSI_SDA{slash}TWI1_SDA{slash}UART1_RX")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "9029a1af-939f-4167-a113-ad18f9f2cb07")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "94127603-1be2-4916-b25a-8c35cbf1b05c")
		(at 238.125 68.405)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C64"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "aef36ab3-b697-4f7f-8186-d80da0d81180")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "d52a245e-6b74-4da8-b762-503729335f78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abd774df-5857-4afe-b3f7-20f5ba736ffe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c73f44e7-c798-4f99-a31e-3448d1022b9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/bd45533a-bb41-4498-93a2-e6a98ad47a53/5f4cff66-20fa-45ad-9e44-90576f0ccf6c")
		(sheetname "/通讯/")
		(sheetfile "Com.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "641ae5fc-acd8-4384-a2ca-59be4cae1860")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8843c7d7-29bc-4629-b1e0-5107d45a7a0a")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4aa6b02b-9042-4125-acda-d5fb64338b0d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f88ec4c-6b19-45ef-8629-8e6d436ac847")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6620bb8-eff5-4422-a2f7-850b8ec36aaf")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20d88ba5-f64d-4f10-9454-46f4f22fa1a4")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b44c2934-79b1-4c79-a448-039cc471b15f")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37655c5d-f046-40d8-a167-7cb6fda45a1b")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9c96db2-70e9-4e91-93a7-0d2cd2d3307a")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15e5d628-4b40-4573-bd79-067c465fe4b1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0d6c0c68-3ffd-428c-be47-8ab936545201")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5f1fd884-126b-48b4-8a2a-2116e6473f4c")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-V3)")
			(pintype "passive")
			(uuid "1e045a41-a790-4497-a605-042e35422488")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "941616cd-6a14-4fa3-90c3-8bda2f6bc5a7")
		(at 63.47 75.51)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "71312f2a-77be-4bf4-b708-9225b7ddbbd2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7635942d-3bc6-4306-891d-bfddc56d7ff4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dfc36cc4-ff8b-4c2b-b1b9-e95f3197da19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54f2a774-2860-4fb6-b23e-ca8140c640d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3b815634-34ad-4846-99e3-1ac85a720240")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f0839d6-dced-42fc-9be2-772f58a84e74")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0935756f-5966-43e5-b76a-f4bf6567b661")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c162d293-7f1c-4a68-9699-487cc5b59eea")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8749e31e-c497-4698-9d22-dc330d0672b4")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1bfd222d-54dc-4ba3-b18b-0c1895440f2c")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee52948c-2849-4568-9543-438d5a2526e7")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8b8d178-cb99-4ffe-a3cb-17b285106c9d")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4100d47e-7cf8-4076-9cc5-51891e0050ec")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "accc5b0d-499a-4c09-ad0f-e6b11177ae8c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f5e9165-ddac-4e64-8395-c50a073b4c4e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f17722da-c361-4e6e-b117-0764014efc89")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "4d93a69a-fc32-4784-8005-2da053486755")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5f247e1b-d290-4fdf-9cdb-645463b89310")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "987c827e-e93f-44ff-9f4d-e626bf831179")
		(at 63.47 80.53)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "abb06374-f69f-4e2d-ba7e-6425f3b8a025")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "f8d0e7fb-9d7c-4673-891f-c72ab424c1be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff6748fa-2efe-4bcf-bca9-18b48fc6f2ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1eeaa15-e89e-4e95-9812-15d3917a6dd0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/6f888262-a844-4968-8d66-7933dcdade56")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84ac6823-4ce5-4b84-8723-10cc33b741d7")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "771e99ea-8559-49e5-8388-8721a2478a8c")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b0db6a2-0fe1-495d-86cc-a838f3bfe1f3")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b19f6f4-bbe1-493c-85b7-03d6c6022d10")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8ecbd2c-c0ca-453f-aefa-a0013ccdae7c")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7df92a9f-b797-428c-a436-3134d4092d8f")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07ca9c63-6d8b-4c61-b708-66bd7a277005")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1996c744-a343-4ef8-8a16-d4da9272a9c3")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fa808d0-9864-437a-a40a-87e02f8223d3")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48f97353-27e3-4506-a69c-71aa1fc480ed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "98e6649d-e450-4691-a869-ff650943b8b1")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "1a924d0b-8ec1-41a2-93b6-e137be6ccc69")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9d14136a-feac-49fa-8915-341b5795e66b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "a5b958c5-b048-4053-9a34-ca3cb4001ee1")
		(at 79.51 73)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "1b131b32-0f63-4a80-8ad8-c5ce46f1b08f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "160eac16-3c0b-4e51-8292-c11666a08bbb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "85d0dc6b-4f4e-4bd3-af3b-d840c27ff496")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f340d02-57a7-44b9-bb36-4d1cbb8988f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/55426719-e824-4de2-a59f-523c840cf5ef")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e427ed1-26cc-4834-8625-2b9a0ebaf368")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8605580-9882-4639-a8e5-78fdc061ce64")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "777ed8fd-0476-46aa-8e66-70c5353b8b4d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "619c5482-5973-4695-a3c0-a85a279e863c")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2aeb0244-6a5c-4447-ba2d-67d5d54bba70")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de2f0e41-745e-4069-8efa-e28f35f836cc")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb02ae28-c766-4687-b430-65fa97db8a5c")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fccb8100-46b6-4b5c-97fe-27c159e84fad")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3f537c2-c5e3-4f76-b975-ba04d1023a95")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7140967-4a64-4be7-903e-6b78e7b611fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "881a08a1-ee3b-4dbb-bd35-76d6e289fbfe")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ff17c816-7788-4d29-8b39-9d12dbf674f0")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "FB2")
			(pintype "passive")
			(uuid "0c6ecb7e-b1dc-4d27-85e4-61dcc2af990e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "a7a23e51-12e2-4075-aff8-d4f18e71c379")
		(at 67.48 65.47)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "68a7cef1-2ac1-4a36-b3ae-26b55cf3c60d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3521161b-2bd4-4781-b561-465391103b08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbc25058-565d-4ec6-8c0e-bc86fc52e167")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "96ddbd89-2f24-4729-82bf-0a4f2cee69fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/bc0fcc7b-c1d0-430e-b16a-54c346bda6ad")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0591a75-9262-46b1-b6b0-795bc2529bdd")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2fbd8e86-7dbc-423e-8915-4f3f8e15747e")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25662b16-8624-4fa6-8fb1-eaca7f43119a")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "638f2caa-03ab-493f-88d5-5d6fb80936b2")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc958243-4761-47aa-a59a-509d970463be")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef5120ac-fc44-4d93-818c-c644a5d26786")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cabb3f0d-20e5-4e33-9f09-b657e6e00e76")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ca1bbcd-d48c-4468-8300-9bb5a17ed2df")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57135d88-8d9c-468f-8c1c-78715c2003c3")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19798ddf-3a14-44c6-a2d8-63cde09058ac")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e80703b4-96f3-49c7-9a7e-340c8417eed0")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pintype "passive")
			(uuid "0e51731d-e970-4b7f-a6d7-05333117d304")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5442fa00-d7d6-452f-9479-2a6d5836a390")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "ab7099c7-1865-401c-9439-bf7342d0f174")
		(at 68.76 117.16)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "5e6f9df5-3a84-4ef9-9e78-db5cf5dc93c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "44f31079-2d5b-43c4-9643-8ee89a4de9a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5558a9e4-32ab-48ab-9cb0-e13ea8d6471c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ceee4b71-1e88-4beb-8d78-f2e4524bba48")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/a8f1b80a-50f2-4c29-8832-ed67fa3b6fad")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "992caabc-89a0-4468-a731-e782c35dc36b")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0b10417-a0ef-48e2-98c8-b4118d1c33b2")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c88728ee-f1c7-4f64-983b-b460557cb998")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "587d6e56-fca0-482f-a678-16f771999629")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1d24a2e-5f31-4a09-808e-b0d3289516f3")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6a2dc37-5f24-4a3a-9aab-73e267d8efae")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bdd6bca4-dd31-4873-b079-c970dcbb55ae")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82f00c31-a958-4ff8-a5c7-d3d1adc834c5")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d57c9a17-4bd2-4384-a559-6433c66612d3")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c345005-5880-405f-8e63-3e8cc0148d19")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "347a7864-6638-4f81-ba4e-dc1477f35a89")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9445ec23-74db-4f35-b224-07f6c66b4234")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "EPHY-RTX")
			(pintype "passive")
			(uuid "1b5acb3e-6d6f-4260-a66d-b02544642f1a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "acf4b878-651e-4274-af67-e8e6139928f3")
		(at 79.51 55.43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "bfb85805-d19d-4cc5-8acc-73cc66cb1817")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8b60fa7d-ffd9-467d-af87-ce6d49b7509c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d529d492-7f12-4c13-9ce7-6f182c8ceebd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "050dfe9c-eb9c-4619-a126-7433d3250c40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/702ef44e-c10d-48a2-93af-258c7aafb504")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5754c38e-0557-4173-99c1-64c0478711da")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3de39ad4-be15-4582-8017-c8df4429be52")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57c83394-021d-41d5-99db-90bc75acb819")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09ba2566-197a-4ffa-9961-6aabab757ae9")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ee70b17-7ffd-4155-b153-1cfe09cefe14")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57b363b2-86f3-4ec1-a6dc-54cb80a2655e")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "208dc3a1-23ab-45c9-8f39-6ce8eb9e3b8c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6adaf56-ea60-4e90-8e70-c45cc544b7ab")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf87047d-786f-4628-8cb1-0e8ce59263a2")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e5191cd-f5a1-41fd-b532-f65ce99e5258")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "caa9946e-4ced-4982-a8f0-03d6619b6459")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3b829c97-b469-49cb-a081-596e478f74c8")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/电源/X24MIN")
			(pintype "passive")
			(uuid "2960d694-d38c-4697-afd9-ce8b1f6ce316")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "b03c0d9d-30ea-4c40-b588-b53f58f29591")
		(at 98.88 119.95)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "02143ca0-d400-444f-90a3-a0ea36b3db01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c8a9e10d-e811-45d0-b2de-133347d54e78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4022180-5824-4ffb-979b-d7ac532570de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0349608d-92cc-4128-95cb-ce01675f1ad4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aaaf3f24-1f7c-48e4-abd7-3efcb84c2d78/15309c2d-faaf-4189-bd84-56c4b8e8f735")
		(sheetname "/主控/")
		(sheetfile "MCU.kicad_sch")
		(attr smd dnp)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ea1ac67-0e23-47a3-8e67-d91d0f68a7fc")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d586f8a6-f9e0-44be-9e63-cae84b2064f5")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e4319eb-a897-4cab-aefc-baac096392b9")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13b3c675-bdd2-440b-9e0b-ad304658e616")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b41af850-4bac-46b0-bc91-42603a9ede0f")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c76b67c4-16dd-47dc-b8bd-7cb319c484df")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe91f4a7-e574-45a3-98e2-8319254455c8")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f301e051-d998-4d92-b3ef-863e62740643")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca785ead-7031-4cd4-93f0-36298d7ae0bc")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6ad3ad5-d392-4a7f-ab18-346a26e2c8eb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "44bbc800-2f33-42ad-8307-f448ab82a368")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "ff372aa9-517f-49dd-8e56-1f8dd1d36480")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "PE21{slash}CSI_SCK{slash}TWI1_SCK{slash}UART1_TX")
			(pintype "passive")
			(uuid "ea0e8977-3879-4641-a76f-52a28fa4eaa6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "b0f309e0-236d-496c-95d3-510e82963dd7")
		(at 63.47 78.02)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "3afa0446-fa8f-45c9-b84e-1c05db79192c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "678a15eb-66a2-415c-ba52-6cf421c21d5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b248a3de-389b-4c41-91ad-ac8d98cd7c86")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fbfa2f2a-547c-49e6-ad85-c7c02fbdb382")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/0d758a81-786f-4700-b763-0fc8110b8c1f")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7abc6b6a-ee8e-4e8f-bd8f-eb9e499a4dda")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8650076a-5d94-4eb8-8f08-235727ea8df6")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1552c02b-21c2-4d45-8634-dc90b0c57c78")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8abf14a3-ce5e-4fcb-b5b5-f35daf7a4659")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edd35556-4b31-407a-835d-f1efb8934a70")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a49eb875-172c-40ed-8a9b-102bd6c5a33a")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c09aa677-5325-4881-b4e7-4c857c5dfad3")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99bd91be-9534-412c-a1c3-1060b0fbcb4b")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbb5b060-6684-40a1-9076-d5c65668aaf3")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b71b29a6-828c-487c-bef0-0130d1b0e139")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f6e30485-abd9-4e4e-85c3-9c3139d44e7d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "e38c097e-afb8-420e-991a-4985a02f4a3a")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "FB1")
			(pintype "passive")
			(uuid "5166e79b-43e2-45ec-b636-56a06b722144")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "b29d4a07-3b1a-492c-91b8-de5c96cb31ab")
		(at 75.5 75.51)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e5404d3c-588e-44ee-89af-763fe8e9f8af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "e536ce2d-b328-4b77-94b7-b40ccd80c2e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f75d208b-5c45-4995-8fe0-dbfac8102817")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32061a61-9574-493d-b19d-61ea7ff23fe2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/fd01d56b-18e1-4825-8db5-46fb47c6fb93")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61e9818c-e2c3-4a7f-bcfc-6df1d900a62d")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d60dd8db-f250-455a-b9ac-b4e2088e03d7")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dff94267-33ac-435e-9f41-42fa2e822e3a")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06132890-0f04-419a-87e7-4d13d9069ffb")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78997745-e6bf-40cd-ba36-940ae1af186f")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98d5d86a-8364-46d9-b0c3-8b7eda45ab63")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5cb7760-87e4-4330-895d-f44ec2986f08")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c278868b-f7f7-4dd1-8aa9-6d37c099fcaf")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8fb14b8-7560-4ba7-88d1-ac2c8be04d83")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "596dd0e2-8cdb-41e0-a9d7-41163ab52ba1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3e53e830-f7c6-4353-9cb0-eefa07039153")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pintype "passive")
			(uuid "b80dcedf-7c2d-4d29-8c74-3f1476516564")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "8786a99f-f169-4ed9-bd86-9ecd3da09ea7")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "bb3f868f-c730-46ce-87af-bc8e7597c3f6")
		(at 75.5 73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f7890827-91c3-4f32-98a9-5288dd53ec72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8ed898c5-e3b3-4b78-99d2-e69f40513287")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f04939fb-334e-42c6-952a-fa711632130a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "84e97501-7053-4d5d-9fbc-ef9f19d6463b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/e25fa133-af39-43d9-8a38-731f447dfa6b")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ab76edd-01d2-46b2-80c0-318d22a76530")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45c59e4d-b886-46b9-bf8c-0db02515d3d5")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8dbef84c-bfb6-48c6-987a-39efeacde069")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fc9eb6c-e0e7-4891-967b-fb4f00123eed")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef31caed-0c67-42c1-aec3-8ef5f7ceb629")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb307dee-53b3-45f0-8ce7-41ae19a60b76")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b757be7-468c-4490-8b8b-7687c0c0aa8c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68a9fc8e-2e69-4c18-829a-131e7251312c")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2de4437-14fa-4cb5-9313-8ab99f939d64")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d96c702-a103-4946-866d-7bef4d1a4230")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7614b2c3-84a4-479f-a2f7-50b93cde00fa")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "SVREF")
			(pintype "passive")
			(uuid "07664dbf-e7ca-4dd2-81dc-4507243e35ff")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8ba6def2-8227-467d-aa96-a7c6e4a58b14")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "bb941db3-2220-40b9-9d7a-d1acede931c0")
		(at 77 123.95)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP9"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "5055b2f2-b6a1-4c11-bb1a-57b4a7bda6b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BT_UART_RTS_N"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "83f3efd0-68b1-4847-9c04-8bd38f1b8b09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b2302ee0-a601-4280-97c8-7f5403212dc5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee0f3f96-1abc-4f4f-b3ed-fd63dfda2184")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/5a350f58-98fa-4bf5-9fb2-17cb155606e7")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "39a754e9-0e38-4533-8452-57742efae9c3")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "14471cf9-1b13-4ee5-a95a-e7f0d56b70df")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e903fc31-64cd-4e3a-92fa-1e369a9b8fe5")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "83a423a0-5bbd-45aa-805a-1842e59b08d8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "2a13702b-b868-4713-95a2-e61cfc4ed7b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "/网口/UART_RTS_N")
			(pinfunction "1")
			(pintype "passive")
			(uuid "c88f0fb6-6110-45f6-99bd-108b29313bf8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "bba95939-3e93-405a-ba83-f3c95954eada")
		(at 79.51 80.53)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "ebac6fba-b10b-4cc7-8f33-dfa761cd60c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "4ff6b7b3-05aa-40bc-9009-28468e6aa717")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea730952-b624-4eef-b5de-beeedeaa13fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7988b7f5-025d-45f0-8baf-02e3c042876d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f17f8884-f429-4845-91ce-8eb81dd3f2f1")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06e1bcdb-fad9-406d-b9f4-cb24bb7c22fa")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e89066a5-c7a9-4b49-8d20-04a8e9d852ca")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "389755c7-0c59-46e8-97a0-4eb87694e35c")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b873e3e-ae99-4c27-8e7a-798e2720ab5a")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab1bf5c7-69d2-4581-a876-bca78ef829b5")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af86e8f4-4043-4f09-9fb6-62a3e123f4f7")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb907477-6b82-4e37-8ad0-60e6bdc05c3a")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3613d7a5-31e7-4ea6-9546-6e968e76b08f")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de855eaa-d02e-4ea5-8299-ef911660be17")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f59e6e73-523d-4ce6-b4f7-ff6fe739b0af")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9caf5bbc-0ec0-4020-b38b-47add844e626")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "0dd7607a-54da-48a3-a4f6-bebb1f6ccba3")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "FB1")
			(pintype "passive")
			(uuid "85b43022-4527-47c2-843f-62c91ab08bb2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "bd3a34a5-130c-41c5-9d11-1e3b3966f53d")
		(at 67.48 67.98)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f5ee992e-b58c-4df8-8a95-d8cf867ae714")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8719fbc2-7e04-41db-b3cc-4a413680ab99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7bbc3f78-abff-4d32-9b10-488b7bee0317")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1aac30f5-b773-4f9f-ae68-74c53871a009")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/7bbc3af2-94c2-4733-b90b-71391d214bb5")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bdb493d8-05ed-41bb-a938-c7fa2a53d8b6")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "123f8eed-1198-4368-b6ad-3a1a02e5e6b3")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ade4ad8c-1603-4e55-97b0-7735046e9b3b")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa1d5647-1a59-4a4e-bd9a-51598e1e1835")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f0cdb4a-a220-42f3-adea-19aa5a764e69")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1ba2318-803a-4bbe-a233-505700391137")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e51a616-4e51-4029-b092-8bdfb5330cbd")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5748be46-cf61-4424-8bdb-68dab240db72")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98c0164f-c5ef-46b4-8f72-a52dac5d28b1")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e87d2b4-3883-4ec0-bc87-0e199346be97")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "db76cc46-5a89-4e65-b464-619f9163da77")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "4cbab3ae-6004-4b91-882e-c5f569cf7f5e")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9166d612-064f-4103-9279-ede5c87a9ba5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "c2bf5b31-6161-4eb8-9139-c1c2d271c57c")
		(at 67.48 78.02)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "87f25822-3119-451c-9495-bcd5d3088cee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9e9d8828-b296-4352-af61-ea7eaf48df80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0f2c515-59c6-4b55-9ffc-4903cd76ed4e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8e1b636-381e-4b00-9401-4e67e3f9cdff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/c8fd0863-2ef5-40a6-8d70-2f02dc386c67")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be829e0e-9144-448c-802a-531d9ce63232")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d775efd3-2ae6-400b-8b20-6231f13a5ad5")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5f4582d-432b-4332-aade-fbb16391b202")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5ca23f3-03e0-4f3c-96ab-ee848cc480d4")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afc6e96f-180c-451d-92ea-dcad27956757")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8761734-d450-4b4d-8909-f99528ba74df")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91e3c4ce-5f14-4c60-9539-8d7552293266")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "977b23e5-579f-469a-9520-e8e698c5c6e4")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b4ee979-226c-4dc3-a0f1-6fa0b31fe57c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "510482cb-5ed0-417f-ba64-21b43ecfa787")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5aab86de-82c9-42f2-a087-a64275e08c68")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "ebb5e067-c92d-4d17-a851-2b327b5914c7")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0db83793-3159-442a-a17c-7d75a778e8d2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "c328be91-0ac0-463f-a1f2-97e3d340b319")
		(at 71.49 62.96)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "9f27dc30-0213-49b2-9a26-695d1c4d9fd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "ac42906e-b9d2-4808-b280-9f1b418552bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "16ceb9b2-180c-4550-86e8-8c112804ece9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "273eb505-5713-4885-bae0-bfb35a6d5a62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f26646c7-4fba-44a0-9ba1-8e94f2a6e2cd")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ed109e1-103b-4357-8c39-0d1b755f4857")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed4d9e99-7001-4f46-9e4d-35564a2becdf")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b87242b-2afe-4b6e-b9c6-01ce302f1fcd")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffacd07f-2d2e-4796-883b-ae3833c09a76")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bfcd668-2cc8-48ab-b984-9e37a3fcb664")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e931538-3e68-4838-9614-cfc951e3abf1")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bb0421a-7140-4ae0-af30-856771dfa87d")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "edb8c0d0-6c11-4602-b00b-0b2eeaa995de")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7158ee0c-5cbb-4b3d-8c48-2f804664b37d")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f6f3bf3-d11d-42ed-a207-6e370f827bab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ceba8799-bb0b-4709-9fc4-c8e25bbfcd49")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "596ae916-5fcf-4d73-bfe9-fa00222880e8")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "08335b4b-7243-41fa-8fdd-e8fe75ec0cee")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "c3711251-61ae-4100-a72c-48d4cb4a9ffd")
		(at 79.51 65.47)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "18b29a1f-41f9-4801-adab-57bd890ffdfd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7d832e7a-74c3-4d47-b91d-febcb9974fd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "27c7fed1-f9ea-4d69-bacd-0d6dfe92c3d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "804b6f8f-532c-4feb-9987-c021af790f89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/028fd6f3-6b3e-4865-8c50-7e183933a2cd")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2387a96-5461-46ca-a8c1-4fabb4134ea8")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5c32c34-3b34-4bfa-8ab4-87101270941c")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cc7b6d0-278f-4431-b49a-a03c1fff90a9")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbe71b29-af36-47e3-b5aa-ad13781810b6")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd31684e-f844-493e-a2b0-a18b363f6be0")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7701ff6-8de6-4291-94ec-c9be9cb57c70")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "184e5a97-2c02-4285-b306-f37ef75109c3")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0dfb57c8-d0bc-4b29-b692-d4b604c43a77")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce184b7f-f146-4e39-a619-d851e92d6c2c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5919dfab-2d52-48f4-a2ee-1ebb395e671d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6c247847-2b93-4d30-a882-0909ba3b0c0f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/电源/RESET")
			(pintype "passive")
			(uuid "4add2953-5716-41d7-8647-1f7991c0a860")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fc50b9be-8a36-4291-926e-8bdadc6fadad")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal"
		(layer "F.Cu")
		(uuid "c6704c66-1a74-43e3-82e7-d5116901d4bf")
		(at 192.425 106.68 90)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "J1"
			(at 0 -5.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "457a241f-64a6-42f6-867b-261883133b11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 6.32 5.075 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "52fcc777-1b4f-48d4-ba0f-3b4171bea7c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ddb95212-ae4d-455c-923e-47def69eeef1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "50d9f3a7-10d0-42af-92c4-e820955980e6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/7d145b7b-52f9-47c6-b9c0-54f63d8968a0")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start 4.67 -0.1)
			(end 4.67 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e2d8e57-959e-4174-8658-b439c8eea9cd")
		)
		(fp_line
			(start -4.67 -0.1)
			(end -4.67 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3207bbc6-47bf-4fbe-81bf-45985ba792db")
		)
		(fp_line
			(start 5 3.675)
			(end -5 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "c9d1f351-c967-45aa-a8a7-a15feea829dd")
		)
		(fp_rect
			(start -5.32 -4.76)
			(end 5.32 4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "eb02a215-9178-4c12-b641-5901fa1d15e7")
		)
		(fp_rect
			(start -4.47 -3.675)
			(end 4.47 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "9808517f-1c49-4611-91f7-a5a7f496e19e")
		)
		(fp_text user "PCB Edge"
			(at 0 3.1 90)
			(unlocked yes)
			(layer "Dwgs.User")
			(uuid "3f974f89-6938-42ba-9eb0-527d94af8b7d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "20cabd7e-e17a-4165-a121-d01f301c3b82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "f88c3f39-c3fd-45e0-a895-0f6e980e3377")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "2624dafb-cb01-46cf-b0f9-286c3f11935d")
		)
		(pad "A1" smd roundrect
			(at -3.2 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "0f775f5f-efd4-4eaf-ba04-c6bed5cb272b")
		)
		(pad "A4" smd roundrect
			(at -2.4 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "73afe56d-5bfa-4ac7-8d3c-684b97058554")
		)
		(pad "A5" smd roundrect
			(at -1.25 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/电源/CC2")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(uuid "a46933e5-73c4-40f0-b9bf-2a7542d669f0")
		)
		(pad "A6" smd roundrect
			(at -0.25 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "DEBUG_DP")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "aa25a740-a2bb-4411-a2fe-779562be47c3")
		)
		(pad "A7" smd roundrect
			(at 0.25 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "DEBUG_DN")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "e8070065-104c-45bb-905b-ede915ce20e0")
		)
		(pad "A8" smd roundrect
			(at 1.25 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(uuid "d7baa584-d7d7-4f9a-b01c-7768bff7add6")
		)
		(pad "A9" smd roundrect
			(at 2.4 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "a7858261-324a-48b7-a9d9-22257a9f0022")
		)
		(pad "A12" smd roundrect
			(at 3.2 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "4575deb6-3081-4106-b95f-22ab17f654ac")
		)
		(pad "B1" smd roundrect
			(at 3.2 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "49c84b3f-4a26-4767-9b8f-79a4bd943e01")
		)
		(pad "B4" smd roundrect
			(at 2.4 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "b231ee9e-ee5d-4c08-a398-15e8dfd886ad")
		)
		(pad "B5" smd roundrect
			(at 1.75 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/电源/CC1")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(uuid "152d61db-58c0-4d59-bfbf-8b39268d3af2")
		)
		(pad "B6" smd roundrect
			(at 0.75 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "USB-DP")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "60fc0cc0-1922-4088-91a8-22f3b0c332b9")
		)
		(pad "B7" smd roundrect
			(at -0.75 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "USB-DM")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "e6be33a9-4869-4147-9716-4fffe689af6c")
		)
		(pad "B8" smd roundrect
			(at -1.75 -3.68 90)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(uuid "0372168d-9002-44af-8916-e7b3d7f2b38c")
		)
		(pad "B9" smd roundrect
			(at -2.4 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "81ad3e61-280f-4171-ac56-28033357dc91")
		)
		(pad "B12" smd roundrect
			(at -3.2 -3.68 90)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "33f8f9dc-59bd-47fc-a0e5-ed8cb3c2192e")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.105 90)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "8864b97e-393e-4ab1-9088-33bc97eeee97")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075 90)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "04ec2fb2-6a59-4de7-a92b-d1a75a05cf32")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.105 90)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "d6c149b7-d6b8-4214-affa-33295b075d58")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075 90)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "dde8aa6c-1e4e-489a-9f6b-1b4da8235ff7")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "c6c70a03-56e8-43cd-bceb-feb9d4542896")
		(at 72.77 124.69)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "4e0b7d0d-5fa7-4249-b7bd-6d40dadd6307")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5b4befae-61ff-4ea2-aed4-d0b8f56db1e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "73bc4ffe-1077-4378-90c1-848741660e00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6124a9eb-c11b-49da-83b5-0f09442e509d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/56321573-e7f7-43fc-aa6e-7a5a18bd8de2")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fe049ee-2b79-42a3-a235-1a17a332cff6")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9d319a9-dc60-4695-8158-f35c30d3f93d")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8aed873-41c5-45ea-8f53-a2862e4d634d")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "102e6bd7-8e4b-4e06-868b-8959704e718d")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7a90e4f-4aea-4474-a2cf-a8746acdb08a")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4df221b-f3f8-4d36-9567-447ef2e879b5")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0c52e8b-4b07-4788-b718-1594768a3360")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1f56a22-d1d8-4de3-aa1c-ebfdb66d2b25")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e897016-463f-4f0a-a1b0-876a5c69dab2")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "247a2504-b1a6-4ac1-ac15-f4d21c15cf6c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3d1b2173-9b8e-433c-9d47-5d0213df895e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "c708686b-01fe-4e0a-95fe-b4f93d3ebf84")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/网口/BT_RST_N")
			(pintype "passive")
			(uuid "c92b659e-4f66-4a90-9db6-8e2a989ed70c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(uuid "c81c0a10-7698-4724-86c1-cf8f292f4d7a")
		(at 153.8625 62)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U5"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "e964fcd4-b815-43d8-bc81-cdd05dccc6d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "XC6206PxxxMR"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "5713094d-e236-4065-b132-7b408ad2aa86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d613646-6372-4b9d-adf2-4b6beb2539ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Positive 60-250mA Low Dropout Regulator, Fixed Output, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ba6036b-808b-4fb6-94cb-b1c09e478d89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23?3*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/c5ee6bf8-8c94-48ba-8d83-3719fbe32326")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e344564-3399-401e-b47f-ad7884916cb1")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53fb1931-5336-4f5c-8a11-4af4674a88fc")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d10654b2-61ce-4137-8ea6-32a33746c820")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5193a2c-7e3f-42cf-a0bd-d357fc79c2db")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84) (xy -1.3 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "2293ae17-63df-4410-8a87-7957b2b85fea")
		)
		(fp_line
			(start -2.05 -1.7)
			(end -2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5b79f9a-26ec-4c7c-ba71-8aaef5dd5afc")
		)
		(fp_line
			(start -2.05 1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ee1624d-d9e5-4703-9723-4fa5d0bc2a18")
		)
		(fp_line
			(start 2.05 -1.7)
			(end -2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "054d1970-1cc7-49f6-8e36-1339dd3d9cd8")
		)
		(fp_line
			(start 2.05 1.7)
			(end 2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27569d13-cc2b-4d9c-9f18-c807fa0cac72")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5537af27-429d-4bbe-b9e7-cc13e8402d6e")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2483a19-6f0c-4cf5-8b8d-b1345775d0f8")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8af31dfe-0ca4-4ce5-bb07-ce498cb98ff2")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c368d89f-cb82-455b-a867-5afe4ab0a8d6")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff26e84e-fc13-4c65-8b28-3e20ea5ca961")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c427df4a-d59d-4920-9b8c-c293f559f7fa")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ce468707-ea5c-4e9f-9317-5d0b9ea0c55b")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "2c88d21a-d0c4-486d-a400-52c227d33f52")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "7ff34dc1-3c54-4f76-a56f-34710b310595")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "cb039300-b19f-4b0c-9e89-1247c37e1aeb")
		(at 63.47 55.43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "ef198942-724e-4fec-9811-3c81fbafefa4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "f82ab5f0-681c-417d-a5b1-ec69d5cfd60f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fff08287-3734-43ae-81e6-674c824921b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8311b0f4-5966-457d-b97d-346e2611a571")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/80919f9c-bf71-4e68-b359-7922bb81497a")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bd26d6a-d6ad-4d39-bc99-c00b07be0617")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a45c302c-5bdd-4055-9785-2168d497c542")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "523b3739-1fed-4dcf-90cd-66cbaafe6fc3")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "622c3254-ffe5-47ff-82cd-3f01e3cae659")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e8dc248-6673-413a-bcca-f04a28bb0fea")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a848b6ae-01d0-476c-8251-762c534a72e4")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6a86c98-5e3e-40c2-bbb8-c5a2b3368a19")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65ea2f25-8846-41aa-9f1f-36ac065782b7")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63525990-e8af-431a-b69d-3e20d1c41af4")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55ba984d-7180-40db-b0ec-d6baec81cd3f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "260b95f3-56d9-4138-b353-abf949521049")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "77fd362a-e4e2-455f-a9ac-0fe507a1f307")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "49ee3d83-5401-4120-9b29-e0b1f6675dec")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(uuid "cc0c384a-6193-4342-afd6-b348d7c40c93")
		(at 87.57 86.89)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "ec0d372c-10ee-4f29-88e3-85356bcd5d8c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "d2cd50f8-fe32-45db-92a2-4705dcf28cf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4aa5041-e665-4f8e-ba10-cec0e56edfad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0cab163a-e7ef-41e7-83a7-bf2042ebe5b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5be9617a-8456-4119-adaf-f0bbf9797e39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/22eb1444-527f-42fb-b784-750c299215ff")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.485 -0.735)
			(end -1.485 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8531f2b-6ec5-481e-85c0-04f2e21bd7d3")
		)
		(fp_line
			(start -1.485 0.735)
			(end 0.8 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b445d9a-2fed-4fab-ad81-b4704087d22d")
		)
		(fp_line
			(start 0.8 -0.735)
			(end -1.485 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed02daa8-dad3-48c2-bdd9-bce67d02c084")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23a3be23-9111-498d-9953-492fc748d3c6")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63aab101-582a-4e68-93b7-85f893f6cf7e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5461c41e-0ca7-4b89-9e2c-b3a4ed1375b0")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30a73cba-cb39-4bcd-9dca-7abb98db5596")
		)
		(fp_line
			(start -0.8 -0.1)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c02a869a-300b-4105-b8a6-923acfd523bf")
		)
		(fp_line
			(start -0.8 0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbe5cda0-a00d-449e-956c-68b30c687baf")
		)
		(fp_line
			(start -0.5 -0.4)
			(end -0.8 -0.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9eaed8b8-9bb3-40ed-aa94-16d92cbb701f")
		)
		(fp_line
			(start 0.8 -0.4)
			(end -0.5 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5748a743-9b82-4c89-be0f-855caf3ac273")
		)
		(fp_line
			(start 0.8 0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad440ebd-7717-48cd-93e2-3c3316d7858a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fbcffcea-2c5b-4c74-b4de-c3c53d803022")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "b096429a-ecee-4082-9b37-7d9a53d6d1b6")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "a3360f91-c1d8-432e-9e02-84385b9773fc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "cc2b6386-88c3-49d9-9878-28754d203d14")
		(at 98.685 124.51)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "3b341fb5-de8a-4cfa-9d6b-7d85683d9a5f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "317cf0bc-27ef-4b3b-be37-1e448b099b8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "349b2e55-0f24-4d27-ab6d-79f1a8bc05d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2016fa6b-1ddc-4095-9858-813c7c928cf8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aaaf3f24-1f7c-48e4-abd7-3efcb84c2d78/d98ef928-46d4-40b3-96ad-c598161d19df")
		(sheetname "/主控/")
		(sheetfile "MCU.kicad_sch")
		(attr smd dnp)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dda82e97-d441-48e1-85ee-bfe443b0ad93")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4eb2aeb4-e820-4c47-9e6b-dc21623f686e")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d93abb1c-77e3-4d92-92ff-428464d82080")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03d2fc02-939f-45d2-9323-1939568e6f82")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "502ad1be-edc6-484c-aea3-ad046cad4285")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89f90b57-d509-422a-be3d-86eefa2d5e8e")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "740f9d6f-1bed-4108-842a-0c04e4cee3cf")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ead46829-5bcc-4c35-9379-35f149676b85")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41fd508b-015a-49ec-be17-d6e37d3d258d")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3b3b8a6-69ea-4fc6-982e-72424739c2f9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4dc0e61b-8ae8-40ef-8ae3-ec6b8c3b40b3")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "7f0d8b89-1e7f-4add-8b00-900999ceeb3a")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "PE22{slash}CSI_SDA{slash}TWI1_SDA{slash}UART1_RX")
			(pintype "passive")
			(uuid "a52d0e81-1f9a-4835-8c35-f3b474abaec9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "cee139a1-32b7-44c7-876f-06a96645c1d2")
		(at 83.52 70.49)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "573a4ef4-9df4-40b0-9f1e-276f81625c84")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "7ee5c099-41c0-4390-a699-e807df42159e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26dd8f43-6466-4b7c-9daa-551255239b90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "46a3f5af-c9bf-4811-908b-448eda9cd725")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/1146d466-8c15-4f00-ab3b-f80b29c48968")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c6937b3-ef5e-4fb3-8d1e-ba100b654edb")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7dc193b2-d2fc-4d20-86bf-a42c742d0266")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5514c28-04aa-40ca-aeda-7047d24c1d60")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f710d3d-efdf-415a-b0c6-7b74a2caf6c1")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c92c792-fc71-4c0d-9c74-5cabe521080b")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58bae0de-55aa-4170-a991-7d10e79656a3")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca811894-9ec3-49f5-9ca7-f9748bbd431a")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2a835e9-b952-443e-831a-7ea80f1dc1ce")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4187d18a-4b89-4bd8-93b6-747138650558")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c81354f-85ab-428c-af39-87ce81e5a434")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2bed362f-d881-4d4d-9ba8-c2fd7f31e03d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "SVREF")
			(pintype "passive")
			(uuid "0ab820d6-d411-4884-b68c-6b1273ab4a3c")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c9856dc8-53fa-4d39-be71-a5dd2b763139")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "d04b9da4-0e6b-40ce-a676-2987dce3ae55")
		(at 75.5 62.96)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "3ba0b3fe-d4e3-4971-b0b1-7db3b2611e5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "392fcd72-8b4c-4b26-b95d-9bdd367427c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bac1bd34-2e14-48af-879c-efaea44646a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "76b4d3ba-ede2-4e9c-a5ae-a2d415a43d01")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/762fe321-5450-4c22-914a-c479d434b033")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "228c3630-3b97-4199-bfcf-b253b1fe9cb2")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ad6c004-76cb-4ff2-90e6-b41486be6a8b")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30d86459-f9a8-4b81-8002-3bcc97b6b2e2")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20a19303-2a23-49b8-9785-45e37adaff5c")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ef2f407-8db8-41f7-b0bf-8808dc20ebed")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2fce3c70-d26b-46d8-82bc-4ab0828e3220")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "876cee54-7ce5-4191-ba7f-c4d7e325299b")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ac23074-cc97-42a9-aef9-b91f5d57d9a5")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de4d6f7c-1b18-46da-b5b2-4b08e2ad5fdf")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2449ec0-38ba-45fa-8128-5358ef4b3d2b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "618ce557-b5d4-436e-b770-25d4ac4b2af0")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "HP_VCCBP")
			(pintype "passive")
			(uuid "c9a779f9-0bc3-4fbb-ba99-6d1a89bfd170")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "34f8ccbc-7228-4dd2-89a1-c0cee0dd01e6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "d3660163-d2c7-4470-90c0-04a3a623ae0c")
		(at 71.49 80.53)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "6847958c-b8b2-4084-bed4-eb5c24fd35d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b1d56b20-19f3-420a-befb-ee9ec7e9f6f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06c17770-a910-4bfb-8333-1a562980348b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4723ba8-ba76-4371-9e33-2dc847be8b4a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/9e284ded-7be3-4ff7-a620-ea5407fabafe")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69fdb4aa-e87c-4128-9073-f94d3a0df35a")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95430f9f-e804-4427-a51e-0b2689ce4865")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aad4e615-8b26-4d42-a837-3904a8637b3f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e96fc30-3a73-4ed7-951a-9db5ff579bc0")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a4a109b-bf88-4c96-8088-8256663522ac")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83503724-da6c-4153-b21b-80586ba623bd")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f655296-6f98-4cd1-ab10-fe7030600bd9")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f33f0df9-2198-40d9-9e2a-3672241ae18e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ef0a8ec-2482-4460-9e49-be57a727e844")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67fddf94-6add-4ab1-a89b-2086a24d35c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9bd19d51-1a4c-4799-bca3-f75268e3f5e5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "f31903e5-0af9-4fda-905f-cfe9dfe81b44")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9212e851-53af-4f67-850d-e2525da4cbaa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "d3853ac4-23fe-4102-a931-8cdae4c23a78")
		(at 88 116)
		(descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x03 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.77 0)
			(layer "F.SilkS")
			(uuid "4792c876-1991-42ba-8f96-f2ebce9ddde9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x03"
			(at 0 7.85 0)
			(layer "F.Fab")
			(uuid "463fc6d7-06d6-4306-8e1f-553f8718dbe0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b56507e2-87ef-4ad2-a5a5-531abc0e79b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec51f2f5-25e4-42e7-8650-85df7bc0813e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/bd45533a-bb41-4498-93a2-e6a98ad47a53/0c411330-6d05-4d37-952e-d4004a4b3422")
		(sheetname "/通讯/")
		(sheetfile "Com.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5add2315-49a3-47d3-b13a-c4b120d0d228")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cb80aa3-2e24-458b-a9cc-2c271f276823")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae83937b-3e5b-4c51-865a-d1b2559ae451")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61afc23d-27e9-4e14-9b40-acb890d43954")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cb5c882-77dd-496e-b072-6625c7f06684")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8145a01a-1e8f-4f63-a728-30bdab471bdf")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56396ddb-1034-4dc1-b78c-79ebe5ffb192")
		)
		(fp_line
			(start -1.8 6.85)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "669f6c14-e3d9-4675-8174-cbbb838b9ef0")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c16c9ee5-3b41-454d-a0ee-d26c089047c7")
		)
		(fp_line
			(start 1.75 6.85)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e83a1214-513e-4b0b-b61c-541a28ae292d")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cb5c94e-6017-48d0-923f-b566bf4bd6b2")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddb97f29-8551-4278-96e2-82930bcd998b")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "664394d4-b4f4-4ba7-b9b7-ad49b5727e4f")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "233c7053-bfaa-4240-94b4-fe87cdad137c")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92ec61df-9f49-4d9b-b913-91c318b8ec1c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "1c4f6ef9-b460-4f3d-8b77-36c2d4f132f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0047bea2-51c9-4d81-95fc-306cd45d6458")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "PB0{slash}UART2_TX{slash}PB_EINT0")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "997b34e1-b884-43d9-9cd9-48b945bd322f")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "PB1{slash}UART2_RX{slash}PB_EINT1")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "596c733e-ffe1-4888-8a9b-c36dc845d978")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "d3cd6af2-67f8-4149-8163-1c133bbffb3d")
		(at 63.47 57.94)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "1af9b693-be6b-4e7a-94b9-f7d00a170507")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "065659bc-c410-476c-917c-e6ec4dcd97c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c1fb4e66-ffec-453c-8482-a57d33956cdd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "316d1375-7874-4680-9fe1-1f9136fa2653")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/1bea95bb-5ad0-44e4-a158-5c92509c7d66")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0b7070fb-52e4-4368-808e-0c90b43f808e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b76b461c-62f1-415e-bafd-46299739e049")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ae47dcd-fe25-48d9-9dea-0e175a9a58dd")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbc13f81-09a5-4a6e-a66e-fa9eb5238b6f")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f7500ad-f441-4bca-85d4-52c1947ed0ba")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf668e52-9405-4a6f-a80d-b5c09c52e4cc")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce4fec68-f5d4-438a-bde2-e80efa03c08a")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18c80c5e-fdc8-42d9-ab2a-47660d3562e7")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b48ff82a-13b8-4c09-b001-ba45fe5aecad")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e2af3bd-6ab0-44ce-822e-fa5f8acc263e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2e0697e2-df94-4a2d-ac58-58a635c64d2b")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "108cb282-9523-4915-864c-0154d2d87b8d")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ad079393-86b3-4dd8-abd6-1371a0a106d8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "d890f74a-0a09-4aa1-9cf4-853b018969dc")
		(at 79.51 57.94)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "411f9b77-8687-4f97-a13e-463245295195")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "b122ad1f-417d-4bca-bbd9-4277696cc389")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "864d6686-2ad6-46d5-a00e-f851d6abeab3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac76d309-00f0-49ec-be87-17cd2adc1131")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/ec540279-9245-4dcb-a464-d4e00ed50626")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5513b450-3971-497a-b0d5-bcaf003b5ffe")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f31ec629-117e-49c6-b478-f779f2b056a2")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79f8f7af-ac33-425b-b898-dee9cf1bd429")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e523a8f-934e-4fa0-a57d-f2250237184e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88e9472f-22fa-41d7-a707-4e8622822baf")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "adcb4e85-502d-4047-8d34-55affe1318a9")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "def1c403-eb90-4dea-8b34-18fd71463f79")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "128bdb4d-a09b-4c57-bc61-a359714d6184")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd735372-baed-4bef-9a43-bbeec5c62b9b")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8810779-f0e0-4abb-bef3-4a89b6dbb2c4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d8d666b8-15fa-4a5d-baa6-b83b2d9c925d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f4beda9b-c65a-4102-96cc-7b1d6c905b3b")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/电源/X24MOUT")
			(pintype "passive")
			(uuid "697f926c-5a88-48ce-9896-1bae91b0af5f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "dd2df91a-db62-43bd-9618-ba0231786d70")
		(at 71.49 78.02)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "b5f44085-6531-4a07-aec2-dde6d0b82716")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "0dd99a74-ce56-451c-8f4e-a0bb466d01ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec2995b7-e412-44cf-9892-ec2a550fed00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1b3a7a0d-87ea-432d-99cf-2dac6c0d3e73")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/bb1869f7-b789-4d7d-adae-0935cc3a116e")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3195026c-7414-4116-9b07-8c09d47a0e4f")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "685a107a-a8e4-448c-a739-46441c4f2ee1")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ead3ecb-a42c-41cc-a009-d539152ce721")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb92ef3f-4ca5-4775-90f8-634397c15445")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc43477d-3b45-4d79-aa99-faa8baca8efa")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd2e682a-115f-4b7b-9cf7-cdbf6b4c0cff")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "010e611f-902e-4f2e-81c6-d80479251c21")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ddc80ab-50e6-4444-809a-c3d16cbb0c4c")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9afdea0-1357-478e-85cf-3b53879e5099")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b75046c-1912-4702-aa58-25135f2d6558")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "186ce070-6a99-490b-8251-007e2607ea13")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "4fe3413d-84af-45f7-90db-5a981722967f")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "216ebd78-5b3f-4e4a-a751-7905d3610141")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "dd6ea904-5a50-42e4-8056-3769cfcda40c")
		(at 87.75 69.75)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP4"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "5fe88fde-53bf-42e1-8aa7-aa339e27c308")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3V3"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "1994e8f1-7b75-4ac4-9ccd-58b25c809568")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f1c7cc33-f589-4a77-875c-8209df723f7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d965a044-006f-45d9-9280-f251313646c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f0ec5a1d-61ee-440f-ade6-e0d44055080f")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "79a9d93a-9329-4023-b922-4dc8c70a196e")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a0947e9d-ca13-4643-b223-5496fd78e41f")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "549667b2-a695-49a4-92d1-7f31468e8a62")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5b4e90e5-41c1-4a26-93aa-c3d4a3713e67")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "614b9c99-3c7e-43c2-adc1-01c0e313a856")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "03debf0c-3bf2-4804-8f7f-25a5c63797a6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "dd8b4de4-cd41-4890-8d7c-addd8c8125cc")
		(at 79.51 62.96)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "045f3eb4-7df5-4ed3-9de9-402d0d43b70c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "6pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "31abb79a-4432-40a6-82df-59a166c2642e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "30e00149-94f6-4019-942f-81f8a7b5157f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "215ea862-cca5-4dda-ac04-2d2175122810")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/7a9caf89-c5ec-4c5a-8819-4d3c30bcf0ac")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a17f3e14-6146-41f4-b549-c3634c613eae")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "640d86eb-7022-443d-a6d3-825a80ffa92b")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07dfc96a-2867-42a6-b9ad-afb6d92d8916")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd941315-328f-4840-a8ce-f53a077667af")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f376f392-eb78-4532-a321-d5f59db37bdd")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d191144c-d713-49a4-b49c-071f1bc3e26f")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "387e585a-1c6e-4e43-b0cf-f6d6ff140cb9")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3ec34a5-87d8-4601-858f-3b96e128b28e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7944ac79-122c-418b-8f54-1fb7ccf6dd0c")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e2738d6-830f-4dbe-9440-53783f66da5c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d684d45d-7473-4d87-95aa-923a6493c1a3")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/电源/X32KIN")
			(pintype "passive")
			(uuid "7a6ba174-27ce-452a-801a-d99517fbdbc6")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c1e7cffc-8e7a-456d-93d3-bf8dc89704ca")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "e0dbd637-7090-4f98-9e88-170675ee1951")
		(at 64.75 119.67)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "2ff5cee3-bcc0-477e-b9eb-d59ebec26ff2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "bc03e234-8470-4419-8342-e86c0180049d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c64ca69a-d19d-4388-a231-7e673611d5de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "082f80c6-8aed-4bce-b4af-ec7d966ef623")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/184c6ef4-8e97-4f28-ae0c-8ad501192545")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b481159-26dd-4116-becf-c604f9940904")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56ca95c0-e5b2-45e2-a800-32c3fae0d9bb")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10d3a3cd-4392-43c0-a41d-51407ed87612")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8e4d1d5-81de-4749-a599-3e2039181e61")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd37d1c2-0787-4af2-bc2e-42d623227c9e")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1de4ff4f-a2d9-4d13-9cb6-a94672701e06")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5aff6b5-b610-4a7f-8bfa-38b6c9a1ed6b")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f2c9181-0336-4776-913d-d2a6f30a5222")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35d08372-cb63-4e8a-b544-1c9830a744eb")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac263ffc-63eb-4c9c-9eff-d5a27b6b7924")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f3c8d7b1-c391-4047-8e3f-237d1c5b78c9")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "8a0c8b45-d54b-424e-b5ac-62da5faac978")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6706a8e0-489d-4272-80f4-dd5e6a9050ef")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "e343e511-cace-483a-b2f9-73fd76e47136")
		(at 68.76 109.63)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C63"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f70e975e-e74f-4c45-88aa-2aaf36ea5725")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3a910816-59ee-4f88-889b-59137bd8a4c0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3284b77f-fd2f-4376-a85e-85046366c572")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "806d2e44-c168-4a20-b764-f6ed55947e85")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/df7d770c-818c-4b27-9cc5-386044bed85a")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a1aefab-ac5c-40a8-acef-243c9da3d27a")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2a72f7a-1548-4c7f-8408-dfed200a08b7")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d0fc209-cdc0-4350-b757-c848c5fbb2cd")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "253510d0-9958-45bb-a125-2a561bf8e4b8")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "763232e8-fb52-4af5-a704-e3a433aa3ee3")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "366cef33-add8-4d14-b329-6e8e163f9266")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69e2bf3a-9912-4f6d-b290-0d798aa3564c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8f259b3-9c92-472f-98e7-83b8634ca529")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "392e2dfa-9083-4867-86b4-06f2daa1a4a3")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7a2d746-89a4-4ecd-8902-4d467723948b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "88d2fe0a-2d9f-421b-9ff0-dcd82580095c")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "c8560615-5f8c-464a-a7d1-0cb3680b1e1d")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "80fc0dbd-f1ff-45fb-90f8-15da670ea2d5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "e83b02eb-6b7c-49cd-997c-dce9cbbf680b")
		(at 75.5 78.02)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "1aa12d33-211f-4b83-9584-5aff740e69cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "e83ce5cd-5986-4785-a27a-92c75bc963a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1bf33675-7f32-4005-af41-4c38c4d4ef7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8bb15b34-96d4-4fe2-a3a5-45e358cd6aba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/b60410f4-ff4f-42b4-9c0b-f0db55cb0d86")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f372c41-1422-45ad-8e76-aa9eefc0c357")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbe7e7cc-0852-4757-b37b-067396ea2797")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ebd98f2b-6243-42a1-aedb-48a1dbef21db")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99f7d197-a9ce-4257-854b-dfdcfcae1877")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "502d4872-cd30-45b3-8819-d7d634bd8f24")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24b1242a-7bb2-4604-a51a-cd6300967dee")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe3cbf66-0c06-497e-b183-4307d2e86f28")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c3812f3-d0ef-4331-8658-20a038b63063")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abd1499a-b386-4a50-93e1-be60a41c8615")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebd24961-27be-4335-8fa7-f8c2f7d6c830")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cabf217e-39a2-4483-ae73-9c69086de448")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+3V0")
			(pintype "passive")
			(uuid "a281f409-ca59-40de-9384-ccebf986bfc0")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "GNDA")
			(pintype "passive")
			(uuid "16584474-a248-4839-a488-e581476b5aca")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "ecfb3153-c380-4620-ab49-9afbd81f44ef")
		(at 83.52 67.98)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a596e449-bd8f-4adc-a1ab-b6ab7de21400")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "91de068d-edbc-4b9d-8c1d-bac9c0233578")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2003737-3d01-4f9e-ab05-49ea0c30e0a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c257ca05-75b2-42bb-9a18-6c715fa44c9c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/3c8a2656-9ada-4fdf-af0a-f61e29301499")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fdecbb0c-3c4a-4580-a263-9cd419e7cc69")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "633eaec7-c3a6-49b3-b245-8453b6e6effc")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78e0ee5b-e526-4634-a8da-243d6b0f1ef7")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6f49c1b-255b-40af-9945-6e61dc8508cb")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "84356ecc-3869-463c-9e03-dfa32c8f3fec")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b75a1de-e17a-4c70-9ed3-e38d09b0a0fb")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b03c3b41-ff33-4ebe-b39a-37a36b652440")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6ea9149-7746-4b82-8ef8-2c97e67d6e5c")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddbf2a0e-5053-4e7a-859a-777835cb8fc2")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be4bc45c-c0f7-4b8a-955a-a58b98a1a059")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8606df4d-3304-435b-bd2a-a4d0dbefafc5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "5fa3f5c2-de88-461d-8516-2288b016f2eb")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "SVREF")
			(pintype "passive")
			(uuid "a6532432-3390-44af-a19f-1da43432089e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "edf6a13c-c37a-4126-bdfd-ea96a7521791")
		(at 72.77 122.18)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "647cd9a4-22d1-424b-88f6-21232961eb43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9469fae8-436c-47dc-a963-2715fd8214b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e40b4b9-415f-49a5-9c48-d6004fcd8cb9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c728ab79-e912-4856-9d28-98875fec0794")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/f60c1cc0-981e-48a3-8f5d-ead17bcbf066")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f47b5f0-f82d-4552-98a3-91e6c9a6d938")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1043bf9e-48e1-4915-8ebc-8b7a05ec4e31")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "940530a9-a8c0-4b74-bac2-ac4c255b8155")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54c47ca8-ec44-4557-8d8f-128059e7db34")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b7cb40b-0bbf-460d-ab01-650d27bdbc1b")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "168fff40-f7e2-437b-8252-00c389819c0c")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae5b04c6-e289-4c3f-be14-0b363595360c")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f3d8602-953f-4fc3-b226-4a41072194a6")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "501efa66-a902-403a-8ac6-912fba3e09d7")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c9a4ae5-f9a3-43c6-9779-57ed111c87f1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b3897deb-f2db-4b5b-b2fc-4fa6698d4241")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/网口/VIN_LDO_OUT")
			(pintype "passive")
			(uuid "9b0ca0f5-3a54-4fd2-b6d3-01fa19ec8c4c")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "97fb3261-6c06-4121-b2cd-6cc9071cdb8f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "ef1e8b44-399a-4277-aad2-c818dd5e395b")
		(at 81.45 110.6)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP10"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "2f7ca2e5-6aa4-4015-9814-9e5b7d99bf16")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BT_UART_TXD"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "9acfa698-d34b-451e-8cfc-1336ae0d8236")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "40508e7a-c615-433c-85c6-dce4de277f7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd106a84-0686-4075-bd75-49496b616366")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/4b54c9dd-f489-48ac-b31b-649042c6226f")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "2657f517-ce1d-43a0-bcc5-24e4a95e43b0")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "bbb66f9f-104f-4486-81be-213cdaca9b95")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8dbf5061-ee1e-43d0-b09c-8f0700556665")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "202135a9-8595-46f6-a738-358921ec9e39")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "28ead311-362d-4624-abed-999bef47f32e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "/网口/UART_TXD")
			(pinfunction "1")
			(pintype "passive")
			(uuid "3d2eb948-bd62-44fc-9dcf-bb31a6b4672a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "ef235ab5-15d2-4c6d-b719-61c428a129b3")
		(at 71.49 65.47)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a55db3fe-f8c4-4427-8636-69e0c173dd0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "cabc98c8-a46c-40a4-a1e4-40f46152d466")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e72c50c-bb9e-4f77-9ecb-d1c70817b5fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "85793161-6137-4c47-99c0-39f355cdd8a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/7efb3f01-f73f-46d0-acaa-60649652aeca")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ab4b034-1281-4c14-9745-ce0307e59c2c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e00b80ca-eb6a-42ae-abfe-ddb335adacad")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bda7022-225c-4185-9597-31bec5e07e46")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58eb49b5-4204-4d67-9626-c2b9ca46bc7c")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df310774-2dde-4496-aeed-6ffe65d50775")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66efac02-4fad-491c-9523-7fe74ec78df7")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "963d0fcc-fd1f-48e0-a41d-ba6c2fe84f10")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1e0e502-9959-41a8-8efd-f0c2922c281c")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c136962-3ed6-4f79-897a-2ffea4c6d38a")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1589ede5-381d-4991-88db-da31ae38839a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "04e8da61-7004-4e98-971d-6946c7b741ac")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "3692ba57-192c-4b51-997b-311f8e41fbd0")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6448115b-d1ea-4001-9e15-051b16983ef8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "f11808df-97d6-44a3-b1e5-f5e3434495b0")
		(at 67.48 73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a687bc44-d731-45c7-9091-dcd7b419e91e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "85a53ee5-dfd6-4d01-8d12-6ada6a1bc245")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c99e55d-1e5f-40b6-a9bf-3ab9469df452")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af8825b0-b307-4ba1-bae2-0ecda9c1bf05")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/16ddc713-1f3f-4180-8a25-8112a44299c2")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "514726b5-cb47-404f-9f18-ed6b5993a78f")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7acb8c3-7b51-43ea-a3ce-2649aa7389e9")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55d7a817-b58d-4b8f-9516-00fffd8e11e0")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95a85c2b-64b6-467e-89f4-5b16f029cd09")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfd21bda-66c1-4973-9870-3cd7bf020329")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a936099c-64f8-46e5-a069-0168380e3200")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75e4315f-f07d-42dd-953d-fa9e719bfa2a")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49585b1d-52e4-4e6b-b668-a71be1122abf")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99a12a81-5c60-402d-a03c-60d04a9ac46a")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d4bbdc0-10cc-4f72-8434-fe42ea3170c0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0df55eb1-1b38-4bfb-906e-4cea1d4937d5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "+1V2")
			(pintype "passive")
			(uuid "e0eed4ff-3389-491f-9048-0df3e25c14d2")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d8555539-a558-4557-a334-8503272737d3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "f1e916ce-c22b-4941-bfac-38213c32a9bb")
		(at 63.47 65.47)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "59ba10b2-7a4a-42f7-9a97-d9e5998db1c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "f60ac4e1-c5a6-45e0-bbb9-1b22cbe35ee5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c82142d7-64c1-4c90-bc39-0652cf3999f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "79dc6208-4726-4ac5-bf2a-aea90e904a53")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/b9b85e83-61f6-4501-844a-58cf91d473e9")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02613d2d-84cf-47f5-8c48-9eefc2f7be8c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c585bf48-3128-487d-abd4-3d4e817f3f22")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e1ab3588-9465-45f6-8b78-da329a4a219f")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9a55497-6bea-45a7-af0c-b887d216c4e9")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f3962a4-6691-4896-95fa-68aaca55bc66")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7d57eef-fd2d-4560-81bb-ddcda18693e9")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f47c8036-13df-4273-b2b0-c3048fc1ac70")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e86df8c8-c769-4359-a80b-d35bc0c51175")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c00b0688-9708-481d-bc98-fb67ee853d91")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91f0c586-fee6-4e71-8d61-0a559f7cfd60")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e14fb98b-ba3f-40ee-8e8b-05840b5fa9c6")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "56cfc402-3a37-4eec-a4ad-c186bcff15c8")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "FB3")
			(pintype "passive")
			(uuid "494ea944-78a4-449a-8071-27dfb1ab3d6d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "f1fe1361-ce1b-4943-9002-68450fbeba51")
		(at 77 119.5)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP8"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "a63cbfe0-a618-43fe-be5f-8aabdccdbc71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BT_RST_N"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "bc105b43-96c7-4478-a778-eb06bf1935cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "541cbafa-7daa-4176-a9ed-dd503208af76")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "118040b8-df8e-4652-9565-ced381840046")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/fe310e55-02aa-4fcc-ae8b-d5f58e4d919b")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "15b1c1db-6de7-4c99-a915-fd2a96fda5b0")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "cbcb16ed-15fe-4126-b9ee-75cadfdcb5e7")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c7a02a58-4944-418a-8383-fa68747072da")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "faecbf05-7f89-4c9e-aa21-6b7dcb96241e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "fe6bd329-ba64-440b-a5d3-dd011e2b8250")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "/网口/BT_RST_N")
			(pinfunction "1")
			(pintype "passive")
			(uuid "156d8b16-c68d-4a17-bd41-8a234c450bb5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "f3d81f99-989b-46b6-affa-1e922ede5a47")
		(at 63.47 83.04)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "830adf16-2ed9-4e14-9faf-79a386d072e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "1ec0b72b-03f4-4c1f-ab14-94b8a058012e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94dcee12-8de6-4cd6-94df-a4aec12d9108")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "00c9b740-f087-4ce7-bb48-6e0a7564cd3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/deed9cfc-abc3-4071-bd86-43bec8dc7315")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdd1a49c-d10c-4ce8-b109-96a8725ea89e")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08693cbf-ba71-4ad6-b25a-cf35c5973407")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e11e8f9-df9c-4c87-a269-a8d56d44fe43")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "595eb5f1-4b50-4ac9-a248-a9fd49243853")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "352649aa-ad59-4931-974f-7fbd1279fd90")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d87d90e1-2e0b-47fb-8c47-2c0e6c8676d7")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc3b8040-a060-4b16-bc99-1e4ec0dfe5e6")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3afb6ac8-858e-4c5e-a5a3-687c04ac0db2")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a79a8d76-a1a9-45fd-8764-c4311afd4880")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8a3858a-95d0-451c-a4c3-4041f3ef2f7f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "89a7f13e-06bc-4d72-ba3f-ff7b9f681924")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "02b71cfd-fd67-4716-adaa-d30228da667a")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "55c4029f-c760-4227-b3b0-b407566257be")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "f7154beb-189a-4224-9b98-0e7cf50e14db")
		(at 68.76 112.14)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "b703bbd2-d9fb-4707-ba5a-d1b0b4afd55e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "15caed70-56d4-4c4e-af7d-7fd3da152fbe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c72eaa4-31bf-462e-8c34-ef1d55cad49f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eeedc168-a00d-4208-b3fb-2e89d3f1aab0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/7aa4e9d5-1d45-40e9-821e-b258b39a3630")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3012e851-96cb-4519-8fec-c0ce47b18fde")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ac95fb4-a3da-4876-aeaa-bba575dfe292")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e0d56e8-71bd-4a41-87e2-3d8a5fc43104")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e320867-0889-4b17-ba78-36a5b6a3c820")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7358c1a-55bb-4ad5-bd1b-791ab4cbb5d8")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "372379b3-9ec3-4381-9d7a-5b6e9e3fa1aa")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6803cd6b-92ad-4a10-9164-583cc2dfcdc0")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "583758fe-66d2-4746-9a87-9331a196b977")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1174d351-790e-4481-86a9-104fa6a444a2")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11798756-e629-4d5f-ab99-08f92100042c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "16a06111-08a6-4928-a63d-46e82443aaf0")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "EPHY-LINK-LED")
			(pintype "passive")
			(uuid "e5bc4b20-8fa6-42ae-8649-adaa27b5baf8")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "Net-(J3-Pad12)")
			(pintype "passive")
			(uuid "09b90a5f-f7bb-4137-8b81-f90d9e7654db")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_DS26_D2.0mm_L6.0mm_Horizontal"
		(layer "F.Cu")
		(uuid "f9d3cb44-0f48-4adc-809c-928db17ab0a6")
		(at 91.3 55.5)
		(descr "Crystal THT DS26 6.0mm length 2.0mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/DS-Series.pdf")
		(tags "['DS26']")
		(property "Reference" "Y2"
			(at -1.57 1.625 90)
			(layer "F.SilkS")
			(uuid "28026624-d90a-43d0-8826-90c8e4398005")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Crystal"
			(at 3.47 1.625 90)
			(layer "F.Fab")
			(uuid "a9c93a1e-cf39-43ec-89e4-1f8e558494e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e74a63af-0bc6-4a4f-9bc6-da9037fc38c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec9ee284-3116-42ec-a3e9-711007d63992")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Crystal*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/76f8641a-1dd2-4d25-a115-d62cc1024b4f")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.25 1.8)
			(end -0.25 8.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "407dd73e-6fc6-47d9-8826-b3e674c389dd")
		)
		(fp_line
			(start -0.25 8.2)
			(end 2.15 8.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a17d7468-4bfe-4025-bca2-6030a942d481")
		)
		(fp_line
			(start 0 0.9)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dcc9ac49-a7df-4ecf-8bf9-0b38db634b00")
		)
		(fp_line
			(start 0.6 1.8)
			(end 0 0.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "173ce995-8dac-44fc-8bfb-a851556c41b8")
		)
		(fp_line
			(start 1.3 1.8)
			(end 1.9 0.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c96a4ac0-84a8-4cdf-81cf-fc69a131251c")
		)
		(fp_line
			(start 1.9 0.9)
			(end 1.9 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8de7f797-9a89-49c7-9715-11da8988ffed")
		)
		(fp_line
			(start 2.15 1.8)
			(end -0.25 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a85fb388-df36-4b19-a619-e716c6a1e621")
		)
		(fp_line
			(start 2.15 8.2)
			(end 2.15 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89083925-e8d9-4bcc-9c47-5d5bb18ea38f")
		)
		(fp_line
			(start -0.8 -0.8)
			(end -0.8 8.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59e7c67c-c233-4e82-9ec2-ac9134086b8a")
		)
		(fp_line
			(start -0.8 8.8)
			(end 2.7 8.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3d1a738e-f4a8-4d4c-8f7b-145c903147e9")
		)
		(fp_line
			(start 2.7 -0.8)
			(end -0.8 -0.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bdcdf025-1cd7-405d-975a-6e6a04c29a8e")
		)
		(fp_line
			(start 2.7 8.8)
			(end 2.7 -0.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c324905c-84b7-4c4f-82e9-bea9ffde29d0")
		)
		(fp_line
			(start -0.05 2)
			(end -0.05 8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f362442f-29a3-4f0c-be73-96344bb87ae1")
		)
		(fp_line
			(start -0.05 8)
			(end 1.95 8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8162bed-bcb7-4868-9273-325c129e9b28")
		)
		(fp_line
			(start 0 1)
			(end 0 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "422394fe-93b3-4760-98d0-c31a449df2e3")
		)
		(fp_line
			(start 0.6 2)
			(end 0 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "194c1cc2-a102-4be7-9872-d8ccf8cceba3")
		)
		(fp_line
			(start 1.3 2)
			(end 1.9 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "380b5028-cf49-4cc0-bc59-b6c2e041ba5b")
		)
		(fp_line
			(start 1.9 1)
			(end 1.9 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "498be8c6-f75c-4a81-85cd-ec9bd3ff9b0b")
		)
		(fp_line
			(start 1.95 2)
			(end -0.05 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84548c8f-cf67-43c7-86d7-3e4283b25519")
		)
		(fp_line
			(start 1.95 8)
			(end 1.95 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6119bdaa-e4db-4f5f-a0b4-62472899f3b4")
		)
		(fp_text user "${REFERENCE}"
			(at 1 4.75 90)
			(layer "F.Fab")
			(uuid "9fc6e346-38ab-4dbd-8222-e335abbdafed")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.105)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/电源/X32KOUT")
			(pinfunction "1")
			(pintype "passive")
			(uuid "b1a871af-4f59-45f5-8208-f1ee3e612668")
		)
		(pad "2" thru_hole circle
			(at 1.9 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/电源/X32KIN")
			(pinfunction "2")
			(pintype "passive")
			(uuid "c0eaf26f-c4f2-4e52-8dc7-84cb16d9bc37")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_DS26_D2.0mm_L6.0mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "faa7ac5f-f59f-4873-ae0b-bed9098a7993")
		(at 79.51 83.04)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "99fc8fe4-f0ca-4e8e-ad5a-a7b00600cc09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1K"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c7b12443-8ca4-4cfe-9027-45a14fd28c4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d2894f1-709d-44b0-9405-b5965e9e9cbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "21044edb-e9db-4416-96a9-a0ac473db35e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/e603887f-2bd2-4cc0-93f5-2eda6e1ca940")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5535b1ea-e036-472e-aa10-cfb4ca7a2847")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d1ca5aa-8795-4ef4-9c19-a9bc714b899f")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ba6983f-bf9f-4943-91ac-727b06c9140c")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c12e3cbc-9de4-43e6-80c5-6011380461f0")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b95ae206-965d-430e-8fb9-7ebffe0dd9d8")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "205fb557-cb49-4f02-880e-7777380ac7dd")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7632ef79-6d30-4f98-aae9-058d9a85020e")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0aa88c2f-18c4-4013-82a4-5b44969e488a")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ad359bc-ca60-4062-a5ae-03c056beccf0")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "613264a3-cc72-41e2-85e7-bb2d18e43064")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a6b764bb-d005-4b3b-82c1-cfccb3d80fb5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/电源/CC2")
			(pintype "passive")
			(uuid "07f69732-b01c-49ca-b741-ba95836710ed")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f828e6e1-8975-4f4e-8753-3ed441065aae")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "fad9c6f3-ce94-4c24-ab3f-3c7fea4ea14a")
		(at 68.76 119.67)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "0898f9ca-0f70-4b9e-9f10-bc398e1e9713")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "fde72eae-c77d-4537-83f6-419a3d5a9a6f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be50c214-ff70-4afb-bfe3-adc6711742d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f0ff135-38d9-4a40-89e2-c7dafad63593")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/1411ac11-e95f-49bd-9234-63adf48b399b")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9895faa-9968-482d-8570-8e0d694c61bc")
		)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05a1e8b6-0ff1-403a-aadf-c541d5b3a3c0")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eacb48da-0220-476f-a7c7-1abd3aa3a1cc")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "269baa84-16b5-4b23-a039-a9db20f7e9b6")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40108dbb-7fe5-4dec-bd47-67d3191397b9")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "527b3467-e043-4f12-9521-e997f63c3137")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bd2cfff-9c0d-41c1-8056-4af953fb83c1")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55eb0735-8cac-4335-b219-ae9902354f27")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2389470-9ee4-46a8-ae13-3e0a456bcbe9")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e786f91-815d-41b7-b883-75707a339a0c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a6841f3b-3c2f-4f5f-a115-69df6b2e53ce")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3V3")
			(pintype "passive")
			(uuid "a2f5a09a-b84a-4ead-96c5-9c907f0d1b71")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BT_3V3")
			(pintype "passive")
			(uuid "ac08b093-2ef5-46ec-af78-475beadfa992")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "fc3086c2-f266-4d31-841f-a074ae9067db")
		(at 71.49 73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "5066432b-879f-4786-b117-e22ba1a36b99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "0ae1797c-bbc9-4591-8949-8ee08785c90b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0de2669e-836a-48b9-bb4a-c1afbf70fbd9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0568be87-14da-4f53-81d7-436e6e7852f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/f36efce9-a8c3-4205-b676-2e5c89a0fa44")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39a23d5c-c30a-42e8-9be2-84794d116688")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c9b81ce-bfe9-41e4-a3eb-9be9344efd23")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d8f6ebd-605e-4aa0-b89a-20efde44d209")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c3d9535-3aea-47ce-a173-e582ee7a7de8")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52cbb3d6-2446-486e-8f89-d2864088e3e6")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16a3b475-d496-4227-994d-bf4c4ee2a4a1")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2008da30-5e4d-4b63-868b-2dc937b949ce")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c74e338-9731-46fc-b880-4e812c71de4e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84c624f8-5ae6-4a36-9bde-75b37eaa1dc9")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5e9b8b4-b161-4211-9b57-1d33e8a59c4a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c1f056bb-1107-4119-875b-7682c3eda482")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+1V8")
			(pintype "passive")
			(uuid "bd96b29e-a056-406c-bc1a-ec935e8ec3ff")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7070189e-bdb9-495a-b5f9-35cdba15cfb3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myPCB:TF-SMD_TF-PUSH"
		(layer "F.Cu")
		(uuid "fc7a8300-2898-483d-8f88-0fa6f572670a")
		(at 157 126.6365)
		(property "Reference" "J4"
			(at -0.096 -6.458 0)
			(layer "F.SilkS")
			(uuid "c4e3ed72-4bdc-447a-97b5-14a1ad778dc7")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify left)
			)
		)
		(property "Value" "Micro_SD_Card_Det1"
			(at -0.096 -8.236 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c935403f-b222-40f5-98ea-4e64f183497b")
			(effects
				(font
					(size 1.143 1.143)
					(thickness 0.152)
				)
				(justify left)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2110151630_XKB-Connectivity-XKTF-015-N_C381082.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e1feeb53-fab0-457c-bf73-802dfde00c08")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Micro SD Card Socket with one card detection pin"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "75e73be5-a32b-4bf7-a1e4-a1ddc9721aad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "microSD*")
		(path "/a471b1a2-6153-4f51-8850-6b912fdf34a0/94dab32c-94b2-4e50-ba46-994c3b77ff0f")
		(sheetname "/存储/")
		(sheetfile "storage .kicad_sch")
		(attr smd)
		(fp_line
			(start -7.26 -3.25)
			(end -7.26 3.91)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44326bca-e2b4-4fb8-bc82-b4982cc6f783")
		)
		(fp_line
			(start -7.24 9.7)
			(end -7.24 6.76)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e753c871-d65b-42eb-bdc1-fa59e1d98227")
		)
		(fp_line
			(start -7.24 9.7)
			(end 8 9.7)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64166ec7-7487-4fbe-836c-b3f3e0f1a8f8")
		)
		(fp_line
			(start 4.702 -5.3)
			(end 2.85 -5.3)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc9df490-72ab-4aa5-b0d9-a1cea5df1690")
		)
		(fp_line
			(start 4.702 -5.3)
			(end 5.489 -5.3)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e12c989-bb92-43cb-a39d-07a15bdeed6a")
		)
		(fp_line
			(start 5.489 -5.3)
			(end 5.489 -3.199)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3756bc3d-420a-4c02-bf9c-0e04483ffd04")
		)
		(fp_line
			(start 5.489 -3.199)
			(end 5.5 -3.2)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fc128fb-8fc5-4efc-b80b-b47f4ccb4df8")
		)
		(fp_line
			(start 7.98 -3.2)
			(end 5.49 -3.2)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b63763b-4b79-4655-8b33-535b9f526537")
		)
		(fp_line
			(start 7.98 3.969)
			(end 7.98 -3.2)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cd81e7d-8be0-4db6-bbae-2f9e0e6f9e4d")
		)
		(fp_line
			(start 8 9.7)
			(end 8 6.71)
			(stroke
				(width 0.254)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0fea9be7-694f-49c3-b76b-cb2d86254aa9")
		)
		(fp_circle
			(center 3.087 -4.552)
			(end 3.139 -4.552)
			(stroke
				(width 0.254)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "aa3dc0c8-8825-422d-a9d5-4639ceda8c0b")
		)
		(fp_circle
			(center -4.95 5.7)
			(end -4.75 5.7)
			(stroke
				(width 0.4)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "81640f70-e42f-4697-878a-ed4da9de6656")
		)
		(fp_circle
			(center 2.81 -5.63)
			(end 2.937 -5.63)
			(stroke
				(width 0.254)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "ac1655ff-a758-4185-8b20-417b3481964c")
		)
		(fp_circle
			(center 3.05 5.7)
			(end 3.25 5.7)
			(stroke
				(width 0.4)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "3b662c93-79cf-429b-99cb-618cf7449b27")
		)
		(fp_text user "gge5749e460e2332bdf"
			(at 0 0 0)
			(layer "Cmts.User")
			(uuid "58cb0e93-a138-4949-b8f4-dde8be2c562e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -4.95 5.7)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(uuid "95ffa77c-c7b3-4138-a0c0-d8cc2b610205")
		)
		(pad "" np_thru_hole circle
			(at 3.05 5.7)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(uuid "11e826e6-cbe6-49ab-ab0c-9f9342535866")
		)
		(pad "1" smd rect
			(at 2.25 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "PF5{slash}SDC0_D2{slash}JTAG_CK")
			(pinfunction "DAT2")
			(pintype "bidirectional")
			(uuid "61b63bf0-9ae3-40f2-a7bb-d1aed54decb7")
		)
		(pad "2" smd rect
			(at 1.15 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "PF4{slash}SDC0_D3{slash}UART0_RX")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
			(uuid "cc145e86-26d4-45bc-a383-ef37b36e76aa")
		)
		(pad "3" smd rect
			(at 0.05 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "PF3{slash}SDC0_CMD{slash}JTAG_DO")
			(pinfunction "CMD")
			(pintype "input")
			(uuid "38795010-4cd8-4142-86f5-ea0f743bd5a6")
		)
		(pad "4" smd rect
			(at -1.05 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "f0beeecf-1337-4113-a332-3f99c896c8da")
		)
		(pad "5" smd rect
			(at -2.15 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "PF2{slash}SDC0_CLK{slash}UART0_TX")
			(pinfunction "CLK")
			(pintype "input")
			(uuid "c9cc4bf8-1e2c-44c8-b57f-5a23ff40f945")
		)
		(pad "6" smd rect
			(at -3.25 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "5bb79429-4592-4cd0-aae5-4d21538c82d1")
		)
		(pad "7" smd rect
			(at -4.35 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "PF1{slash}SDC0_D0{slash}JTAG_DI")
			(pinfunction "DAT0")
			(pintype "bidirectional")
			(uuid "f4515d88-8991-4e3e-8ee4-a915e91f40fe")
		)
		(pad "8" smd rect
			(at -5.45 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "PF0{slash}SDC0_D1{slash}JTAG_MS")
			(pinfunction "DAT1")
			(pintype "bidirectional")
			(uuid "0af0698c-6d6e-4824-9b88-70e6105bae07")
		)
		(pad "9" smd rect
			(at -6.55 -5.3)
			(size 0.7 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "DET")
			(pintype "passive")
			(uuid "7e0ceda1-8642-4d80-9087-e969827fd458")
		)
		(pad "10" smd rect
			(at -7.75 -4.3)
			(size 1.2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "fd900ffd-0123-450e-a54a-00bfc7209fc4")
		)
		(pad "10" smd rect
			(at -7.75 5.3)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "63335764-c3ff-47a3-ad7c-7dce7d5ae9f7")
		)
		(pad "10" smd rect
			(at 6.85 -4.3)
			(size 1.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "da54d0ff-366b-4b7f-b6e3-ba769eb9bfcf")
		)
		(pad "10" smd rect
			(at 7.75 5.3)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "a8c3fbe4-7f93-40cf-90ad-f5613bd01bcb")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "ff36ab83-584f-4dcb-9a6b-42e05c137427")
		(at 67.48 60.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "12c3123a-eeb6-4269-9e61-f4c7334aa855")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5a17d0cb-17de-4387-9c35-be936ccf0602")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "956e34e9-6f8e-47cf-80f2-b79298b0e74f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "910a6f0d-6d9f-4528-8ca3-9e43d88b8ead")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1438734a-8b49-4271-9715-3246df660f68/77af8e5e-40f1-4d79-a1d2-9124d16a1d01")
		(sheetname "/电源/")
		(sheetfile "Power_sch.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f54642a-bdd3-465f-ab3b-8a4879a50979")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b8d7588-b265-440c-9db9-f1d224773f0d")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b63379b4-0132-43db-90c1-a6c1db2eb895")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5adc745a-41fd-4fdc-9bce-c9caf908151c")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35a70cc8-97bc-4491-b924-724d7e3f75df")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33eec59d-4a34-456b-a497-3cf10579d425")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "daaae980-0786-48a9-b93e-fab9d685430b")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "303268b5-dd1c-43a2-aa13-6510f89c3059")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "012e05b4-4bf3-4fb9-a64e-268ad4e56326")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e46a19e4-7582-470b-9ba0-8b40ffa7e31a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fe7e5570-d12b-492f-934d-4a53a7453237")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
			(uuid "344fbbf7-5249-404e-b401-f0545c12ebc6")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "2cf491ff-3822-4db0-8b87-17c0eb0a3458")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit"
		(layer "F.Cu")
		(uuid "ffafe0fe-3634-4ad5-88e6-554a73873e8f")
		(at 77 115.05)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
		(tags "solder Pin_ loose fit")
		(property "Reference" "TP7"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(uuid "61e1d699-da84-46a8-8576-b07badb61779")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "WL_HOST_WAKE"
			(at 0 -2.05 0)
			(layer "F.Fab")
			(uuid "81d03e3f-ef10-4020-ab9c-dc90fb14ba89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac51c0ac-39e6-42be-a41c-c11f49ca2e7b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "159485e1-112b-4f11-8cb1-79a2503732fd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5cb0d8cc-5d1d-402c-885f-2542a1a2f0e6/277e998d-43bf-452f-a50e-fb7977549aa1")
		(sheetname "/网口/")
		(sheetfile "Ethernet.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 0 0)
			(end 1.5 0.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "0f7bc380-7b10-4dcb-ab8d-2a664f0f1f04")
		)
		(fp_circle
			(center 0 0)
			(end 1.7 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "17ab3305-22e1-4c19-a644-ff29de5aaf93")
		)
		(fp_circle
			(center 0 0)
			(end 0.5 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "bd27afad-4b33-49db-b2f1-ceac7369976e")
		)
		(fp_circle
			(center 0 0)
			(end 1.2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "72762fbb-a4d0-4913-adcd-0c5c37623b5f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.25 0)
			(layer "F.Fab")
			(uuid "e66f487e-1f18-455b-a982-af2a8c350a34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/网口/WL_HOST_WAKE")
			(pinfunction "1")
			(pintype "passive")
			(uuid "7f1ee215-4405-4894-a955-439160784ec3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
